<?xml version='1.0' encoding='UTF-8'?>
<firmware version="0.14" type="rbf" temp_range="industrial" wr_sign="0xE502A5A5" crc32="0xDC0C6DC5">
  <devices>
    <device name="E502" chip="Cyclone IV" revision="0"/>
  </devices>
  <data>[encoded data, 183848 characters]</data>
</firmware>	