ARM GAS  /tmp/cc42qbQx.s 			page 1


   1              		.cpu cortex-m7
   2              		.arch armv7e-m
   3              		.fpu fpv5-d16
   4              		.eabi_attribute 28, 1
   5              		.eabi_attribute 20, 1
   6              		.eabi_attribute 21, 1
   7              		.eabi_attribute 23, 3
   8              		.eabi_attribute 24, 1
   9              		.eabi_attribute 25, 1
  10              		.eabi_attribute 26, 1
  11              		.eabi_attribute 30, 1
  12              		.eabi_attribute 34, 1
  13              		.eabi_attribute 18, 4
  14              		.file	"stm32f7xx_ll_rcc.c"
  15              		.text
  16              	.Ltext0:
  17              		.cfi_sections	.debug_frame
  18              		.file 1 "Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c"
  19              		.section	.text.LL_RCC_DeInit,"ax",%progbits
  20              		.align	1
  21              		.global	LL_RCC_DeInit
  22              		.syntax unified
  23              		.thumb
  24              		.thumb_func
  26              	LL_RCC_DeInit:
  27              	.LFB295:
   1:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @file    stm32f7xx_ll_rcc.c
   4:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief   RCC LL module driver.
   6:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * This software is licensed under terms that can be found in the LICENSE file in
  13:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   ******************************************************************************
  16:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
  17:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(USE_FULL_LL_DRIVER)
  18:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  19:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Includes ------------------------------------------------------------------*/
  20:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #include "stm32f7xx_ll_rcc.h"
  21:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #ifdef  USE_FULL_ASSERT
  22:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   #include "stm32_assert.h"
  23:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #else
  24:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   #define assert_param(expr) ((void)0U)
  25:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif
  26:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  27:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup STM32F7xx_LL_Driver
  28:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
  29:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
  30:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  31:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(RCC)
ARM GAS  /tmp/cc42qbQx.s 			page 2


  32:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  33:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL
  34:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
  35:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
  36:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  37:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Private types -------------------------------------------------------------*/
  38:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Private variables ---------------------------------------------------------*/
  39:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Private constants ---------------------------------------------------------*/
  40:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Private macros ------------------------------------------------------------*/
  41:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL_Private_Macros
  42:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
  43:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
  44:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_USART_CLKSOURCE(__VALUE__)  (((__VALUE__) == LL_RCC_USART1_CLKSOURCE) \
  45:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_USART2_CLKSOURCE) \
  46:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_USART3_CLKSOURCE) \
  47:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_USART6_CLKSOURCE))
  48:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  49:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_UART_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_UART4_CLKSOURCE) \
  50:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                              || ((__VALUE__) == LL_RCC_UART5_CLKSOURCE) \
  51:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                              || ((__VALUE__) == LL_RCC_UART7_CLKSOURCE) \
  52:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                              || ((__VALUE__) == LL_RCC_UART8_CLKSOURCE))
  53:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  54:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(I2C4)
  55:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_I2C_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_I2C1_CLKSOURCE) \
  56:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_I2C2_CLKSOURCE) \
  57:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_I2C3_CLKSOURCE) \
  58:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_I2C4_CLKSOURCE))
  59:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #else
  60:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_I2C_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_I2C1_CLKSOURCE) \
  61:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_I2C2_CLKSOURCE) \
  62:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_I2C3_CLKSOURCE))
  63:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* I2C4 */
  64:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  65:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_LPTIM_CLKSOURCE(__VALUE__)  (((__VALUE__) == LL_RCC_LPTIM1_CLKSOURCE))
  66:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  67:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_SAI_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_SAI1_CLKSOURCE) \
  68:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_SAI2_CLKSOURCE))
  69:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  70:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SDMMC2)
  71:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_SDMMC_CLKSOURCE(__VALUE__)  (((__VALUE__) == LL_RCC_SDMMC1_CLKSOURCE) \
  72:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                             || ((__VALUE__) == LL_RCC_SDMMC2_CLKSOURCE))
  73:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #else
  74:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_SDMMC_CLKSOURCE(__VALUE__)  (((__VALUE__) == LL_RCC_SDMMC1_CLKSOURCE))
  75:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SDMMC2 */
  76:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  77:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_RNG_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_RNG_CLKSOURCE))
  78:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  79:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_USB_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_USB_CLKSOURCE))
  80:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  81:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DFSDM1_Channel0)
  82:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_DFSDM_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_DFSDM1_CLKSOURCE))
  83:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  84:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_DFSDM_AUDIO_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_DFSDM1_AUDIO_CLKSOURC
  85:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DFSDM1_Channel0 */
  86:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  87:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_I2S_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_I2S1_CLKSOURCE))
  88:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
ARM GAS  /tmp/cc42qbQx.s 			page 3


  89:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(CEC)
  90:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_CEC_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_CEC_CLKSOURCE))
  91:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* CEC */
  92:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  93:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DSI)
  94:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_DSI_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_DSI_CLKSOURCE))
  95:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DSI */
  96:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
  97:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(LTDC)
  98:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_LTDC_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_LTDC_CLKSOURCE))
  99:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* LTDC */
 100:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 101:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SPDIFRX)
 102:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #define IS_LL_RCC_SPDIFRX_CLKSOURCE(__VALUE__)    (((__VALUE__) == LL_RCC_SPDIFRX1_CLKSOURCE))
 103:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SPDIFRX */
 104:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 105:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 106:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @}
 107:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 108:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 109:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Private function prototypes -----------------------------------------------*/
 110:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @defgroup RCC_LL_Private_Functions RCC Private functions
 111:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
 112:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 113:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetSystemClockFreq(void);
 114:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetHCLKClockFreq(uint32_t SYSCLK_Frequency);
 115:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetPCLK1ClockFreq(uint32_t HCLK_Frequency);
 116:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetPCLK2ClockFreq(uint32_t HCLK_Frequency);
 117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_SYS(void);
 118:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_SAI(void);
 119:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_48M(void);
 120:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DSI)
 121:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_DSI(void);
 122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DSI */
 123:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_SAI(void);
 124:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_48M(void);
 125:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(LTDC)
 126:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_LTDC(void);
 127:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* LTDC */
 128:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_I2S(void);
 129:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_SAI(void);
 130:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SPDIFRX)
 131:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_SPDIFRX(void);
 132:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SPDIFRX */
 133:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 134:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @}
 135:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 136:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 137:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 138:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /* Exported functions --------------------------------------------------------*/
 139:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL_Exported_Functions
 140:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
 141:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 142:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 143:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL_EF_Init
 144:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
 145:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 4


 146:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 147:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 148:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Reset the RCC clock configuration to the default reset state.
 149:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   The default reset state of the clock configuration is given below:
 150:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - HSI ON and used as system clock source
 151:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - HSE, PLL, PLLI2S, PLLSAI OFF
 152:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - AHB, APB1 and APB2 prescaler set to 1.
 153:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - CSS, MCO OFF
 154:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - All interrupts disabled
 155:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   This function doesn't modify the configuration of the
 156:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - Peripheral clocks
 157:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - LSI, LSE and RTC clocks
 158:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval An ErrorStatus enumeration value:
 159:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *          - SUCCESS: RCC registers are de-initialized
 160:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *          - ERROR: not applicable
 161:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 162:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** ErrorStatus LL_RCC_DeInit(void)
 163:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
  28              		.loc 1 163 1 view -0
  29              		.cfi_startproc
  30              		@ args = 0, pretend = 0, frame = 8
  31              		@ frame_needed = 0, uses_anonymous_args = 0
  32              		@ link register save eliminated.
  33 0000 82B0     		sub	sp, sp, #8
  34              	.LCFI0:
  35              		.cfi_def_cfa_offset 8
 164:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   __IO uint32_t vl_mask;
  36              		.loc 1 164 3 view .LVU1
 165:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 166:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Set HSION bit */
 167:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_HSI_Enable();
  37              		.loc 1 167 3 view .LVU2
  38              	.LBB234:
  39              	.LBI234:
  40              		.file 2 "Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h"
   1:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @file    stm32f7xx_ll_rcc.h
   4:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief   Header file of RCC LL module.
   6:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * This software is licensed under terms that can be found in the LICENSE file in
  13:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
  16:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  17:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  18:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Define to prevent recursive inclusion -------------------------------------*/
  19:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #ifndef __STM32F7xx_LL_RCC_H
  20:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __STM32F7xx_LL_RCC_H
  21:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  22:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #ifdef __cplusplus
ARM GAS  /tmp/cc42qbQx.s 			page 5


  23:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** extern "C" {
  24:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif
  25:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  26:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Includes ------------------------------------------------------------------*/
  27:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #include "stm32f7xx.h"
  28:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  29:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @addtogroup STM32F7xx_LL_Driver
  30:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  31:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  32:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  33:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC)
  34:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  35:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL RCC
  36:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  37:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  38:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  39:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private types -------------------------------------------------------------*/
  40:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private variables ---------------------------------------------------------*/
  41:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Private_Variables RCC Private Variables
  42:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  43:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  44:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  45:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_DCKCFGR1_PLLSAIDIVR)
  46:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** static const uint8_t aRCC_PLLSAIDIVRPrescTable[4] = {2, 4, 8, 16};
  47:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_DCKCFGR1_PLLSAIDIVR */
  48:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  49:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  50:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  51:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  52:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private constants ---------------------------------------------------------*/
  53:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private macros ------------------------------------------------------------*/
  54:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
  55:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Private_Macros RCC Private Macros
  56:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  57:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  58:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  59:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  60:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  61:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /*USE_FULL_LL_DRIVER*/
  62:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported types ------------------------------------------------------------*/
  63:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
  64:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Types RCC Exported Types
  65:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  66:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  67:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  68:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup LL_ES_CLOCK_FREQ Clocks Frequency Structure
  69:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  70:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  71:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  72:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  73:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  RCC Clocks Frequency Structure
  74:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  75:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** typedef struct
  76:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
  77:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t SYSCLK_Frequency;        /*!< SYSCLK clock frequency */
  78:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t HCLK_Frequency;          /*!< HCLK clock frequency */
  79:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t PCLK1_Frequency;         /*!< PCLK1 clock frequency */
ARM GAS  /tmp/cc42qbQx.s 			page 6


  80:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t PCLK2_Frequency;         /*!< PCLK2 clock frequency */
  81:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** } LL_RCC_ClocksTypeDef;
  82:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  83:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  84:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  85:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  86:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  87:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  88:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  89:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  90:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* USE_FULL_LL_DRIVER */
  91:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  92:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported constants --------------------------------------------------------*/
  93:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Constants RCC Exported Constants
  94:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  95:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  96:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  97:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_OSC_VALUES Oscillator Values adaptation
  98:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Defines used to adapt values of different oscillators
  99:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note     These values could be modified in the user environment according to 
 100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *           HW set-up.
 101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (HSE_VALUE)
 104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define HSE_VALUE    25000000U  /*!< Value of the HSE oscillator in Hz */
 105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* HSE_VALUE */
 106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (HSI_VALUE)
 108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define HSI_VALUE    16000000U  /*!< Value of the HSI oscillator in Hz */
 109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* HSI_VALUE */
 110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (LSE_VALUE)
 112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LSE_VALUE    32768U     /*!< Value of the LSE oscillator in Hz */
 113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LSE_VALUE */
 114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (LSI_VALUE)
 116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LSI_VALUE    32000U     /*!< Value of the LSI oscillator in Hz */
 117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LSI_VALUE */
 118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (EXTERNAL_CLOCK_VALUE)
 120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_CLOCK_VALUE    12288000U /*!< Value of the I2S_CKIN external oscillator in Hz */
 121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_CLOCK_VALUE */
 122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined (EXTERNAL_SAI1_CLOCK_VALUE)
 124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_SAI1_CLOCK_VALUE    48000U /*!< Value of the SAI1_EXTCLK external oscillator in Hz
 125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_SAI1_CLOCK_VALUE */
 126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined (EXTERNAL_SAI2_CLOCK_VALUE)
 128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_SAI2_CLOCK_VALUE    48000U /*!< Value of the SAI2_EXTCLK external oscillator in Hz
 129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_SAI2_CLOCK_VALUE */
 130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CLEAR_FLAG Clear Flags Defines
 135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Flags defines which can be used with LL_RCC_WriteReg function
 136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
ARM GAS  /tmp/cc42qbQx.s 			page 7


 137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYC                RCC_CIR_LSIRDYC     /*!< LSI Ready Interrupt Clear */
 139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYC                RCC_CIR_LSERDYC     /*!< LSE Ready Interrupt Clear */
 140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYC                RCC_CIR_HSIRDYC     /*!< HSI Ready Interrupt Clear */
 141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYC                RCC_CIR_HSERDYC     /*!< HSE Ready Interrupt Clear */
 142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYC                RCC_CIR_PLLRDYC     /*!< PLL Ready Interrupt Clear */
 143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYC             RCC_CIR_PLLI2SRDYC  /*!< PLLI2S Ready Interrupt Clear */
 144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYC             RCC_CIR_PLLSAIRDYC  /*!< PLLSAI Ready Interrupt Clear */
 145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_CSSC                   RCC_CIR_CSSC        /*!< Clock Security System Interrupt 
 146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_GET_FLAG Get Flags Defines
 151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Flags defines which can be used with LL_RCC_ReadReg function
 152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYF                RCC_CIR_LSIRDYF     /*!< LSI Ready Interrupt flag */
 155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYF                RCC_CIR_LSERDYF     /*!< LSE Ready Interrupt flag */
 156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYF                RCC_CIR_HSIRDYF     /*!< HSI Ready Interrupt flag */
 157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYF                RCC_CIR_HSERDYF     /*!< HSE Ready Interrupt flag */
 158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYF                RCC_CIR_PLLRDYF     /*!< PLL Ready Interrupt flag */
 159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYF             RCC_CIR_PLLI2SRDYF  /*!< PLLI2S Ready Interrupt flag */
 160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYF             RCC_CIR_PLLSAIRDYF  /*!< PLLSAI Ready Interrupt flag */
 161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_CSSF                   RCC_CIR_CSSF        /*!< Clock Security System Interrupt 
 162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_LPWRRSTF                RCC_CSR_LPWRRSTF   /*!< Low-Power reset flag */
 163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_PINRSTF                 RCC_CSR_PINRSTF    /*!< PIN reset flag */
 164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_PORRSTF                 RCC_CSR_PORRSTF    /*!< POR/PDR reset flag */
 165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_SFTRSTF                 RCC_CSR_SFTRSTF    /*!< Software Reset flag */
 166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_IWDGRSTF                RCC_CSR_IWDGRSTF   /*!< Independent Watchdog reset flag 
 167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_WWDGRSTF                RCC_CSR_WWDGRSTF   /*!< Window watchdog reset flag */
 168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_BORRSTF                 RCC_CSR_BORRSTF    /*!< BOR reset flag */
 169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_IT IT Defines
 174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    IT defines which can be used with LL_RCC_ReadReg and  LL_RCC_WriteReg functions
 175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYIE               RCC_CIR_LSIRDYIE      /*!< LSI Ready Interrupt Enable */
 178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYIE               RCC_CIR_LSERDYIE      /*!< LSE Ready Interrupt Enable */
 179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYIE               RCC_CIR_HSIRDYIE      /*!< HSI Ready Interrupt Enable */
 180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYIE               RCC_CIR_HSERDYIE      /*!< HSE Ready Interrupt Enable */
 181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYIE               RCC_CIR_PLLRDYIE      /*!< PLL Ready Interrupt Enable */
 182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYIE            RCC_CIR_PLLI2SRDYIE   /*!< PLLI2S Ready Interrupt Enable 
 183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYIE            RCC_CIR_PLLSAIRDYIE   /*!< PLLSAI Ready Interrupt Enable 
 184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LSEDRIVE  LSE oscillator drive capability
 189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_LOW                0x00000000U             /*!< Xtal mode lower driving cap
 192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_MEDIUMHIGH         RCC_BDCR_LSEDRV_0       /*!< Xtal mode medium high drivi
 193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_MEDIUMLOW          RCC_BDCR_LSEDRV_1       /*!< Xtal mode medium low drivin
ARM GAS  /tmp/cc42qbQx.s 			page 8


 194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_HIGH               RCC_BDCR_LSEDRV         /*!< Xtal mode higher driving ca
 195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYS_CLKSOURCE  System clock switch
 200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_HSI           RCC_CFGR_SW_HSI    /*!< HSI selection as system clock */
 203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_HSE           RCC_CFGR_SW_HSE    /*!< HSE selection as system clock */
 204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_PLL           RCC_CFGR_SW_PLL    /*!< PLL selection as system clock */
 205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYS_CLKSOURCE_STATUS  System clock switch status
 210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_HSI    RCC_CFGR_SWS_HSI   /*!< HSI used as system clock */
 213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_HSE    RCC_CFGR_SWS_HSE   /*!< HSE used as system clock */
 214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_PLL    RCC_CFGR_SWS_PLL   /*!< PLL used as system clock */
 215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYSCLK_DIV  AHB prescaler
 220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_1                RCC_CFGR_HPRE_DIV1   /*!< SYSCLK not divided */
 223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_2                RCC_CFGR_HPRE_DIV2   /*!< SYSCLK divided by 2 */
 224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_4                RCC_CFGR_HPRE_DIV4   /*!< SYSCLK divided by 4 */
 225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_8                RCC_CFGR_HPRE_DIV8   /*!< SYSCLK divided by 8 */
 226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_16               RCC_CFGR_HPRE_DIV16  /*!< SYSCLK divided by 16 */
 227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_64               RCC_CFGR_HPRE_DIV64  /*!< SYSCLK divided by 64 */
 228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_128              RCC_CFGR_HPRE_DIV128 /*!< SYSCLK divided by 128 */
 229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_256              RCC_CFGR_HPRE_DIV256 /*!< SYSCLK divided by 256 */
 230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_512              RCC_CFGR_HPRE_DIV512 /*!< SYSCLK divided by 512 */
 231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_APB1_DIV  APB low-speed prescaler (APB1)
 236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_1                  RCC_CFGR_PPRE1_DIV1  /*!< HCLK not divided */
 239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_2                  RCC_CFGR_PPRE1_DIV2  /*!< HCLK divided by 2 */
 240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_4                  RCC_CFGR_PPRE1_DIV4  /*!< HCLK divided by 4 */
 241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_8                  RCC_CFGR_PPRE1_DIV8  /*!< HCLK divided by 8 */
 242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_16                 RCC_CFGR_PPRE1_DIV16 /*!< HCLK divided by 16 */
 243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_APB2_DIV  APB high-speed prescaler (APB2)
 247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_1                  RCC_CFGR_PPRE2_DIV1  /*!< HCLK not divided */
 250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_2                  RCC_CFGR_PPRE2_DIV2  /*!< HCLK divided by 2 */
ARM GAS  /tmp/cc42qbQx.s 			page 9


 251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_4                  RCC_CFGR_PPRE2_DIV4  /*!< HCLK divided by 4 */
 252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_8                  RCC_CFGR_PPRE2_DIV8  /*!< HCLK divided by 8 */
 253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_16                 RCC_CFGR_PPRE2_DIV16 /*!< HCLK divided by 16 */
 254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_MCOxSOURCE  MCO source selection
 259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_HSI              (uint32_t)(RCC_CFGR_MCO1|0x00000000U)                   
 262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_LSE              (uint32_t)(RCC_CFGR_MCO1|(RCC_CFGR_MCO1_0 >> 16U))      
 263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_HSE              (uint32_t)(RCC_CFGR_MCO1|(RCC_CFGR_MCO1_1 >> 16U))      
 264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_PLLCLK           (uint32_t)(RCC_CFGR_MCO1|((RCC_CFGR_MCO1_1|RCC_CFGR_MCO1
 265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_SYSCLK           (uint32_t)(RCC_CFGR_MCO2|0x00000000U)                   
 266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_PLLI2S           (uint32_t)(RCC_CFGR_MCO2|(RCC_CFGR_MCO2_0 >> 16U))      
 267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_HSE              (uint32_t)(RCC_CFGR_MCO2|(RCC_CFGR_MCO2_1 >> 16U))      
 268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_PLLCLK           (uint32_t)(RCC_CFGR_MCO2|((RCC_CFGR_MCO2_1|RCC_CFGR_MCO2
 269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_MCOx_DIV  MCO prescaler
 274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_1                  (uint32_t)(RCC_CFGR_MCO1PRE|0x00000000U)                
 277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_2                  (uint32_t)(RCC_CFGR_MCO1PRE|(RCC_CFGR_MCO1PRE_2 >> 16U))
 278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_3                  (uint32_t)(RCC_CFGR_MCO1PRE|((RCC_CFGR_MCO1PRE_2|RCC_CFG
 279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_4                  (uint32_t)(RCC_CFGR_MCO1PRE|((RCC_CFGR_MCO1PRE_2|RCC_CFG
 280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_5                  (uint32_t)(RCC_CFGR_MCO1PRE|(RCC_CFGR_MCO1PRE >> 16U))  
 281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_1                  (uint32_t)(RCC_CFGR_MCO2PRE|0x00000000U)                
 282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_2                  (uint32_t)(RCC_CFGR_MCO2PRE|(RCC_CFGR_MCO2PRE_2 >> 16U))
 283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_3                  (uint32_t)(RCC_CFGR_MCO2PRE|((RCC_CFGR_MCO2PRE_2|RCC_CFG
 284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_4                  (uint32_t)(RCC_CFGR_MCO2PRE|((RCC_CFGR_MCO2PRE_2|RCC_CFG
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_5                  (uint32_t)(RCC_CFGR_MCO2PRE|(RCC_CFGR_MCO2PRE >> 16U))  
 286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RTC_HSEDIV  HSE prescaler for RTC clock
 291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_NOCLOCK                  0x00000000U             /*!< HSE not divided */
 294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_2                RCC_CFGR_RTCPRE_1       /*!< HSE clock divided by 2 */
 295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_3                (RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_4                RCC_CFGR_RTCPRE_2       /*!< HSE clock divided by 4 */
 297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_5                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_6                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_7                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_8                RCC_CFGR_RTCPRE_3       /*!< HSE clock divided by 8 */
 301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_9                (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_10               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_11               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_12               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2)       /*!< HSE cl
 305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_13               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)
 306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_14               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)
 307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_15               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|
ARM GAS  /tmp/cc42qbQx.s 			page 10


 308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_16               RCC_CFGR_RTCPRE_4       /*!< HSE clock divided by 16 */
 309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_17               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_18               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_19               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_20               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2)       /*!< HSE cl
 313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_21               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)
 314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_22               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)
 315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_23               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|
 316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_24               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3)       /*!< HSE cl
 317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_25               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_0)
 318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_26               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1)
 319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_27               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1|
 320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_28               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2)
 321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_29               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_30               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_31               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
 329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PERIPH_FREQUENCY Peripheral clock frequency
 330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PERIPH_FREQUENCY_NO         0x00000000U                 /*!< No clock enabled for th
 333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PERIPH_FREQUENCY_NA         0xFFFFFFFFU                 /*!< Frequency cannot be pro
 334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* USE_FULL_LL_DRIVER */
 338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USARTx_CLKSOURCE  Peripheral USART clock source selection
 340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_PCLK2      (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | 0x00000000U
 343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | 0x00000000U
 347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | 0x00000000U
 351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_PCLK2      (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | 0x00000000U
 355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_UARTx_CLKSOURCE  Peripheral UART clock source selection
 363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 11


 365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | 0x00000000U) 
 366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | 0x00000000U) 
 370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | 0x00000000U) 
 374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | 0x00000000U) 
 378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2Cx_CLKSOURCE  Peripheral I2C clock source selection
 386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C1SEL|0x00000000U) /*!< PCLK1 
 389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C1SEL|(RCC_DCKCFGR2_I2C1SEL_0 
 390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C1SEL|(RCC_DCKCFGR2_I2C1SEL_1 
 391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C2SEL|0x00000000U) /*!< PCLK1 
 392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C2SEL|(RCC_DCKCFGR2_I2C2SEL_0 
 393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C2SEL|(RCC_DCKCFGR2_I2C2SEL_1 
 394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C3SEL|0x00000000U) /*!< PCLK1 
 395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C3SEL|(RCC_DCKCFGR2_I2C3SEL_0 
 396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C3SEL|(RCC_DCKCFGR2_I2C3SEL_1 
 397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(I2C4)
 398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C4SEL|0x00000000U) /*!< PCLK1 
 399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C4SEL|(RCC_DCKCFGR2_I2C4SEL_0 
 400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C4SEL|(RCC_DCKCFGR2_I2C4SEL_1 
 401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* I2C4 */
 402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LPTIM1_CLKSOURCE  Peripheral LPTIM clock source selection
 407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_PCLK1       0x00000000U                 /*!< PCLK1 clock used as LP
 410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_LSI         RCC_DCKCFGR2_LPTIM1SEL_0    /*!< LSI oscillator clock u
 411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_HSI         RCC_DCKCFGR2_LPTIM1SEL_1    /*!< HSI oscillator clock u
 412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_LSE         (uint32_t)(RCC_DCKCFGR2_LPTIM1SEL_1 | RCC_DCKCFGR2_LPTI
 413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SAIx_CLKSOURCE  Peripheral SAI clock source selection
 418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLSAI       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | 0x00000000U)          
 421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLI2S       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL_
ARM GAS  /tmp/cc42qbQx.s 			page 12


 422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PIN          (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL_
 423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_SAI1SEL_PLLSRC_SUPPORT)
 424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLSRC       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL 
 425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_SAI1SEL_PLLSRC_SUPPORT */
 426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLSAI       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | 0x00000000U)          
 427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLI2S       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL_
 428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PIN          (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL_
 429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_SAI2SEL_PLLSRC_SUPPORT)
 430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLSRC       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL 
 431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_SAI2SEL_PLLSRC_SUPPORT */
 432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SDMMCx_CLKSOURCE  Peripheral SDMMC clock source selection
 437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK       (uint32_t)(RCC_DCKCFGR2_SDMMC1SEL | 0x00000000U)    
 440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE_SYSCLK         (uint32_t)(RCC_DCKCFGR2_SDMMC1SEL | (RCC_DCKCFGR2_SD
 441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SDMMC2)
 442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK       (uint32_t)(RCC_DCKCFGR2_SDMMC2SEL | 0x00000000U)    
 443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE_SYSCLK         (uint32_t)(RCC_DCKCFGR2_SDMMC2SEL | (RCC_DCKCFGR2_SD
 444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SDMMC2 */
 445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RNG_CLKSOURCE  Peripheral RNG clock source selection
 450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE_PLL          0x00000000U            /*!< PLL clock used as RNG clock s
 453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE_PLLSAI       RCC_DCKCFGR2_CK48MSEL  /*!< PLLSAI clock used as RNG cloc
 454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USB_CLKSOURCE  Peripheral USB clock source selection
 459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE_PLL          0x00000000U            /*!< PLL clock used as USB clock s
 462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE_PLLSAI       RCC_DCKCFGR2_CK48MSEL  /*!< PLLSAI1 clock used as USB clo
 463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
 468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DSI_CLKSOURCE  Peripheral DSI clock source selection
 469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE_PHY          0x00000000U           /*!< DSI-PHY clock used as DSI byte
 472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE_PLL          RCC_DCKCFGR2_DSISEL   /*!< PLL clock used as DSI byte lan
 473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
 477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
ARM GAS  /tmp/cc42qbQx.s 			page 13


 479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CEC_CLKSOURCE  Peripheral CEC clock source selection
 480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE_LSE               0x00000000U                /*!< LSE oscillator clock
 483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE_HSI_DIV488        RCC_DCKCFGR2_CECSEL        /*!< HSI oscillator clock
 484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
 488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2S1_CLKSOURCE  Peripheral I2S clock source selection
 490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE_PLLI2S           0x00000000U                /*!< I2S oscillator clock
 493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE_PIN              RCC_CFGR_I2SSRC            /*!< External pin clock u
 494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CK48M_CLKSOURCE  Peripheral 48Mhz domain clock source selection
 499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE_PLL             0x00000000U                /*!< PLL oscillator clock
 502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE_PLLSAI          RCC_DCKCFGR2_CK48MSEL      /*!< PLLSAI oscillator cl
 503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
 508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM1_AUDIO_CLKSOURCE  Peripheral DFSDM Audio clock source selection
 509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1     0x00000000U                /*!< SAI1 clock used as D
 512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2     RCC_DCKCFGR1_ADFSDM1SEL    /*!< SAI2 clock used as D
 513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM1_CLKSOURCE  Peripheral DFSDM clock source selection
 518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE_PCLK2          0x00000000U                /*!< PCLK2 clock used as 
 521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE_SYSCLK         RCC_DCKCFGR1_DFSDM1SEL     /*!< System clock used as
 522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
 526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USARTx  Peripheral USART get clock source
 528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE            RCC_DCKCFGR2_USART1SEL /*!< USART1 Clock source selectio
 531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE            RCC_DCKCFGR2_USART2SEL /*!< USART2 Clock source selectio
 532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE            RCC_DCKCFGR2_USART3SEL /*!< USART3 Clock source selectio
 533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE            RCC_DCKCFGR2_USART6SEL /*!< USART6 Clock source selectio
 534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
ARM GAS  /tmp/cc42qbQx.s 			page 14


 536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_UARTx  Peripheral UART get clock source
 539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE             RCC_DCKCFGR2_UART4SEL /*!< UART4 Clock source selection 
 542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE             RCC_DCKCFGR2_UART5SEL /*!< UART5 Clock source selection 
 543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE             RCC_DCKCFGR2_UART7SEL /*!< UART7 Clock source selection 
 544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE             RCC_DCKCFGR2_UART8SEL /*!< UART8 Clock source selection 
 545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2Cx  Peripheral I2C get clock source
 550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE              RCC_DCKCFGR2_I2C1SEL  /*!< I2C1 Clock source selection *
 553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE              RCC_DCKCFGR2_I2C2SEL  /*!< I2C2 Clock source selection *
 554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE              RCC_DCKCFGR2_I2C3SEL  /*!< I2C3 Clock source selection *
 555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(I2C4)
 556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE              RCC_DCKCFGR2_I2C4SEL  /*!< I2C4 Clock source selection *
 557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* I2C4 */
 558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LPTIM1  Peripheral LPTIM get clock source
 563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE            RCC_DCKCFGR2_LPTIM1SEL /*!< LPTIM1 Clock source selectio
 566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SAIx  Peripheral SAI get clock source
 571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE              RCC_DCKCFGR1_SAI1SEL /*!< SAI1 Clock source selection */
 574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE              RCC_DCKCFGR1_SAI2SEL /*!< SAI2 Clock source selection */
 575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SDMMCx  Peripheral SDMMC get clock source
 580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE            RCC_DCKCFGR2_SDMMC1SEL /*!< SDMMC1 Clock source selectio
 583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SDMMC2)
 584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE            RCC_DCKCFGR2_SDMMC2SEL /*!< SDMMC2 Clock source selectio
 585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SDMMC2 */
 586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CK48M  Peripheral CK48M get clock source
 591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 15


 593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE             RCC_DCKCFGR2_CK48MSEL /*!< CK48M Domain clock source sel
 594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RNG  Peripheral RNG get clock source
 599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE               RCC_DCKCFGR2_CK48MSEL /*!< RNG Clock source selection */
 602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USB  Peripheral USB get clock source
 607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE               RCC_DCKCFGR2_CK48MSEL /*!< USB Clock source selection */
 610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
 615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CEC  Peripheral CEC get clock source
 616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE               RCC_DCKCFGR2_CECSEL /*!< CEC Clock source selection */
 619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
 623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2S1  Peripheral I2S get clock source
 625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE              RCC_CFGR_I2SSRC /*!< I2S Clock source selection */
 628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
 632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM_AUDIO  Peripheral DFSDM Audio get clock source
 633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE      RCC_DCKCFGR1_ADFSDM1SEL /*!< DFSDM Audio Clock source se
 636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM  Peripheral DFSDM get clock source
 641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE            RCC_DCKCFGR1_DFSDM1SEL /*!< DFSDM Clock source selection
 644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
 648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
ARM GAS  /tmp/cc42qbQx.s 			page 16


 650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DSI  Peripheral DSI get clock source
 651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE               RCC_DCKCFGR2_DSISEL /*!< DSI Clock source selection */
 654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
 658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(LTDC)
 660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LTDC  Peripheral LTDC get clock source
 661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LTDC_CLKSOURCE              RCC_DCKCFGR1_PLLSAIDIVR /*!< LTDC Clock source selection
 664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LTDC */
 668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
 670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SPDIFRX  Peripheral SPDIFRX get clock source
 671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPDIFRX1_CLKSOURCE           RCC_PLLI2SCFGR_PLLI2SP /*!< SPDIFRX Clock source select
 674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
 678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RTC_CLKSOURCE  RTC clock source selection
 680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_NONE          0x00000000U             /*!< No clock used as RTC clock 
 683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_LSE           RCC_BDCR_RTCSEL_0       /*!< LSE oscillator clock used a
 684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_LSI           RCC_BDCR_RTCSEL_1       /*!< LSI oscillator clock used a
 685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_HSE           RCC_BDCR_RTCSEL         /*!< HSE oscillator clock divide
 686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_TIM_CLKPRESCALER  Timers clocks prescalers selection
 691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_TIM_PRESCALER_TWICE          0x00000000U                  /*!< Timers clock to twice
 694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_TIM_PRESCALER_FOUR_TIMES     RCC_DCKCFGR1_TIMPRE          /*!< Timers clock to four 
 695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSOURCE  PLL, PLLI2S and PLLSAI entry clock source
 700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSOURCE_HSI               RCC_PLLCFGR_PLLSRC_HSI  /*!< HSI16 clock selected as PLL
 703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSOURCE_HSE               RCC_PLLCFGR_PLLSRC_HSE  /*!< HSE clock selected as PLL e
 704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 17


 707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLM_DIV  PLL, PLLI2S and PLLSAI division factor
 709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_2                  (RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI2S and PLLSAI divisio
 712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_3                  (RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_4                  (RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI2S and PLLSAI divisio
 714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_5                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_6                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_7                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_8                  (RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI2S and PLLSAI divisio
 718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_9                  (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_10                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_11                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_12                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_13                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_14                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_15                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_16                 (RCC_PLLCFGR_PLLM_4) /*!< PLL, PLLI2S and PLLSAI divisio
 726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_17                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_18                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_19                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_20                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_21                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_22                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_23                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_24                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI
 734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_25                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_26                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_27                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_28                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_29                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_30                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_31                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_32                 (RCC_PLLCFGR_PLLM_5) /*!< PLL, PLLI2S and PLLSAI divisio
 742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_33                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_34                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_35                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_36                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_37                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_38                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_39                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_40                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI
 750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_41                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_42                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_43                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_44                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_45                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_46                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_47                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_48                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4) /*!< PLL, PLLI
 758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_49                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_50                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_51                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_52                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_53                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_54                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
ARM GAS  /tmp/cc42qbQx.s 			page 18


 764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_55                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_56                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_57                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_58                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_59                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_60                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_61                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_62                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_63                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLCFGR_PLLR)
 778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLR_DIV  PLL division factor (PLLR)
 779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_2                  (RCC_PLLCFGR_PLLR_1)                     /*!< Main PLL d
 782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_3                  (RCC_PLLCFGR_PLLR_1|RCC_PLLCFGR_PLLR_0)  /*!< Main PLL d
 783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_4                  (RCC_PLLCFGR_PLLR_2)                     /*!< Main PLL d
 784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_5                  (RCC_PLLCFGR_PLLR_2|RCC_PLLCFGR_PLLR_0)  /*!< Main PLL d
 785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_6                  (RCC_PLLCFGR_PLLR_2|RCC_PLLCFGR_PLLR_1)  /*!< Main PLL d
 786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_7                  (RCC_PLLCFGR_PLLR)                       /*!< Main PLL d
 787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLCFGR_PLLR */
 791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLP_DIV  PLL division factor (PLLP)
 793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_2                  0x00000000U            /*!< Main PLL division factor for
 796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_4                  RCC_PLLCFGR_PLLP_0     /*!< Main PLL division factor for
 797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_6                  RCC_PLLCFGR_PLLP_1     /*!< Main PLL division factor for
 798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_8                  (RCC_PLLCFGR_PLLP_1 | RCC_PLLCFGR_PLLP_0)   /*!< Main PL
 799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLQ_DIV  PLL division factor (PLLQ)
 804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_2                  RCC_PLLCFGR_PLLQ_1                      /*!< Main PLL di
 807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_3                  (RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_4                  RCC_PLLCFGR_PLLQ_2                      /*!< Main PLL di
 809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_5                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_6                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_1) /*!< Main PLL di
 811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_7                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_
 812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_8                  RCC_PLLCFGR_PLLQ_3                      /*!< Main PLL di
 813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_9                  (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_10                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_1) /*!< Main PLL di
 815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_11                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_
 816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_12                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2) /*!< Main PLL di
 817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_13                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_14                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_15                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/cc42qbQx.s 			page 19


 821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLL_SPRE_SEL  PLL Spread Spectrum Selection
 825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPREAD_SELECT_CENTER        0x00000000U                   /*!< PLL center spread spe
 828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPREAD_SELECT_DOWN          RCC_SSCGR_SPREADSEL           /*!< PLL down spread spect
 829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SQ  PLLI2SQ division factor (PLLI2SQ)
 834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_2              RCC_PLLI2SCFGR_PLLI2SQ_1        /*!< PLLI2S division fact
 837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_3              (RCC_PLLI2SCFGR_PLLI2SQ_1 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_4              RCC_PLLI2SCFGR_PLLI2SQ_2        /*!< PLLI2S division fact
 839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_5              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_6              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_1)    
 841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_7              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_1 | RC
 842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_8              RCC_PLLI2SCFGR_PLLI2SQ_3        /*!< PLLI2S division fact
 843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_9              (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_10             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_1)    
 845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_11             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_1 | RC
 846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_12             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2)    
 847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_13             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_14             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_15             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SDIVQ  PLLI2SDIVQ division factor (PLLI2SDIVQ)
 855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_1           0x00000000U                        /*!< PLLI2S division f
 858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_2           RCC_DCKCFGR1_PLLI2SDIVQ_0          /*!< PLLI2S division f
 859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_3           RCC_DCKCFGR1_PLLI2SDIVQ_1          /*!< PLLI2S division f
 860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_4           (RCC_DCKCFGR1_PLLI2SDIVQ_1 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_5           RCC_DCKCFGR1_PLLI2SDIVQ_2          /*!< PLLI2S division f
 862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_6           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_7           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_8           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_9           RCC_DCKCFGR1_PLLI2SDIVQ_3          /*!< PLLI2S division f
 866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_10          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_11          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_12          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_13          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2)  
 870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_14          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_15          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_16          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_17          RCC_DCKCFGR1_PLLI2SDIVQ_4          /*!< PLLI2S division f
 874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_18          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_19          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_20          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_21          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2)  
ARM GAS  /tmp/cc42qbQx.s 			page 20


 878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_22          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_23          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_24          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_25          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3)  
 882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_26          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_27          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_28          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_29          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_30          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_31          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_32          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SR  PLLI2SR division factor (PLLI2SR)
 894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_2              RCC_PLLI2SCFGR_PLLI2SR_1                                 
 897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_3              (RCC_PLLI2SCFGR_PLLI2SR_1 | RCC_PLLI2SCFGR_PLLI2SR_0)    
 898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_4              RCC_PLLI2SCFGR_PLLI2SR_2                                 
 899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_5              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_0)    
 900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_6              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_1)    
 901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_7              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_1 | RC
 902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLI2SCFGR_PLLI2SP)
 907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SP  PLLI2SP division factor (PLLI2SP)
 908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_2              0x00000000U            /*!< PLLI2S division factor for PL
 911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_4              RCC_PLLI2SCFGR_PLLI2SP_0        /*!< PLLI2S division fact
 912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_6              RCC_PLLI2SCFGR_PLLI2SP_1        /*!< PLLI2S division fact
 913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_8              (RCC_PLLI2SCFGR_PLLI2SP_1 | RCC_PLLI2SCFGR_PLLI2SP_0)    
 914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLI2SCFGR_PLLI2SP */
 918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIQ  PLLSAIQ division factor (PLLSAIQ)
 920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_2              RCC_PLLSAICFGR_PLLSAIQ_1        /*!< PLLSAI division fact
 923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_3              (RCC_PLLSAICFGR_PLLSAIQ_1 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_4              RCC_PLLSAICFGR_PLLSAIQ_2        /*!< PLLSAI division fact
 925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_5              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_6              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_1)    
 927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_7              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_1 | RC
 928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_8              RCC_PLLSAICFGR_PLLSAIQ_3        /*!< PLLSAI division fact
 929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_9              (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_10             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_1)    
 931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_11             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_1 | RC
 932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_12             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2)    
 933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_13             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
 934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_14             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
ARM GAS  /tmp/cc42qbQx.s 			page 21


 935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_15             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
 936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIDIVQ  PLLSAIDIVQ division factor (PLLSAIDIVQ)
 941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_1           0x00000000U               /*!< PLLSAI division factor for
 944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_2           RCC_DCKCFGR1_PLLSAIDIVQ_0          /*!< PLLSAI division f
 945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_3           RCC_DCKCFGR1_PLLSAIDIVQ_1          /*!< PLLSAI division f
 946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_4           (RCC_DCKCFGR1_PLLSAIDIVQ_1 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_5           RCC_DCKCFGR1_PLLSAIDIVQ_2          /*!< PLLSAI division f
 948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_6           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_7           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_8           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_9           RCC_DCKCFGR1_PLLSAIDIVQ_3          /*!< PLLSAI division f
 952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_10          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_11          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_12          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_13          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2)  
 956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_14          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_15          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_16          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_17          RCC_DCKCFGR1_PLLSAIDIVQ_4         /*!< PLLSAI division fa
 960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_18          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_19          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_20          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_21          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2)  
 964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_22          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_23          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_24          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_25          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3)  
 968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_26          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_27          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_28          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_29          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_30          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_31          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_32          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLSAICFGR_PLLSAIR)
 980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIR  PLLSAIR division factor (PLLSAIR)
 981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_2              RCC_PLLSAICFGR_PLLSAIR_1                                 
 984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_3              (RCC_PLLSAICFGR_PLLSAIR_1 | RCC_PLLSAICFGR_PLLSAIR_0)    
 985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_4              RCC_PLLSAICFGR_PLLSAIR_2                                 
 986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_5              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_0)    
 987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_6              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_1)    
 988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_7              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_1 | RC
 989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 22


 992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLSAICFGR_PLLSAIR */
 993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_DCKCFGR1_PLLSAIDIVR)
 995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIDIVR  PLLSAIDIVR division factor (PLLSAIDIVR)
 996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_2           0x00000000U             /*!< PLLSAI division factor for P
 999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_4           RCC_DCKCFGR1_PLLSAIDIVR_0        /*!< PLLSAI division fac
1000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_8           RCC_DCKCFGR1_PLLSAIDIVR_1        /*!< PLLSAI division fac
1001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_16          (RCC_DCKCFGR1_PLLSAIDIVR_1 | RCC_DCKCFGR1_PLLSAIDIVR_0)  
1002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_DCKCFGR1_PLLSAIDIVR */
1006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIP  PLLSAIP division factor (PLLSAIP)
1008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_2              0x00000000U               /*!< PLLSAI division factor for
1011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_4              RCC_PLLSAICFGR_PLLSAIP_0        /*!< PLLSAI division fact
1012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_6              RCC_PLLSAICFGR_PLLSAIP_1        /*!< PLLSAI division fact
1013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_8              (RCC_PLLSAICFGR_PLLSAIP_1 | RCC_PLLSAICFGR_PLLSAIP_0)    
1014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported macro ------------------------------------------------------------*/
1023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Macros RCC Exported Macros
1024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EM_WRITE_READ Common Write and read registers Macros
1028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Write a value in RCC register
1033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __REG__ Register to be written
1034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __VALUE__ Value to be written in the register
1035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_WriteReg(__REG__, __VALUE__) WRITE_REG(RCC->__REG__, (__VALUE__))
1038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Read a value in RCC register
1041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __REG__ Register to be read
1042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Register value
1043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_ReadReg(__REG__) READ_REG(RCC->__REG__)
1045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 23


1049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EM_CALC_FREQ Calculate frequencies
1050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency on system domain
1055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetP ());
1057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
ARM GAS  /tmp/cc42qbQx.s 			page 24


1106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLP__ This parameter can be one of the following values:
1123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
1124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
1125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
1126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
1127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLP__) ((__INPUTFREQ__) / (
1130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLP__) >> RCC_PLLCFGR_PLLP_Pos ) + 1U) * 2U))
1131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency used on 48M domain
1134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_48M_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetQ ());
1136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
ARM GAS  /tmp/cc42qbQx.s 			page 25


1163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLQ__ This parameter can be one of the following values:
1202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
1203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
1204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
1205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
1206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
1207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
1208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
1209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
1210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
1211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
1212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
1213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
1214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
1215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
1216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_48M_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLQ__) ((__INPUTFREQ__)
1219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLQ__) >> RCC_PLLCFGR_PLLQ_Pos ))
ARM GAS  /tmp/cc42qbQx.s 			page 26


1220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
1222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency used on DSI
1224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_DSI_FREQ (HSE_VALUE, @ref LL_RCC_PLL_GetDivider (),
1225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetR ());
1226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
ARM GAS  /tmp/cc42qbQx.s 			page 27


1277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLR__ This parameter can be one of the following values:
1292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
1293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
1294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
1295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
1296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
1297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
1298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_DSI_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLR__) ((__INPUTFREQ__)
1301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLR__) >> RCC_PLLCFGR_PLLR_Pos ))
1302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
1303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used for SAI1 and SAI2 domains
1306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_SAI_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetQ (), @ref LL_RCC_PLLSAI_GetDIVQ 
1308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
ARM GAS  /tmp/cc42qbQx.s 			page 28


1334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIQ__ This parameter can be one of the following values:
1374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_2
1375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_3
1376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_4
1377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_5
1378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_6
1379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_7
1380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_8
1381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_9
1382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_10
1383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_11
1384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_12
1385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_13
1386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_14
1387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_15
1388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIDIVQ__ This parameter can be one of the following values:
1389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_1
1390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_2
ARM GAS  /tmp/cc42qbQx.s 			page 29


1391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_3
1392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_4
1393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_5
1394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_6
1395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_7
1396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_8
1397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_9
1398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_10
1399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_11
1400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_12
1401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_13
1402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_14
1403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_15
1404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_16
1405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_17
1406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_18
1407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_19
1408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_20
1409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_21
1410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_22
1411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_23
1412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_24
1413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_25
1414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_26
1415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_27
1416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_28
1417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_29
1418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_30
1419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_31
1420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_32
1421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_SAI_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIQ__, __PLLSAIDI
1424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLSAIQ__) >> RCC_PLLSAICFGR_PLLSAIQ_Pos) * (((__PLLSAIDIVQ__) >> RCC_DCKCF
1425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used on 48Mhz domain
1428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_48M_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetP ());
1430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
ARM GAS  /tmp/cc42qbQx.s 			page 30


1448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIP__ This parameter can be one of the following values:
1496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_2
1497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_4
1498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_6
1499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_8
1500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_48M_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIP__) (((__INPUT
1503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLSAIP__) >> RCC_PLLSAICFGR_PLLSAIP_Pos) + 1U ) * 2U))
1504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 31


1505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(LTDC)
1506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used for LTDC domain
1508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_LTDC_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetR (), @ref LL_RCC_PLLSAI_GetDIVR 
1510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
ARM GAS  /tmp/cc42qbQx.s 			page 32


1562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIR__ This parameter can be one of the following values:
1576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_2
1577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_3
1578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_4
1579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_5
1580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_6
1581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_7
1582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIDIVR__ This parameter can be one of the following values:
1583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_2
1584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_4
1585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_8
1586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_16
1587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_LTDC_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIR__, __PLLSAID
1590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLSAIR__) >> RCC_PLLSAICFGR_PLLSAIR_Pos) * (aRCC_PLLSAIDIVRPrescTable[(__P
1591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LTDC */
1592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used for SAI1 and SAI2 domains
1595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_SAI_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetQ (), @ref LL_RCC_PLLI2S_GetDIVQ 
1597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
ARM GAS  /tmp/cc42qbQx.s 			page 33


1619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SQ__ This parameter can be one of the following values:
1663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
1664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
1665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
1666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
1667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
1668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
1669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
1670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
1671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
1672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
1673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
1674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
1675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
ARM GAS  /tmp/cc42qbQx.s 			page 34


1676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
1677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SDIVQ__ This parameter can be one of the following values:
1678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
1679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
1680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
1681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
1682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
1683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
1684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
1685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
1686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
1687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
1688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
1689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
1690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
1691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
1692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
1693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
1694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
1695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
1696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
1697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
1698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
1699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
1700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
1701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
1702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
1703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
1704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
1705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
1706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
1707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
1708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
1709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
1710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
1711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_SAI_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SQ__, __PLLI2SDI
1713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLI2SQ__) >> RCC_PLLI2SCFGR_PLLI2SQ_Pos) * (((__PLLI2SDIVQ__) >> RCC_DCKCF
1714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
1716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used on SPDIFRX domain
1718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_SPDIFRX_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetP ());
1720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
ARM GAS  /tmp/cc42qbQx.s 			page 35


1733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SP__ This parameter can be one of the following values:
1786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
1787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
1788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
1789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
ARM GAS  /tmp/cc42qbQx.s 			page 36


1790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
1791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_SPDIFRX_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SP__) (((__I
1793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLI2SP__) >> RCC_PLLI2SCFGR_PLLI2SP_Pos) + 1U) * 2U))
1794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
1795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used for I2S domain
1798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_I2S_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetR ());
1800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
ARM GAS  /tmp/cc42qbQx.s 			page 37


1847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SR__ This parameter can be one of the following values:
1866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
1867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
1868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
1869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
1870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
1871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
1872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
1873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_I2S_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SR__) (((__INPUT
1875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLI2SR__) >> RCC_PLLI2SCFGR_PLLI2SR_Pos))
1876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the HCLK frequency
1879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __SYSCLKFREQ__ SYSCLK frequency (based on HSE/HSI/PLLCLK)
1880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __AHBPRESCALER__ This parameter can be one of the following values:
1881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
1882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
1883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
1884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
1885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
1886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
1887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
1888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
1889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
1890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval HCLK clock frequency (in Hz)
1891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_HCLK_FREQ(__SYSCLKFREQ__, __AHBPRESCALER__) ((__SYSCLKFREQ__) >> AHBPrescTabl
1893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PCLK1 frequency (ABP1)
1896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __HCLKFREQ__ HCLK frequency
1897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __APB1PRESCALER__ This parameter can be one of the following values:
1898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
1899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
1900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
1901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
1902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
1903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PCLK1 clock frequency (in Hz)
ARM GAS  /tmp/cc42qbQx.s 			page 38


1904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PCLK1_FREQ(__HCLKFREQ__, __APB1PRESCALER__) ((__HCLKFREQ__) >> APBPrescTable[
1906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PCLK2 frequency (ABP2)
1909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __HCLKFREQ__ HCLK frequency
1910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __APB2PRESCALER__ This parameter can be one of the following values:
1911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
1912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
1913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
1914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
1915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
1916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PCLK2 clock frequency (in Hz)
1917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PCLK2_FREQ(__HCLKFREQ__, __APB2PRESCALER__) ((__HCLKFREQ__) >> APBPrescTable[
1919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported functions --------------------------------------------------------*/
1929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Functions RCC Exported Functions
1930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_HSE HSE
1934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable the Clock Security System.
1939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           CSSON         LL_RCC_HSE_EnableCSS
1940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_EnableCSS(void)
1943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_CSSON);
1945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSE external oscillator (HSE Bypass)
1949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEBYP        LL_RCC_HSE_EnableBypass
1950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_EnableBypass(void)
1953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSEBYP);
1955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSE external oscillator (HSE Bypass)
1959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEBYP        LL_RCC_HSE_DisableBypass
1960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
ARM GAS  /tmp/cc42qbQx.s 			page 39


1961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_DisableBypass(void)
1963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSEBYP);
1965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSE crystal oscillator (HSE ON)
1969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEON         LL_RCC_HSE_Enable
1970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_Enable(void)
1973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSEON);
1975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSE crystal oscillator (HSE ON)
1979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEON         LL_RCC_HSE_Disable
1980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_Disable(void)
1983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSEON);
1985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if HSE oscillator Ready
1989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSERDY        LL_RCC_HSE_IsReady
1990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
1991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSE_IsReady(void)
1993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_HSERDY) == (RCC_CR_HSERDY));
1995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_HSI HSI
2002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSI oscillator
2007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSION         LL_RCC_HSI_Enable
2008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_Enable(void)
  41              		.loc 2 2010 22 view .LVU3
  42              	.LBB235:
2011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSION);
  43              		.loc 2 2012 3 view .LVU4
  44 0002 224A     		ldr	r2, .L7
  45 0004 1368     		ldr	r3, [r2]
ARM GAS  /tmp/cc42qbQx.s 			page 40


  46 0006 43F00103 		orr	r3, r3, #1
  47 000a 1360     		str	r3, [r2]
  48              	.LBE235:
  49              	.LBE234:
 168:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 169:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Wait for HSI READY bit */
 170:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   while(LL_RCC_HSI_IsReady() != 1U)
  50              		.loc 1 170 3 view .LVU5
  51              	.L2:
 171:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
  52              		.loc 1 171 4 view .LVU6
 170:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
  53              		.loc 1 170 30 discriminator 1 view .LVU7
  54              	.LBB236:
  55              	.LBI236:
2013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSI oscillator
2017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSION         LL_RCC_HSI_Disable
2018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_Disable(void)
2021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSION);
2023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if HSI clock is ready
2027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSIRDY        LL_RCC_HSI_IsReady
2028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_IsReady(void)
  56              		.loc 2 2030 26 view .LVU8
  57              	.LBB237:
2031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_HSIRDY) == (RCC_CR_HSIRDY));
  58              		.loc 2 2032 3 view .LVU9
  59              		.loc 2 2032 11 is_stmt 0 view .LVU10
  60 000c 1F4B     		ldr	r3, .L7
  61 000e 1B68     		ldr	r3, [r3]
  62              	.LBE237:
  63              	.LBE236:
 170:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
  64              		.loc 1 170 30 discriminator 1 view .LVU11
  65 0010 13F0020F 		tst	r3, #2
  66 0014 FAD0     		beq	.L2
 172:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 173:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset CFGR register */
 174:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_WriteReg(CFGR, 0x00000000U);
  67              		.loc 1 174 3 is_stmt 1 view .LVU12
  68 0016 1D4B     		ldr	r3, .L7
  69 0018 0022     		movs	r2, #0
  70 001a 9A60     		str	r2, [r3, #8]
 175:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 176:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Read CR register */
 177:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   vl_mask = LL_RCC_ReadReg(CR);
ARM GAS  /tmp/cc42qbQx.s 			page 41


  71              		.loc 1 177 3 view .LVU13
  72              		.loc 1 177 13 is_stmt 0 view .LVU14
  73 001c 1A68     		ldr	r2, [r3]
  74              		.loc 1 177 11 view .LVU15
  75 001e 0192     		str	r2, [sp, #4]
 178:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   
 179:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset HSEON, HSEBYP, PLLON, CSSON, PLLI2SON and PLLSAION bits */
 180:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   CLEAR_BIT(vl_mask, (RCC_CR_HSEON | RCC_CR_HSEBYP | RCC_CR_PLLON | RCC_CR_CSSON | RCC_CR_PLLSAION 
  76              		.loc 1 180 3 is_stmt 1 view .LVU16
  77 0020 0199     		ldr	r1, [sp, #4]
  78 0022 1B4A     		ldr	r2, .L7+4
  79 0024 0A40     		ands	r2, r2, r1
  80 0026 0192     		str	r2, [sp, #4]
 181:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 182:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Write new value in CR register */
 183:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_WriteReg(CR, vl_mask);
  81              		.loc 1 183 3 view .LVU17
  82 0028 019A     		ldr	r2, [sp, #4]
  83 002a 1A60     		str	r2, [r3]
 184:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 185:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Set HSITRIM bits to the reset value*/
 186:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_HSI_SetCalibTrimming(0x10U);
  84              		.loc 1 186 3 view .LVU18
  85              	.LVL0:
  86              	.LBB238:
  87              	.LBI238:
2033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSI Calibration value
2037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note When HSITRIM is written, HSICAL is updated with the sum of
2038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       HSITRIM and the factory trim value
2039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSICAL        LL_RCC_HSI_GetCalibration
2040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data = 0x00 and Max_Data = 0xFF
2041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_GetCalibration(void)
2043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CR, RCC_CR_HSICAL) >> RCC_CR_HSICAL_Pos);
2045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set HSI Calibration trimming
2049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note user-programmable trimming value that is added to the HSICAL
2050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Default value is 16, which, when added to the HSICAL value,
2051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       should trim the HSI to 16 MHz +/- 1 %
2052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSITRIM       LL_RCC_HSI_SetCalibTrimming
2053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Value Between Min_Data = 0 and Max_Data = 31
2054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_SetCalibTrimming(uint32_t Value)
  88              		.loc 2 2056 22 view .LVU19
  89              	.LBB239:
2057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CR, RCC_CR_HSITRIM, Value << RCC_CR_HSITRIM_Pos);
  90              		.loc 2 2058 3 view .LVU20
  91 002c 1A68     		ldr	r2, [r3]
  92 002e 22F0F802 		bic	r2, r2, #248
ARM GAS  /tmp/cc42qbQx.s 			page 42


  93 0032 42F08002 		orr	r2, r2, #128
  94 0036 1A60     		str	r2, [r3]
  95              	.LVL1:
  96              		.loc 2 2058 3 is_stmt 0 view .LVU21
  97              	.LBE239:
  98              	.LBE238:
 187:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 188:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Wait for PLL READY bit to be reset */
 189:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   while(LL_RCC_PLL_IsReady() != 0U)
  99              		.loc 1 189 3 is_stmt 1 view .LVU22
 100              	.L3:
 190:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 101              		.loc 1 190 4 view .LVU23
 189:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 102              		.loc 1 189 30 discriminator 1 view .LVU24
 103              	.LBB240:
 104              	.LBI240:
2059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSI Calibration trimming
2063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSITRIM       LL_RCC_HSI_GetCalibTrimming
2064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data = 0 and Max_Data = 31
2065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_GetCalibTrimming(void)
2067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CR, RCC_CR_HSITRIM) >> RCC_CR_HSITRIM_Pos);
2069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_LSE LSE
2076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable  Low Speed External (LSE) crystal.
2081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEON         LL_RCC_LSE_Enable
2082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_Enable(void)
2085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_LSEON);
2087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable  Low Speed External (LSE) crystal.
2091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEON         LL_RCC_LSE_Disable
2092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_Disable(void)
2095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_LSEON);
2097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 43


2099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable external clock source (LSE bypass).
2101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEBYP        LL_RCC_LSE_EnableBypass
2102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_EnableBypass(void)
2105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_LSEBYP);
2107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable external clock source (LSE bypass).
2111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEBYP        LL_RCC_LSE_DisableBypass
2112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_DisableBypass(void)
2115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_LSEBYP);
2117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set LSE oscillator drive capability
2121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note The oscillator is in Xtal mode when it is not in bypass mode.
2122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEDRV        LL_RCC_LSE_SetDriveCapability
2123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LSEDrive This parameter can be one of the following values:
2124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_LOW
2125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMHIGH
2126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMLOW
2127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_HIGH
2128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_SetDriveCapability(uint32_t LSEDrive)
2131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->BDCR, RCC_BDCR_LSEDRV, LSEDrive);
2133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get LSE oscillator drive capability
2137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEDRV        LL_RCC_LSE_GetDriveCapability
2138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_LOW
2140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMHIGH
2141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMLOW
2142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_HIGH
2143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSE_GetDriveCapability(void)
2145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->BDCR, RCC_BDCR_LSEDRV));
2147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if LSE oscillator Ready
2151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSERDY        LL_RCC_LSE_IsReady
2152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSE_IsReady(void)
2155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
ARM GAS  /tmp/cc42qbQx.s 			page 44


2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->BDCR, RCC_BDCR_LSERDY) == (RCC_BDCR_LSERDY));
2157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_LSI LSI
2164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable LSI Oscillator
2169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSION         LL_RCC_LSI_Enable
2170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSI_Enable(void)
2173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CSR, RCC_CSR_LSION);
2175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable LSI Oscillator
2179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSION         LL_RCC_LSI_Disable
2180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSI_Disable(void)
2183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CSR, RCC_CSR_LSION);
2185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if LSI is Ready
2189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSIRDY        LL_RCC_LSI_IsReady
2190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSI_IsReady(void)
2193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CSR, RCC_CSR_LSIRDY) == (RCC_CSR_LSIRDY));
2195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_System System
2202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure the system clock source
2207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         SW            LL_RCC_SetSysClkSource
2208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_HSI
2210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_HSE
2211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_PLL
2212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
ARM GAS  /tmp/cc42qbQx.s 			page 45


2213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSysClkSource(uint32_t Source)
2215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_SW, Source);
2217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get the system clock source
2221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         SWS           LL_RCC_GetSysClkSource
2222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_HSI
2224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_HSE
2225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_PLL
2226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSysClkSource(void)
2228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_SWS));
2230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set AHB prescaler
2234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         HPRE          LL_RCC_SetAHBPrescaler
2235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
2237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
2238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
2239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
2240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
2241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
2242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
2243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
2244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
2245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAHBPrescaler(uint32_t Prescaler)
2248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_HPRE, Prescaler);
2250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set APB1 prescaler
2254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE1         LL_RCC_SetAPB1Prescaler
2255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
2257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
2258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
2259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
2260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
2261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAPB1Prescaler(uint32_t Prescaler)
2264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_PPRE1, Prescaler);
2266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set APB2 prescaler
ARM GAS  /tmp/cc42qbQx.s 			page 46


2270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE2         LL_RCC_SetAPB2Prescaler
2271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
2273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
2274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
2275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
2276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
2277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAPB2Prescaler(uint32_t Prescaler)
2280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_PPRE2, Prescaler);
2282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get AHB prescaler
2286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         HPRE          LL_RCC_GetAHBPrescaler
2287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
2289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
2290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
2291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
2292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
2293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
2294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
2295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
2296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
2297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAHBPrescaler(void)
2299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_HPRE));
2301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get APB1 prescaler
2305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE1         LL_RCC_GetAPB1Prescaler
2306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
2308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
2309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
2310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
2311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
2312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAPB1Prescaler(void)
2314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_PPRE1));
2316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get APB2 prescaler
2320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE2         LL_RCC_GetAPB2Prescaler
2321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
2323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
2324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
2325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
2326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
ARM GAS  /tmp/cc42qbQx.s 			page 47


2327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAPB2Prescaler(void)
2329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_PPRE2));
2331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_MCO MCO
2338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure MCOx
2343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         MCO1          LL_RCC_ConfigMCO\n
2344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO1PRE       LL_RCC_ConfigMCO\n
2345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO2          LL_RCC_ConfigMCO\n
2346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO2PRE       LL_RCC_ConfigMCO
2347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  MCOxSource This parameter can be one of the following values:
2348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_HSI
2349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_LSE
2350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_HSE
2351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_PLLCLK
2352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_SYSCLK
2353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_PLLI2S
2354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_HSE
2355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_PLLCLK
2356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  MCOxPrescaler This parameter can be one of the following values:
2357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_1
2358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_2
2359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_3
2360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_4
2361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_5
2362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_1
2363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_2
2364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_3
2365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_4
2366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_5
2367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ConfigMCO(uint32_t MCOxSource, uint32_t MCOxPrescaler)
2370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, (MCOxSource & 0xFFFF0000U) | (MCOxPrescaler & 0xFFFF0000U),  (MCOxSource <<
2372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_Peripheral_Clock_Source Peripheral Clock Source
2379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure USARTx clock source
ARM GAS  /tmp/cc42qbQx.s 			page 48


2384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        USART1SEL     LL_RCC_SetUSARTClockSource\n
2385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART2SEL     LL_RCC_SetUSARTClockSource\n
2386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART3SEL     LL_RCC_SetUSARTClockSource\n
2387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART6SEL     LL_RCC_SetUSARTClockSource
2388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USARTxSource This parameter can be one of the following values:
2389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_PCLK2
2390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_SYSCLK
2391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_HSI
2392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_LSE
2393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_PCLK1
2394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_SYSCLK
2395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_HSI
2396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_LSE
2397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_PCLK1
2398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_SYSCLK
2399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_HSI
2400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_LSE
2401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_PCLK2
2402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_SYSCLK
2403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_HSI
2404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_LSE
2405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUSARTClockSource(uint32_t USARTxSource)
2408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (USARTxSource >> 16U), (USARTxSource & 0x0000FFFFU));
2410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure UARTx clock source
2414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        UART4SEL      LL_RCC_SetUARTClockSource\n
2415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART5SEL      LL_RCC_SetUARTClockSource\n
2416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART7SEL      LL_RCC_SetUARTClockSource\n
2417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART8SEL      LL_RCC_SetUARTClockSource
2418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  UARTxSource This parameter can be one of the following values:
2419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_PCLK1
2420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_SYSCLK
2421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_HSI
2422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_LSE
2423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_PCLK1
2424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_SYSCLK
2425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_HSI
2426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_LSE
2427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_PCLK1
2428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_SYSCLK
2429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_HSI
2430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_LSE
2431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_PCLK1
2432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_SYSCLK
2433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_HSI
2434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_LSE
2435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUARTClockSource(uint32_t UARTxSource)
2438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (UARTxSource >> 16U), (UARTxSource & 0x0000FFFFU));
2440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/cc42qbQx.s 			page 49


2441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure I2Cx clock source
2444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        I2C1SEL       LL_RCC_SetI2CClockSource\n
2445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C2SEL       LL_RCC_SetI2CClockSource\n
2446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C3SEL       LL_RCC_SetI2CClockSource\n
2447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C4SEL       LL_RCC_SetI2CClockSource
2448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2CxSource This parameter can be one of the following values:
2449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_PCLK1
2450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_SYSCLK
2451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_HSI
2452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_PCLK1
2453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_SYSCLK
2454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_HSI
2455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_PCLK1
2456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_SYSCLK
2457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_HSI
2458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_PCLK1 (*)
2459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_SYSCLK (*)
2460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_HSI (*)
2461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetI2CClockSource(uint32_t I2CxSource)
2466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (I2CxSource & 0xFFFF0000U),  (I2CxSource << 16U));
2468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure LPTIMx clock source
2472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        LPTIM1SEL     LL_RCC_SetLPTIMClockSource
2473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LPTIMxSource This parameter can be one of the following values:
2474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_PCLK1
2475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSI
2476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_HSI
2477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSE
2478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetLPTIMClockSource(uint32_t LPTIMxSource)
2481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_LPTIM1SEL, LPTIMxSource);
2483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure SAIx clock source
2487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1        SAI1SEL       LL_RCC_SetSAIClockSource\n
2488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1        SAI2SEL       LL_RCC_SetSAIClockSource
2489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SAIxSource This parameter can be one of the following values:
2490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSAI
2491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLI2S
2492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PIN
2493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSRC (*)
2494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSAI
2495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLI2S
2496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PIN
2497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSRC (*)
ARM GAS  /tmp/cc42qbQx.s 			page 50


2498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSAIClockSource(uint32_t SAIxSource)
2503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, (SAIxSource & 0xFFFF0000U), (SAIxSource << 16U));
2505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure SDMMC clock source
2509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        SDMMC1SEL      LL_RCC_SetSDMMCClockSource\n
2510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        SDMMC2SEL      LL_RCC_SetSDMMCClockSource
2511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SDMMCxSource This parameter can be one of the following values:
2512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK
2513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_SYSCLK
2514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK (*)
2515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_SYSCLK (*)
2516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSDMMCClockSource(uint32_t SDMMCxSource)
2521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (SDMMCxSource & 0xFFFF0000U), (SDMMCxSource << 16U));
2523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure 48Mhz domain clock source
2527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetCK48MClockSource
2528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CK48MxSource This parameter can be one of the following values:
2529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLL
2530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLLSAI
2531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetCK48MClockSource(uint32_t CK48MxSource)
2534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, CK48MxSource);
2536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure RNG clock source
2540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetRNGClockSource
2541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  RNGxSource This parameter can be one of the following values:
2542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLL
2543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLLSAI
2544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRNGClockSource(uint32_t RNGxSource)
2547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, RNGxSource);
2549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure USB clock source
2553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetUSBClockSource
2554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USBxSource This parameter can be one of the following values:
ARM GAS  /tmp/cc42qbQx.s 			page 51


2555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLL
2556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLLSAI
2557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUSBClockSource(uint32_t USBxSource)
2560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, USBxSource);
2562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
2565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure CEC clock source
2567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         CECSEL        LL_RCC_SetCECClockSource
2568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_LSE
2570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_HSI_DIV488
2571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetCECClockSource(uint32_t Source)
2574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CECSEL, Source);
2576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
2578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure I2S clock source
2581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         I2SSRC        LL_RCC_SetI2SClockSource
2582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PLLI2S
2584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PIN
2585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetI2SClockSource(uint32_t Source)
2588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_I2SSRC, Source);
2590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
2593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DSI clock source
2595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         DSISEL        LL_RCC_SetDSIClockSource
2596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PHY
2598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PLL
2599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDSIClockSource(uint32_t Source)
2602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_DSISEL, Source);
2604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
2606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
2608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DFSDM Audio clock source
2610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         ADFSDM1SEL        LL_RCC_SetDFSDMAudioClockSource
2611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
ARM GAS  /tmp/cc42qbQx.s 			page 52


2612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1
2613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2
2614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDFSDMAudioClockSource(uint32_t Source)
2617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_ADFSDM1SEL, Source);
2619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DFSDM Kernel clock source
2623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         DFSDM1SEL        LL_RCC_SetDFSDMClockSource
2624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_PCLK2
2626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_SYSCLK
2627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDFSDMClockSource(uint32_t Source)
2630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_DFSDM1SEL, Source);
2632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
2634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get USARTx clock source
2637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        USART1SEL     LL_RCC_GetUSARTClockSource\n
2638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART2SEL     LL_RCC_GetUSARTClockSource\n
2639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART3SEL     LL_RCC_GetUSARTClockSource\n
2640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART6SEL     LL_RCC_GetUSARTClockSource
2641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USARTx This parameter can be one of the following values:
2642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE
2643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE
2644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE
2645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE
2646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_PCLK2
2648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_SYSCLK
2649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_HSI
2650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_LSE
2651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_PCLK1
2652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_SYSCLK
2653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_HSI
2654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_LSE
2655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_PCLK1
2656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_SYSCLK
2657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_HSI
2658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_LSE
2659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_PCLK2
2660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_SYSCLK
2661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_HSI
2662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_LSE
2663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUSARTClockSource(uint32_t USARTx)
2665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, USARTx) | (USARTx << 16U));
2667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 53


2669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get UARTx clock source
2671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        UART4SEL      LL_RCC_GetUARTClockSource\n
2672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART5SEL      LL_RCC_GetUARTClockSource\n
2673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART7SEL      LL_RCC_GetUARTClockSource\n
2674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART8SEL      LL_RCC_GetUARTClockSource
2675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  UARTx This parameter can be one of the following values:
2676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE
2677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE
2678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE
2679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE
2680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_PCLK1
2682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_SYSCLK
2683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_HSI
2684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_LSE
2685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_PCLK1
2686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_SYSCLK
2687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_HSI
2688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_LSE
2689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_PCLK1
2690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_SYSCLK
2691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_HSI
2692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_LSE
2693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_PCLK1
2694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_SYSCLK
2695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_HSI
2696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_LSE
2697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUARTClockSource(uint32_t UARTx)
2699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, UARTx) | (UARTx << 16U));
2701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2Cx clock source
2705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        I2C1SEL       LL_RCC_GetI2CClockSource\n
2706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C2SEL       LL_RCC_GetI2CClockSource\n
2707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C3SEL       LL_RCC_GetI2CClockSource\n
2708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C4SEL       LL_RCC_GetI2CClockSource
2709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2Cx This parameter can be one of the following values:
2710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE
2711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE
2712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE
2713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE (*)
2714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_PCLK1
2716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_SYSCLK
2717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_HSI
2718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_PCLK1
2719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_SYSCLK
2720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_HSI
2721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_PCLK1
2722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_SYSCLK
2723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_HSI
2724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_PCLK1 (*)
2725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_SYSCLK (*)
ARM GAS  /tmp/cc42qbQx.s 			page 54


2726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_HSI (*)
2727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****  */
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetI2CClockSource(uint32_t I2Cx)
2731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)((READ_BIT(RCC->DCKCFGR2, I2Cx) >> 16U) | I2Cx);
2733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get LPTIMx clock source
2737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        LPTIM1SEL     LL_RCC_GetLPTIMClockSource
2738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LPTIMx This parameter can be one of the following values:
2739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE
2740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_PCLK1
2742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSI
2743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_HSI
2744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSE
2745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetLPTIMClockSource(uint32_t LPTIMx)
2747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, RCC_DCKCFGR2_LPTIM1SEL));
2749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIx clock source
2753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1        SAI1SEL       LL_RCC_GetSAIClockSource\n
2754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1        SAI2SEL       LL_RCC_GetSAIClockSource
2755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SAIx This parameter can be one of the following values:
2756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE
2757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE
2758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSAI
2760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLI2S
2761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PIN
2762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSRC (*)
2763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSAI
2764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLI2S
2765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PIN
2766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSRC (*)
2767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSAIClockSource(uint32_t SAIx)
2771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, SAIx) >> 16U | SAIx);
2773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SDMMCx clock source
2777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        SDMMC1SEL      LL_RCC_GetSDMMCClockSource\n
2778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        SDMMC2SEL      LL_RCC_GetSDMMCClockSource
2779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SDMMCx This parameter can be one of the following values:
2780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE
2781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE (*)
2782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
ARM GAS  /tmp/cc42qbQx.s 			page 55


2783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK
2784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_SYSCLK
2785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK (*)
2786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_SYSCLK (*)
2787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSDMMCClockSource(uint32_t SDMMCx)
2791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, SDMMCx) >> 16U | SDMMCx);
2793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get 48Mhz domain clock source
2797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetCK48MClockSource
2798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CK48Mx This parameter can be one of the following values:
2799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE
2800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLL
2802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLLSAI
2803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetCK48MClockSource(uint32_t CK48Mx)
2805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, CK48Mx));
2807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get RNGx clock source
2811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetRNGClockSource
2812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  RNGx This parameter can be one of the following values:
2813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE
2814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLL
2816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLLSAI
2817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRNGClockSource(uint32_t RNGx)
2819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, RNGx));
2821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get USBx clock source
2825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetUSBClockSource
2826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USBx This parameter can be one of the following values:
2827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE
2828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLL
2830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLLSAI
2831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUSBClockSource(uint32_t USBx)
2833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, USBx));
2835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
2838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get CEC Clock Source
ARM GAS  /tmp/cc42qbQx.s 			page 56


2840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         CECSEL        LL_RCC_GetCECClockSource
2841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CECx This parameter can be one of the following values:
2842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE
2843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_LSE
2845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_HSI_DIV488
2846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetCECClockSource(uint32_t CECx)
2848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, CECx));
2850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
2852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2S Clock Source
2855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         I2SSRC        LL_RCC_GetI2SClockSource
2856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2Sx This parameter can be one of the following values:
2857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE
2858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PLLI2S
2860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PIN
2861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetI2SClockSource(uint32_t I2Sx)
2863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, I2Sx));
2865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
2868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DFSDM Audio Clock Source
2870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         ADFSDM1SEL        LL_RCC_GetDFSDMAudioClockSource
2871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DFSDMx This parameter can be one of the following values:
2872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE
2873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1
2875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2
2876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDFSDMAudioClockSource(uint32_t DFSDMx)
2878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, DFSDMx));
2880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DFSDM Audio Clock Source
2884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         DFSDM1SEL        LL_RCC_GetDFSDMClockSource
2885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DFSDMx This parameter can be one of the following values:
2886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE
2887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_PCLK2
2889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_SYSCLK
2890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDFSDMClockSource(uint32_t DFSDMx)
2892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, DFSDMx));
2894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
2896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 57


2897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
2898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DSI Clock Source
2900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         DSISEL        LL_RCC_GetDSIClockSource
2901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DSIx This parameter can be one of the following values:
2902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE
2903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PHY
2905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PLL
2906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDSIClockSource(uint32_t DSIx)
2908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, DSIx));
2910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
2912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_RTC RTC
2918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set RTC Clock Source
2923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Once the RTC clock source has been selected, it cannot be changed anymore unless
2924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       the Backup domain is reset, or unless a failure is detected on LSE (LSECSSD is
2925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       set). The BDRST bit can be used to reset them.
2926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCSEL        LL_RCC_SetRTCClockSource
2927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_NONE
2929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSE
2930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSI
2931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_HSE
2932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRTCClockSource(uint32_t Source)
2935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->BDCR, RCC_BDCR_RTCSEL, Source);
2937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get RTC Clock Source
2941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCSEL        LL_RCC_GetRTCClockSource
2942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_NONE
2944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSE
2945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSI
2946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_HSE
2947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRTCClockSource(void)
2949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->BDCR, RCC_BDCR_RTCSEL));
2951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/cc42qbQx.s 			page 58


2954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable RTC
2955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_EnableRTC
2956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_EnableRTC(void)
2959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_RTCEN);
2961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable RTC
2965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_DisableRTC
2966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_DisableRTC(void)
2969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_RTCEN);
2971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if RTC has been enabled or not
2975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_IsEnabledRTC
2976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_IsEnabledRTC(void)
2979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->BDCR, RCC_BDCR_RTCEN) == (RCC_BDCR_RTCEN));
2981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Force the Backup domain reset
2985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         BDRST         LL_RCC_ForceBackupDomainReset
2986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ForceBackupDomainReset(void)
2989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_BDRST);
2991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Release the Backup domain reset
2995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         BDRST         LL_RCC_ReleaseBackupDomainReset
2996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ReleaseBackupDomainReset(void)
2999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_BDRST);
3001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set HSE Prescalers for RTC Clock
3005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         RTCPRE        LL_RCC_SetRTC_HSEPrescaler
3006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
3007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_NOCLOCK
3008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_2
3009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_3
3010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_4
ARM GAS  /tmp/cc42qbQx.s 			page 59


3011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_5
3012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_6
3013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_7
3014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_8
3015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_9
3016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_10
3017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_11
3018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_12
3019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_13
3020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_14
3021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_15
3022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_16
3023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_17
3024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_18
3025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_19
3026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_20
3027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_21
3028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_22
3029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_23
3030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_24
3031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_25
3032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_26
3033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_27
3034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_28
3035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_29
3036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_30
3037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_31
3038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRTC_HSEPrescaler(uint32_t Prescaler)
3041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_RTCPRE, Prescaler);
3043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSE Prescalers for RTC Clock
3047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         RTCPRE        LL_RCC_GetRTC_HSEPrescaler
3048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_NOCLOCK
3050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_2
3051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_3
3052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_4
3053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_5
3054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_6
3055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_7
3056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_8
3057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_9
3058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_10
3059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_11
3060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_12
3061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_13
3062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_14
3063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_15
3064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_16
3065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_17
3066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_18
3067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_19
ARM GAS  /tmp/cc42qbQx.s 			page 60


3068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_20
3069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_21
3070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_22
3071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_23
3072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_24
3073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_25
3074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_26
3075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_27
3076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_28
3077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_29
3078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_30
3079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_31
3080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRTC_HSEPrescaler(void)
3082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_RTCPRE));
3084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
3088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_TIM_CLOCK_PRESCALER TIM
3091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
3092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set Timers Clock Prescalers
3096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         TIMPRE        LL_RCC_SetTIMPrescaler
3097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
3098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_TWICE
3099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_FOUR_TIMES
3100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetTIMPrescaler(uint32_t Prescaler)
3103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_TIMPRE, Prescaler);
3105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Timers Clock Prescalers
3109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         TIMPRE        LL_RCC_GetTIMPrescaler
3110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_TWICE
3112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_FOUR_TIMES
3113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetTIMPrescaler(void)
3115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_TIMPRE));
3117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
3121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLL PLL
3124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
ARM GAS  /tmp/cc42qbQx.s 			page 61


3125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLL
3129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLON         LL_RCC_PLL_Enable
3130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_Enable(void)
3133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLON);
3135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLL
3139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Cannot be disabled if the PLL clock is used as the system clock
3140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLON         LL_RCC_PLL_Disable
3141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_Disable(void)
3144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLON);
3146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLL Ready
3150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLRDY        LL_RCC_PLL_IsReady
3151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
3152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_IsReady(void)
 105              		.loc 2 3153 26 view .LVU25
 106              	.LBB241:
3154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLRDY) == (RCC_CR_PLLRDY));
 107              		.loc 2 3155 3 view .LVU26
 108              		.loc 2 3155 11 is_stmt 0 view .LVU27
 109 0038 144B     		ldr	r3, .L7
 110 003a 1B68     		ldr	r3, [r3]
 111              	.LBE241:
 112              	.LBE240:
 189:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 113              		.loc 1 189 30 discriminator 1 view .LVU28
 114 003c 13F0007F 		tst	r3, #33554432
 115 0040 FAD1     		bne	.L3
 116              	.L4:
 191:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 192:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Wait for PLLI2S READY bit to be reset */
 193:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   while(LL_RCC_PLLI2S_IsReady() != 0U)
 194:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 117              		.loc 1 194 4 is_stmt 1 view .LVU29
 193:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 118              		.loc 1 193 33 discriminator 1 view .LVU30
 119              	.LBB242:
 120              	.LBI242:
3156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for SYSCLK Domain
ARM GAS  /tmp/cc42qbQx.s 			page 62


3160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLP can be written only when PLL is disabled
3163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_SYS\n
3164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_SYS\n
3165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_SYS\n
3166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLP          LL_RCC_PLL_ConfigDomain_SYS
3167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
ARM GAS  /tmp/cc42qbQx.s 			page 63


3217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLP This parameter can be one of the following values:
3235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
3236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
3237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
3238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
3239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_SYS(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
3245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for 48Mhz domain clock
3249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLQ can be written only when PLL is disabled
3252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for USB, RNG, SDMMC1
3253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_48M\n
3254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_48M\n
3255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_48M\n
3256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLQ          LL_RCC_PLL_ConfigDomain_48M
3257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
ARM GAS  /tmp/cc42qbQx.s 			page 64


3274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLQ This parameter can be one of the following values:
3325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
3326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
3327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
3328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
3329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
3330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
ARM GAS  /tmp/cc42qbQx.s 			page 65


3331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
3332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
3333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
3334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
3335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
3336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
3337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
3338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
3339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_48M(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLQ);
3345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
3348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for DSI clock
3350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLR can be written only when PLL is disabled
3353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for DSI
3354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_DSI\n
3355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_DSI\n
3356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_DSI\n
3357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLR          LL_RCC_PLL_ConfigDomain_DSI
3358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
ARM GAS  /tmp/cc42qbQx.s 			page 66


3388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLR This parameter can be one of the following values:
3426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
3427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
3428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
3429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
3430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
3431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
3432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_DSI(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLR);
3438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
3440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL clock source
3443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_SetMainSource
3444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param PLLSource This parameter can be one of the following values:
ARM GAS  /tmp/cc42qbQx.s 			page 67


3445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SetMainSource(uint32_t PLLSource)
3450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC, PLLSource);
3452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get the oscillator used as PLL clock source.
3456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_GetMainSource
3457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetMainSource(void)
3462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC));
3464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL multiplication factor for VCO
3468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLN          LL_RCC_PLL_GetN
3469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between 50 and 432
3470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetN(void)
3472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLN) >>  RCC_PLLCFGR_PLLN_Pos);
3474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLP 
3478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLP       LL_RCC_PLL_GetP
3479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
3481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
3482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
3483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
3484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetP(void)
3486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLP));
3488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLQ
3492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLL48MCLK selected for USB, RNG, SDMMC (48 MHz clock)
3493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLQ          LL_RCC_PLL_GetQ
3494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
3496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
3497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
3498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
3499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
3500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
3501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
ARM GAS  /tmp/cc42qbQx.s 			page 68


3502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
3503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
3504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
3505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
3506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
3507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
3508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
3509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetQ(void)
3511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLQ));
3513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLCFGR_PLLR)
3516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLR
3518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLCLK (system clock)
3519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLR          LL_RCC_PLL_GetR
3520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
3522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
3523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
3524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
3525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
3526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
3527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetR(void)
3529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLR));
3531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLCFGR_PLLR */
3533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Division factor for the main PLL and other PLL
3536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLM          LL_RCC_PLL_GetDivider
3537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
ARM GAS  /tmp/cc42qbQx.s 			page 69


3559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetDivider(void)
3602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLM));
3604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure Spread Spectrum used for PLL
3608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note These bits must be written before enabling PLL
3609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR        MODPER        LL_RCC_PLL_ConfigSpreadSpectrum\n
3610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         SSCGR        INCSTEP       LL_RCC_PLL_ConfigSpreadSpectrum\n
3611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         SSCGR        SPREADSEL     LL_RCC_PLL_ConfigSpreadSpectrum
3612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Mod Between Min_Data=0 and Max_Data=8191
3613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Inc Between Min_Data=0 and Max_Data=32767
3614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Sel This parameter can be one of the following values:
3615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_CENTER
ARM GAS  /tmp/cc42qbQx.s 			page 70


3616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_DOWN
3617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigSpreadSpectrum(uint32_t Mod, uint32_t Inc, uint32_t Sel)
3620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->SSCGR, RCC_SSCGR_MODPER | RCC_SSCGR_INCSTEP | RCC_SSCGR_SPREADSEL, Mod | (Inc << 
3622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Modulation Period for PLL
3626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         MODPER        LL_RCC_PLL_GetPeriodModulation
3627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data=0 and Max_Data=8191
3628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetPeriodModulation(void)
3630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_MODPER));
3632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Incrementation Step for PLL
3636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Must be written before enabling PLL
3637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         INCSTEP        LL_RCC_PLL_GetStepIncrementation
3638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data=0 and Max_Data=32767
3639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetStepIncrementation(void)
3641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_INCSTEP) >> RCC_SSCGR_INCSTEP_Pos);
3643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Selection for PLL
3647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Must be written before enabling PLL
3648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SPREADSEL        LL_RCC_PLL_GetSpreadSelection
3649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_CENTER
3651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_DOWN
3652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetSpreadSelection(void)
3654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_SPREADSEL));
3656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable Spread Spectrum for PLL.
3660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SSCGEN         LL_RCC_PLL_SpreadSpectrum_Enable
3661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SpreadSpectrum_Enable(void)
3664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->SSCGR, RCC_SSCGR_SSCGEN);
3666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable Spread Spectrum for PLL.
3670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SSCGEN         LL_RCC_PLL_SpreadSpectrum_Disable
3671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 71


3673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SpreadSpectrum_Disable(void)
3674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->SSCGR, RCC_SSCGR_SSCGEN);
3676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
3680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLLI2S PLLI2S
3683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
3684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLLI2S
3688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SON     LL_RCC_PLLI2S_Enable
3689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_Enable(void)
3692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLI2SON);
3694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLLI2S
3698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SON     LL_RCC_PLLI2S_Disable
3699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_Disable(void)
3702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLI2SON);
3704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLLI2S Ready
3708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SRDY    LL_RCC_PLLI2S_IsReady
3709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
3710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_IsReady(void)
 121              		.loc 2 3711 26 view .LVU31
 122              	.LBB243:
3712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLI2SRDY) == (RCC_CR_PLLI2SRDY));
 123              		.loc 2 3713 3 view .LVU32
 124              		.loc 2 3713 11 is_stmt 0 view .LVU33
 125 0042 124B     		ldr	r3, .L7
 126 0044 1B68     		ldr	r3, [r3]
 127              	.LBE243:
 128              	.LBE242:
 193:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 129              		.loc 1 193 33 discriminator 1 view .LVU34
 130 0046 13F0006F 		tst	r3, #134217728
 131 004a FAD1     		bne	.L4
 132              	.L5:
 195:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 196:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Wait for PLLSAI READY bit to be reset */
 197:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   while(LL_RCC_PLLSAI_IsReady() != 0U)
ARM GAS  /tmp/cc42qbQx.s 			page 72


 198:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 133              		.loc 1 198 4 is_stmt 1 view .LVU35
 197:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 134              		.loc 1 197 33 discriminator 1 view .LVU36
 135              	.LBB244:
 136              	.LBI244:
3714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLI2S used for SAI1 and SAI2 domain clock
3718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLQ can be written only when PLLI2S is disabled
3721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This can be selected for SAI1 and SAI2
3722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_SAI\n
3723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_SAI\n
3724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_SAI\n
3725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SQ       LL_RCC_PLLI2S_ConfigDomain_SAI\n
3726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1      PLLI2SDIVQ    LL_RCC_PLLI2S_ConfigDomain_SAI
3727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
ARM GAS  /tmp/cc42qbQx.s 			page 73


3765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLQ This parameter can be one of the following values:
3795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
3796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
3797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
3798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
3799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
3800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
3801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
3802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
3803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
3804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
3805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
3806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
3807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
3808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
3809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLDIVQ This parameter can be one of the following values:
3810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
3811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
3812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
3813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
3814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
3815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
3816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
3817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
3818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
3819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
3820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
3821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
ARM GAS  /tmp/cc42qbQx.s 			page 74


3822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
3823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
3824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
3825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
3826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
3827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
3828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
3829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
3830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
3831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
3832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
3833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
3834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
3835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
3836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
3837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
3838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
3839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
3840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
3841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
3842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_SAI(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
3845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
3847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SQ, PLLN << RCC_PLLI2SCF
3848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLI2SDIVQ, PLLDIVQ);
3849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
3852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief Configure PLLI2S used for SPDIFRX domain clock
3854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLP can be written only when PLLI2S is disabled
3857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for SPDIFRX
3858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SP       LL_RCC_PLLI2S_ConfigDomain_SPDIFRX
3862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
ARM GAS  /tmp/cc42qbQx.s 			page 75


3879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLP This parameter can be one of the following values:
3930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
3931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
3932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
3933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
3934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 76


3936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_SPDIFRX(uint32_t Source, uint32_t PLLM, uint32_t PL
3937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
3939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SP, PLLN << RCC_PLLI2SCF
3940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
3942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLI2S used for I2S1 domain clock
3945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLR can be written only when PLLI2S is disabled
3948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for I2S
3949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_I2S\n
3950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_I2S\n
3951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_I2S\n
3952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SR       LL_RCC_PLLI2S_ConfigDomain_I2S
3953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
ARM GAS  /tmp/cc42qbQx.s 			page 77


3993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
4000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
4001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
4002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
4003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
4004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
4005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
4006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
4007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
4008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
4009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
4010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
4011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
4012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
4013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
4014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
4015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
4016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
4017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
4018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
4019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
4020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLR This parameter can be one of the following values:
4021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
4022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
4023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
4024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
4025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
4026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
4027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_I2S(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
4030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
4032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SR, PLLN << RCC_PLLI2SCF
4033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL multiplication factor for VCO
4037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SN      LL_RCC_PLLI2S_GetN
4038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between 50 and 432
4039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetN(void)
4041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN) >> RCC_PLLI2SCFGR_PLLI2SN_Pos
4043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SQ
4047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SQ      LL_RCC_PLLI2S_GetQ
4048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
ARM GAS  /tmp/cc42qbQx.s 			page 78


4050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
4051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
4052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
4053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
4054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
4055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
4056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
4057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
4058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
4059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
4060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
4061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
4062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
4063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetQ(void)
4065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SQ));
4067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SR
4071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLI2SCLK (I2S clock)
4072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SR      LL_RCC_PLLI2S_GetR
4073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
4075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
4076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
4077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
4078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
4079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
4080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetR(void)
4082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SR));
4084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLI2SCFGR_PLLI2SP)
4087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SP
4089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLSPDIFRXCLK (SPDIFRX clock)
4090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SP      LL_RCC_PLLI2S_GetP
4091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
4093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
4094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
4095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
4096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetP(void)
4098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SP));
4100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLI2SCFGR_PLLI2SP */
4102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SDIVQ
4105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used PLLSAI1CLK, PLLSAI2CLK selected (SAI1 and SAI2 clock)
4106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1   PLLI2SDIVQ      LL_RCC_PLLI2S_GetDIVQ
ARM GAS  /tmp/cc42qbQx.s 			page 79


4107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
4109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
4110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
4111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
4112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
4113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
4114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
4115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
4116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
4117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
4118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
4119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
4120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
4121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
4122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
4123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
4124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
4125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
4126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
4127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
4128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
4129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
4130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
4131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
4132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
4133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
4134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
4135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
4136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
4137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
4138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
4139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
4140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetDIVQ(void)
4142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLI2SDIVQ));
4144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
4148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLLSAI PLLSAI
4151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
4152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLLSAI
4156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAION     LL_RCC_PLLSAI_Enable
4157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_Enable(void)
4160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLSAION);
4162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/cc42qbQx.s 			page 80


4164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLLSAI
4166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAION     LL_RCC_PLLSAI_Disable
4167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_Disable(void)
4170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLSAION);
4172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLLSAI Ready
4176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAIRDY    LL_RCC_PLLSAI_IsReady
4177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
4178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_IsReady(void)
 137              		.loc 2 4179 26 view .LVU37
 138              	.LBB245:
4180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLSAIRDY) == (RCC_CR_PLLSAIRDY));
 139              		.loc 2 4181 3 view .LVU38
 140              		.loc 2 4181 11 is_stmt 0 view .LVU39
 141 004c 0F4B     		ldr	r3, .L7
 142 004e 1B68     		ldr	r3, [r3]
 143              	.LBE245:
 144              	.LBE244:
 197:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {}
 145              		.loc 1 197 33 discriminator 1 view .LVU40
 146 0050 13F0005F 		tst	r3, #536870912
 147 0054 FAD1     		bne	.L5
 199:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 200:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset PLLCFGR register */
 201:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_WriteReg(PLLCFGR, 0x24003010U);
 148              		.loc 1 201 3 is_stmt 1 view .LVU41
 149 0056 0D4B     		ldr	r3, .L7
 150 0058 0E4A     		ldr	r2, .L7+8
 151 005a 5A60     		str	r2, [r3, #4]
 202:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 203:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset PLLI2SCFGR register */
 204:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_WriteReg(PLLI2SCFGR, 0x24003000U);
 152              		.loc 1 204 3 view .LVU42
 153 005c 103A     		subs	r2, r2, #16
 154 005e C3F88420 		str	r2, [r3, #132]
 205:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 206:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset PLLSAICFGR register */
 207:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   LL_RCC_WriteReg(PLLSAICFGR, 0x24003000U);
 155              		.loc 1 207 3 view .LVU43
 156 0062 C3F88820 		str	r2, [r3, #136]
 208:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 209:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Disable all interrupts */
 210:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   CLEAR_BIT(RCC->CIR, RCC_CIR_LSIRDYIE | RCC_CIR_LSERDYIE | RCC_CIR_HSIRDYIE | RCC_CIR_HSERDYIE | R
 157              		.loc 1 210 3 view .LVU44
 158 0066 DA68     		ldr	r2, [r3, #12]
 159 0068 22F4FE42 		bic	r2, r2, #32512
 160 006c DA60     		str	r2, [r3, #12]
 211:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 212:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Clear all interrupt flags */
ARM GAS  /tmp/cc42qbQx.s 			page 81


 213:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   SET_BIT(RCC->CIR, RCC_CIR_LSIRDYC | RCC_CIR_LSERDYC | RCC_CIR_HSIRDYC | RCC_CIR_HSERDYC | RCC_CIR
 161              		.loc 1 213 3 view .LVU45
 162 006e DA68     		ldr	r2, [r3, #12]
 163 0070 42F47F02 		orr	r2, r2, #16711680
 164 0074 DA60     		str	r2, [r3, #12]
 214:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 215:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Clear LSION bit */
 216:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   CLEAR_BIT(RCC->CSR, RCC_CSR_LSION);
 165              		.loc 1 216 3 view .LVU46
 166 0076 5A6F     		ldr	r2, [r3, #116]
 167 0078 22F00102 		bic	r2, r2, #1
 168 007c 5A67     		str	r2, [r3, #116]
 217:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 218:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Reset all CSR flags */
 219:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   SET_BIT(RCC->CSR, RCC_CSR_RMVF);
 169              		.loc 1 219 3 view .LVU47
 170 007e 5A6F     		ldr	r2, [r3, #116]
 171 0080 42F08072 		orr	r2, r2, #16777216
 172 0084 5A67     		str	r2, [r3, #116]
 220:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 221:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return SUCCESS;
 173              		.loc 1 221 3 view .LVU48
 222:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 174              		.loc 1 222 1 is_stmt 0 view .LVU49
 175 0086 0020     		movs	r0, #0
 176 0088 02B0     		add	sp, sp, #8
 177              	.LCFI1:
 178              		.cfi_def_cfa_offset 0
 179              		@ sp needed
 180 008a 7047     		bx	lr
 181              	.L8:
 182              		.align	2
 183              	.L7:
 184 008c 00380240 		.word	1073887232
 185 0090 FFFFF2EA 		.word	-353173505
 186 0094 10300024 		.word	603992080
 187              		.cfi_endproc
 188              	.LFE295:
 190              		.section	.text.LL_RCC_GetCECClockFreq,"ax",%progbits
 191              		.align	1
 192              		.global	LL_RCC_GetCECClockFreq
 193              		.syntax unified
 194              		.thumb
 195              		.thumb_func
 197              	LL_RCC_GetCECClockFreq:
 198              	.LVL2:
 199              	.LFB305:
 223:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 224:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 225:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @}
 226:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 227:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 228:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL_EF_Get_Freq
 229:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return the frequencies of different on chip clocks;  System, AHB, APB1 and APB2 buses c
 230:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         and different peripheral clocks available on the device.
 231:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   If SYSCLK source is HSI, function returns values based on HSI_VALUE(**)
 232:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   If SYSCLK source is HSE, function returns values based on HSE_VALUE(***)
ARM GAS  /tmp/cc42qbQx.s 			page 82


 233:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   If SYSCLK source is PLL, function returns values based on HSE_VALUE(***)
 234:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         or HSI_VALUE(**) multiplied/divided by the PLL factors.
 235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   (**) HSI_VALUE is a constant defined in this file (default value
 236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *              16 MHz) but the real value may vary depending on the variations
 237:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *              in voltage and temperature.
 238:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   (***) HSE_VALUE is a constant defined in this file (default value
 239:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *               25 MHz), user has to ensure that HSE_VALUE is same as the real
 240:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *               frequency of the crystal used. Otherwise, this function may
 241:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *               have wrong result.
 242:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   The result of this function could be incorrect when using fractional
 243:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         value for HSE crystal.
 244:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   This function can be used by the user application to compute the
 245:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         baud-rate for the communication peripherals or configure other parameters.
 246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
 247:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 249:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return the frequencies of different on chip clocks;  System, AHB, APB1 and APB2 buses c
 251:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @note   Each time SYSCLK, HCLK, PCLK1 and/or PCLK2 clock changes, this function
 252:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         must be called to update structure fields. Otherwise, any
 253:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         configuration based on this function will be incorrect.
 254:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  RCC_Clocks pointer to a @ref LL_RCC_ClocksTypeDef structure which will hold the clocks 
 255:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval None
 256:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 257:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** void LL_RCC_GetSystemClocksFreq(LL_RCC_ClocksTypeDef *RCC_Clocks)
 258:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 259:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Get SYSCLK frequency */
 260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   RCC_Clocks->SYSCLK_Frequency = RCC_GetSystemClockFreq();
 261:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 262:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* HCLK clock frequency */
 263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   RCC_Clocks->HCLK_Frequency   = RCC_GetHCLKClockFreq(RCC_Clocks->SYSCLK_Frequency);
 264:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 265:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PCLK1 clock frequency */
 266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   RCC_Clocks->PCLK1_Frequency  = RCC_GetPCLK1ClockFreq(RCC_Clocks->HCLK_Frequency);
 267:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 268:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PCLK2 clock frequency */
 269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   RCC_Clocks->PCLK2_Frequency  = RCC_GetPCLK2ClockFreq(RCC_Clocks->HCLK_Frequency);
 270:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 271:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 272:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 273:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return USARTx clock frequency
 274:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  USARTxSource This parameter can be one of the following values:
 275:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE
 276:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE
 277:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE
 278:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE
 279:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval USART clock frequency (in Hz)
 280:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator (HSI or LSE) is not ready
 281:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 282:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetUSARTClockFreq(uint32_t USARTxSource)
 283:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 284:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 285:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 286:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 287:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_USART_CLKSOURCE(USARTxSource));
 288:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 289:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (USARTxSource == LL_RCC_USART1_CLKSOURCE)
ARM GAS  /tmp/cc42qbQx.s 			page 83


 290:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 291:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* USART1CLK clock frequency */
 292:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUSARTClockSource(USARTxSource))
 293:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 294:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART1_CLKSOURCE_SYSCLK: /* USART1 Clock is System Clock */
 295:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetSystemClockFreq();
 296:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 297:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 298:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART1_CLKSOURCE_HSI:    /* USART1 Clock is HSI Osc. */
 299:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 300:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 301:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = HSI_VALUE;
 302:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 303:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 304:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 305:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART1_CLKSOURCE_LSE:    /* USART1 Clock is LSE Osc. */
 306:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 307:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 308:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = LSE_VALUE;
 309:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 310:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 311:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 312:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART1_CLKSOURCE_PCLK2:  /* USART1 Clock is PCLK2 */
 313:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetPCLK2ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 315:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 316:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 317:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 318:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (USARTxSource == LL_RCC_USART2_CLKSOURCE)
 319:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 320:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* USART2CLK clock frequency */
 321:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUSARTClockSource(USARTxSource))
 322:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 323:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART2_CLKSOURCE_SYSCLK: /* USART2 Clock is System Clock */
 324:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetSystemClockFreq();
 325:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 326:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 327:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART2_CLKSOURCE_HSI:    /* USART2 Clock is HSI Osc. */
 328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 329:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = HSI_VALUE;
 331:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 332:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 333:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 334:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART2_CLKSOURCE_LSE:    /* USART2 Clock is LSE Osc. */
 335:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 336:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 337:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = LSE_VALUE;
 338:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 339:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 340:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 341:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART2_CLKSOURCE_PCLK1:  /* USART2 Clock is PCLK1 */
 342:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 345:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 346:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
ARM GAS  /tmp/cc42qbQx.s 			page 84


 347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (USARTxSource == LL_RCC_USART6_CLKSOURCE)
 348:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 349:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* USART6CLK clock frequency */
 350:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUSARTClockSource(USARTxSource))
 351:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 352:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART6_CLKSOURCE_SYSCLK: /* USART6 Clock is System Clock */
 353:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetSystemClockFreq();
 354:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 356:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART6_CLKSOURCE_HSI:    /* USART6 Clock is HSI Osc. */
 357:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 358:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 359:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = HSI_VALUE;
 360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 361:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 362:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 363:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART6_CLKSOURCE_LSE:    /* USART6 Clock is LSE Osc. */
 364:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 366:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = LSE_VALUE;
 367:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 368:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 369:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_USART6_CLKSOURCE_PCLK2:  /* USART6 Clock is PCLK2 */
 371:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usart_frequency = RCC_GetPCLK2ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 374:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 375:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 376:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 378:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     if (USARTxSource == LL_RCC_USART3_CLKSOURCE)
 379:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 380:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       /* USART3CLK clock frequency */
 381:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       switch (LL_RCC_GetUSARTClockSource(USARTxSource))
 382:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 383:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_USART3_CLKSOURCE_SYSCLK: /* USART3 Clock is System Clock */
 384:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = RCC_GetSystemClockFreq();
 385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 386:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 387:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_USART3_CLKSOURCE_HSI:    /* USART3 Clock is HSI Osc. */
 388:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           if (LL_RCC_HSI_IsReady())
 389:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             usart_frequency = HSI_VALUE;
 391:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 392:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 393:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 394:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_USART3_CLKSOURCE_LSE:    /* USART3 Clock is LSE Osc. */
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           if (LL_RCC_LSE_IsReady())
 396:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             usart_frequency = LSE_VALUE;
 398:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 399:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 400:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 401:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_USART3_CLKSOURCE_PCLK1:  /* USART3 Clock is PCLK1 */
 402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         default:
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           usart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
ARM GAS  /tmp/cc42qbQx.s 			page 85


 404:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 405:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 406:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 407:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 408:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return usart_frequency;
 409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 410:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 411:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 412:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return UARTx clock frequency
 413:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  UARTxSource This parameter can be one of the following values:
 414:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE
 415:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE
 416:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE
 417:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE
 418:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval UART clock frequency (in Hz)
 419:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator (HSI or LSE) is not ready
 420:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 421:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetUARTClockFreq(uint32_t UARTxSource)
 422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 423:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t uart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 424:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 425:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 426:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_UART_CLKSOURCE(UARTxSource));
 427:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 428:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (UARTxSource == LL_RCC_UART4_CLKSOURCE)
 429:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 430:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* UART4CLK clock frequency */
 431:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUARTClockSource(UARTxSource))
 432:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 433:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART4_CLKSOURCE_SYSCLK: /* UART4 Clock is System Clock */
 434:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetSystemClockFreq();
 435:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 436:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 437:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART4_CLKSOURCE_HSI:    /* UART4 Clock is HSI Osc. */
 438:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 439:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 440:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = HSI_VALUE;
 441:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 442:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 443:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 444:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART4_CLKSOURCE_LSE:    /* UART4 Clock is LSE Osc. */
 445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 446:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 447:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = LSE_VALUE;
 448:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 449:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 450:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 451:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART4_CLKSOURCE_PCLK1:  /* UART4 Clock is PCLK1 */
 452:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 454:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 455:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 456:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (UARTxSource == LL_RCC_UART5_CLKSOURCE)
 458:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 459:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* UART5CLK clock frequency */
 460:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUARTClockSource(UARTxSource))
ARM GAS  /tmp/cc42qbQx.s 			page 86


 461:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 462:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART5_CLKSOURCE_SYSCLK: /* UART5 Clock is System Clock */
 463:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetSystemClockFreq();
 464:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 466:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART5_CLKSOURCE_HSI:    /* UART5 Clock is HSI Osc. */
 467:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 468:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = HSI_VALUE;
 470:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 471:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 472:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 473:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART5_CLKSOURCE_LSE:    /* UART5 Clock is LSE Osc. */
 474:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 475:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 476:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = LSE_VALUE;
 477:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 478:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 479:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 480:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART5_CLKSOURCE_PCLK1:  /* UART5 Clock is PCLK1 */
 481:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 483:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 484:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 485:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 486:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (UARTxSource == LL_RCC_UART7_CLKSOURCE)
 487:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 488:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* UART7CLK clock frequency */
 489:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetUARTClockSource(UARTxSource))
 490:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 491:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART7_CLKSOURCE_SYSCLK: /* UART7 Clock is System Clock */
 492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetSystemClockFreq();
 493:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 494:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART7_CLKSOURCE_HSI:    /* UART7 Clock is HSI Osc. */
 496:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 497:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = HSI_VALUE;
 499:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 500:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 501:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 502:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART7_CLKSOURCE_LSE:    /* UART7 Clock is LSE Osc. */
 503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 505:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = LSE_VALUE;
 506:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 507:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 508:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 509:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_UART7_CLKSOURCE_PCLK1:  /* UART7 Clock is PCLK1 */
 510:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         uart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 512:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 513:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 514:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 515:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 516:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 517:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     if (UARTxSource == LL_RCC_UART8_CLKSOURCE)
ARM GAS  /tmp/cc42qbQx.s 			page 87


 518:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 519:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       /* UART8CLK clock frequency */
 520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       switch (LL_RCC_GetUARTClockSource(UARTxSource))
 521:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 522:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_UART8_CLKSOURCE_SYSCLK: /* UART8 Clock is System Clock */
 523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = RCC_GetSystemClockFreq();
 524:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 525:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 526:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_UART8_CLKSOURCE_HSI:    /* UART8 Clock is HSI Osc. */
 527:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           if (LL_RCC_HSI_IsReady())
 528:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 529:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             uart_frequency = HSI_VALUE;
 530:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 531:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 532:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 533:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_UART8_CLKSOURCE_LSE:    /* UART8 Clock is LSE Osc. */
 534:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           if (LL_RCC_LSE_IsReady())
 535:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 536:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             uart_frequency = LSE_VALUE;
 537:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 538:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 539:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 540:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_UART8_CLKSOURCE_PCLK1:  /* UART8 Clock is PCLK1 */
 541:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         default:
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           uart_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 543:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 544:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 545:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 546:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 547:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return uart_frequency;
 548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 549:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 550:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 551:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return I2Cx clock frequency
 552:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  I2CxSource This parameter can be one of the following values:
 553:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE
 554:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE
 555:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE
 556:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE (*)
 557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *
 558:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         (*) value not defined in all devices.
 559:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval I2C clock frequency (in Hz)
 560:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that HSI oscillator is not ready
 561:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 562:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetI2CClockFreq(uint32_t I2CxSource)
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 564:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2c_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 565:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 566:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 567:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_I2C_CLKSOURCE(I2CxSource));
 568:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 569:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (I2CxSource == LL_RCC_I2C1_CLKSOURCE)
 570:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 571:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* I2C1 CLK clock frequency */
 572:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetI2CClockSource(I2CxSource))
 573:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 574:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C1_CLKSOURCE_SYSCLK: /* I2C1 Clock is System Clock */
ARM GAS  /tmp/cc42qbQx.s 			page 88


 575:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetSystemClockFreq();
 576:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 577:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 578:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C1_CLKSOURCE_HSI:    /* I2C1 Clock is HSI Osc. */
 579:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 580:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 581:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2c_frequency = HSI_VALUE;
 582:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 583:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 584:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 585:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C1_CLKSOURCE_PCLK1:  /* I2C1 Clock is PCLK1 */
 586:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 588:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 589:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 590:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 591:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (I2CxSource == LL_RCC_I2C2_CLKSOURCE)
 592:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 593:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* I2C2 CLK clock frequency */
 594:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetI2CClockSource(I2CxSource))
 595:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 596:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C2_CLKSOURCE_SYSCLK: /* I2C2 Clock is System Clock */
 597:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetSystemClockFreq();
 598:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 599:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 600:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C2_CLKSOURCE_HSI:    /* I2C2 Clock is HSI Osc. */
 601:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 602:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 603:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2c_frequency = HSI_VALUE;
 604:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 605:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 606:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 607:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C2_CLKSOURCE_PCLK1:  /* I2C2 Clock is PCLK1 */
 608:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 610:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 611:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 612:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 613:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else if (I2CxSource == LL_RCC_I2C3_CLKSOURCE)
 614:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 615:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* I2C3 CLK clock frequency */
 616:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetI2CClockSource(I2CxSource))
 617:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 618:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C3_CLKSOURCE_SYSCLK: /* I2C3 Clock is System Clock */
 619:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetSystemClockFreq();
 620:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 621:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 622:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C3_CLKSOURCE_HSI:    /* I2C3 Clock is HSI Osc. */
 623:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 624:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 625:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2c_frequency = HSI_VALUE;
 626:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 627:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 628:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 629:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2C3_CLKSOURCE_PCLK1:  /* I2C3 Clock is PCLK1 */
 630:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2c_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
ARM GAS  /tmp/cc42qbQx.s 			page 89


 632:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 633:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 634:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 635:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(I2C4)
 636:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 637:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 638:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     if (I2CxSource == LL_RCC_I2C4_CLKSOURCE)
 639:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 640:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       /* I2C4 CLK clock frequency */
 641:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       switch (LL_RCC_GetI2CClockSource(I2CxSource))
 642:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 643:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_I2C4_CLKSOURCE_SYSCLK: /* I2C4 Clock is System Clock */
 644:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2c_frequency = RCC_GetSystemClockFreq();
 645:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 646:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 647:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_I2C4_CLKSOURCE_HSI:    /* I2C4 Clock is HSI Osc. */
 648:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           if (LL_RCC_HSI_IsReady())
 649:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 650:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             i2c_frequency = HSI_VALUE;
 651:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 652:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 653:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 654:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_I2C4_CLKSOURCE_PCLK1:  /* I2C4 Clock is PCLK1 */
 655:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         default:
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2c_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 657:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 658:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 659:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 660:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 661:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #else
 662:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 663:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 664:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* Nothing to do */
 665:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 666:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* I2C4 */
 667:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 668:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return i2c_frequency;
 669:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 670:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 671:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 672:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return I2Sx clock frequency
 673:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  I2SxSource This parameter can be one of the following values:
 674:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE
 675:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval I2S clock frequency (in Hz)
 676:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that PLLI2S oscillator is not ready
 677:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 678:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetI2SClockFreq(uint32_t I2SxSource)
 679:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 680:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2s_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 681:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 682:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 683:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_I2S_CLKSOURCE(I2SxSource));
 684:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 685:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (I2SxSource == LL_RCC_I2S1_CLKSOURCE)
 686:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 687:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* I2S1 CLK clock frequency */
 688:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetI2SClockSource(I2SxSource))
ARM GAS  /tmp/cc42qbQx.s 			page 90


 689:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 690:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2S1_CLKSOURCE_PLLI2S:       /* I2S1 Clock is PLLI2S */
 691:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_PLLI2S_IsReady())
 692:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 693:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           i2s_frequency = RCC_PLLI2S_GetFreqDomain_I2S();
 694:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 695:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 696:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 697:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_I2S1_CLKSOURCE_PIN:          /* I2S1 Clock is External clock */
 698:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         i2s_frequency = EXTERNAL_CLOCK_VALUE;
 700:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 701:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 702:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 703:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 704:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return i2s_frequency;
 705:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 706:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 707:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 708:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return LPTIMx clock frequency
 709:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  LPTIMxSource This parameter can be one of the following values:
 710:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE
 711:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval LPTIM clock frequency (in Hz)
 712:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator (HSI, LSI or LSE) is not r
 713:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 714:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetLPTIMClockFreq(uint32_t LPTIMxSource)
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 716:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t lptim_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 717:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 718:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 719:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_LPTIM_CLKSOURCE(LPTIMxSource));
 720:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 721:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (LPTIMxSource == LL_RCC_LPTIM1_CLKSOURCE)
 722:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 723:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* LPTIM1CLK clock frequency */
 724:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetLPTIMClockSource(LPTIMxSource))
 725:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 726:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_LPTIM1_CLKSOURCE_LSI:    /* LPTIM1 Clock is LSI Osc. */
 727:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSI_IsReady())
 728:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           lptim_frequency = LSI_VALUE;
 730:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 731:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 732:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 733:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_LPTIM1_CLKSOURCE_HSI:    /* LPTIM1 Clock is HSI Osc. */
 734:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_HSI_IsReady())
 735:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 736:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           lptim_frequency = HSI_VALUE;
 737:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 738:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 739:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 740:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_LPTIM1_CLKSOURCE_LSE:    /* LPTIM1 Clock is LSE Osc. */
 741:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_LSE_IsReady())
 742:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 743:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           lptim_frequency = LSE_VALUE;
 744:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 745:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
ARM GAS  /tmp/cc42qbQx.s 			page 91


 746:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 747:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_LPTIM1_CLKSOURCE_PCLK1:  /* LPTIM1 Clock is PCLK1 */
 748:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 749:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         lptim_frequency = RCC_GetPCLK1ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
 750:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 751:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 752:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 753:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 754:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return lptim_frequency;
 755:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 756:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 757:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 758:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return SAIx clock frequency
 759:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  SAIxSource This parameter can be one of the following values:
 760:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE
 761:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE
 762:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval SAI clock frequency (in Hz)
 763:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that PLL is not ready
 764:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 765:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetSAIClockFreq(uint32_t SAIxSource)
 766:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 767:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sai_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 768:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 769:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 770:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_SAI_CLKSOURCE(SAIxSource));
 771:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 772:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (SAIxSource == LL_RCC_SAI1_CLKSOURCE)
 773:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 774:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* SAI1CLK clock frequency */
 775:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetSAIClockSource(SAIxSource))
 776:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 777:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI1_CLKSOURCE_PLLSAI:    /* PLLSAI clock used as SAI1 clock source */
 778:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_PLLSAI_IsReady())
 779:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 780:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           sai_frequency = RCC_PLLSAI_GetFreqDomain_SAI();
 781:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 782:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 783:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 784:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI1_CLKSOURCE_PLLI2S:    /* PLLI2S clock used as SAI1 clock source */
 785:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_PLLI2S_IsReady())
 786:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 787:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           sai_frequency = RCC_PLLI2S_GetFreqDomain_SAI();
 788:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 789:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 790:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 791:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(RCC_SAI1SEL_PLLSRC_SUPPORT)
 792:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI1_CLKSOURCE_PLLSRC:
 793:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         switch (LL_RCC_PLL_GetMainSource())
 794:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 795:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_PLLSOURCE_HSE:       /* HSE clock used as SAI1 clock source */
 796:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_HSE_IsReady())
 797:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 798:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sai_frequency = HSE_VALUE;
 799:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 800:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              break;
 801:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 802:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_PLLSOURCE_HSI:       /* HSI clock used as SAI1 clock source */
ARM GAS  /tmp/cc42qbQx.s 			page 92


 803:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            default:
 804:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_HSI_IsReady())
 805:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 806:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sai_frequency = HSI_VALUE;
 807:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 808:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              break;
 809:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 810:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 811:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* RCC_SAI1SEL_PLLSRC_SUPPORT */
 812:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI1_CLKSOURCE_PIN:        /* External input clock used as SAI1 clock source */
 813:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         sai_frequency = EXTERNAL_SAI1_CLOCK_VALUE;
 814:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 815:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 816:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 817:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 818:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 819:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 820:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 821:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 822:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     if (SAIxSource == LL_RCC_SAI2_CLKSOURCE)
 823:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 824:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       /* SAI2CLK clock frequency */
 825:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       switch (LL_RCC_GetSAIClockSource(SAIxSource))
 826:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 827:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI2_CLKSOURCE_PLLSAI:    /* PLLSAI clock used as SAI2 clock source */
 828:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_PLLSAI_IsReady())
 829:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 830:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           sai_frequency = RCC_PLLSAI_GetFreqDomain_SAI();
 831:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 832:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 833:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 834:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI2_CLKSOURCE_PLLI2S:    /* PLLI2S clock used as SAI2 clock source */
 835:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         if (LL_RCC_PLLI2S_IsReady())
 836:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 837:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           sai_frequency = RCC_PLLI2S_GetFreqDomain_SAI();
 838:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 839:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 840:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 841:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(RCC_SAI2SEL_PLLSRC_SUPPORT)
 842:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SAI2_CLKSOURCE_PLLSRC:
 843:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         switch (LL_RCC_PLL_GetMainSource())
 844:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 845:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_PLLSOURCE_HSE:       /* HSE clock used as SAI2 clock source */
 846:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_HSE_IsReady())
 847:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 848:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sai_frequency = HSE_VALUE;
 849:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 850:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              break;
 851:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 852:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_PLLSOURCE_HSI:       /* HSI clock used as SAI2 clock source */
 853:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            default:
 854:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_HSI_IsReady())
 855:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 856:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sai_frequency = HSI_VALUE;
 857:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 858:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              break;
 859:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
ARM GAS  /tmp/cc42qbQx.s 			page 93


 860:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 861:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* RCC_SAI2SEL_PLLSRC_SUPPORT */
 862:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         case LL_RCC_SAI2_CLKSOURCE_PIN:      /* External input clock used as SAI2 clock source */
 863:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           sai_frequency = EXTERNAL_SAI2_CLOCK_VALUE;
 864:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 865:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 866:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 867:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 868:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 869:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 870:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 871:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 872:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return sai_frequency;
 873:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 874:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 875:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 876:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return SDMMCx clock frequency
 877:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  SDMMCxSource This parameter can be one of the following values:
 878:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE
 879:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE (*)
 880:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *
 881:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         (*) value not defined in all devices.
 882:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval SDMMC clock frequency (in Hz)
 883:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator PLL is not ready
 884:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 885:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetSDMMCClockFreq(uint32_t SDMMCxSource)
 886:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 887:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sdmmc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 888:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 889:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 890:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_SDMMC_CLKSOURCE(SDMMCxSource));
 891:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 892:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (SDMMCxSource == LL_RCC_SDMMC1_CLKSOURCE)
 893:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 894:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     /* SDMMC1CLK clock frequency */
 895:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     switch (LL_RCC_GetSDMMCClockSource(SDMMCxSource))
 896:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 897:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK:        /* PLL48 clock used as SDMMC1 clock source */
 898:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         switch (LL_RCC_GetCK48MClockSource(LL_RCC_CK48M_CLKSOURCE))
 899:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 900:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           case LL_RCC_CK48M_CLKSOURCE_PLL:         /* PLL clock used as 48Mhz domain clock */
 901:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             if (LL_RCC_PLL_IsReady())
 902:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 903:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****               sdmmc_frequency = RCC_PLL_GetFreqDomain_48M();
 904:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 905:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 906:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 907:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           case LL_RCC_CK48M_CLKSOURCE_PLLSAI:      /* PLLSAI clock used as 48Mhz domain clock */
 908:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           default:
 909:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             if (LL_RCC_PLLSAI_IsReady())
 910:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 911:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****               sdmmc_frequency = RCC_PLLSAI_GetFreqDomain_48M();
 912:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 913:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             break;
 914:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 915:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 916:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
ARM GAS  /tmp/cc42qbQx.s 			page 94


 917:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       case LL_RCC_SDMMC1_CLKSOURCE_SYSCLK:        /* PLL clock used as SDMMC1 clock source */
 918:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       default:
 919:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       sdmmc_frequency = RCC_GetSystemClockFreq();
 920:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 921:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 922:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 923:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SDMMC2)
 924:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   else
 925:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 926:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      /* SDMMC2CLK clock frequency */
 927:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      switch (LL_RCC_GetSDMMCClockSource(SDMMCxSource))
 928:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      {
 929:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        case LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK:        /* PLL48 clock used as SDMMC2 clock source */
 930:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****          switch (LL_RCC_GetCK48MClockSource(LL_RCC_CK48M_CLKSOURCE))
 931:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****          {
 932:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_CK48M_CLKSOURCE_PLL:         /* PLL clock used as 48Mhz domain clock */
 933:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_PLL_IsReady())
 934:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 935:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sdmmc_frequency = RCC_PLL_GetFreqDomain_48M();
 936:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 937:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            break;
 938:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 939:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            case LL_RCC_CK48M_CLKSOURCE_PLLSAI:      /* PLLSAI clock used as 48Mhz domain clock */
 940:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****            default:
 941:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              if (LL_RCC_PLLSAI_IsReady())
 942:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 943:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                sdmmc_frequency = RCC_PLLSAI_GetFreqDomain_48M();
 944:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 945:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              break;
 946:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****          }
 947:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****          break;
 948:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 949:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        case LL_RCC_SDMMC2_CLKSOURCE_SYSCLK:        /* PLL clock used as SDMMC2 clock source */
 950:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        default:
 951:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        sdmmc_frequency = RCC_GetSystemClockFreq();
 952:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        break;
 953:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      }
 954:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 955:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SDMMC2 */
 956:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 957:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return sdmmc_frequency;
 958:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 959:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 960:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 961:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return RNGx clock frequency
 962:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  RNGxSource This parameter can be one of the following values:
 963:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE
 964:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval RNG clock frequency (in Hz)
 965:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator is not ready
 966:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
 967:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetRNGClockFreq(uint32_t RNGxSource)
 968:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 969:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t rng_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 970:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 971:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
 972:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_RNG_CLKSOURCE(RNGxSource));
 973:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
ARM GAS  /tmp/cc42qbQx.s 			page 95


 974:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* RNGCLK clock frequency */
 975:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetRNGClockSource(RNGxSource))
 976:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 977:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_RNG_CLKSOURCE_PLL:           /* PLL clock used as RNG clock source */
 978:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_PLL_IsReady())
 979:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 980:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         rng_frequency = RCC_PLL_GetFreqDomain_48M();
 981:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 982:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 983:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 984:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_RNG_CLKSOURCE_PLLSAI:       /* PLLSAI clock used as RNG clock source */
 985:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
 986:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_PLLSAI_IsReady())
 987:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 988:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         rng_frequency = RCC_PLLSAI_GetFreqDomain_48M();
 989:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 990:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 991:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 992:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 993:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return rng_frequency;
 994:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 995:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 996:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(CEC)
 997:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
 998:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return CEC clock frequency
 999:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  CECxSource This parameter can be one of the following values:
1000:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE
1001:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval CEC clock frequency (in Hz)
1002:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator (HSI or LSE) is not ready
1003:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1004:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetCECClockFreq(uint32_t CECxSource)
1005:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 200              		.loc 1 1005 1 is_stmt 1 view -0
 201              		.cfi_startproc
 202              		@ args = 0, pretend = 0, frame = 0
 203              		@ frame_needed = 0, uses_anonymous_args = 0
 204              		@ link register save eliminated.
1006:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t cec_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 205              		.loc 1 1006 3 view .LVU51
1007:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1008:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1009:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_CEC_CLKSOURCE(CECxSource));
 206              		.loc 1 1009 3 view .LVU52
1010:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1011:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* CECCLK clock frequency */
1012:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetCECClockSource(CECxSource))
 207              		.loc 1 1012 3 view .LVU53
 208              	.LBB246:
 209              	.LBI246:
2847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 210              		.loc 2 2847 26 view .LVU54
 211              	.LBB247:
2849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 212              		.loc 2 2849 3 view .LVU55
2849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 213              		.loc 2 2849 21 is_stmt 0 view .LVU56
 214 0000 0A4B     		ldr	r3, .L15
ARM GAS  /tmp/cc42qbQx.s 			page 96


 215 0002 D3F89030 		ldr	r3, [r3, #144]
 216              	.LVL3:
2849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 217              		.loc 2 2849 21 view .LVU57
 218              	.LBE247:
 219              	.LBE246:
 220              		.loc 1 1012 3 discriminator 1 view .LVU58
 221 0006 1842     		tst	r0, r3
 222 0008 05D1     		bne	.L10
1013:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1014:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_CEC_CLKSOURCE_LSE:           /* CEC Clock is LSE Osc. */
1015:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_LSE_IsReady())
 223              		.loc 1 1015 7 is_stmt 1 view .LVU59
 224              	.LBB248:
 225              	.LBI248:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 226              		.loc 2 2154 26 view .LVU60
 227              	.LBB249:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 228              		.loc 2 2156 3 view .LVU61
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 229              		.loc 2 2156 11 is_stmt 0 view .LVU62
 230 000a 084B     		ldr	r3, .L15
 231 000c 186F     		ldr	r0, [r3, #112]
 232              	.LVL4:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 233              		.loc 2 2156 11 view .LVU63
 234              	.LBE249:
 235              	.LBE248:
 236              		.loc 1 1015 10 discriminator 1 view .LVU64
 237 000e 10F00200 		ands	r0, r0, #2
 238 0012 08D1     		bne	.L14
 239              	.LVL5:
 240              	.L9:
1016:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
1017:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         cec_frequency = LSE_VALUE;
1018:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
1019:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1020:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1021:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_CEC_CLKSOURCE_HSI_DIV488:    /* CEC Clock is HSI Osc. */
1022:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1023:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_HSI_IsReady())
1024:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
1025:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         cec_frequency = HSI_VALUE/488U;
1026:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
1027:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1028:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1029:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1030:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return cec_frequency;
1031:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 241              		.loc 1 1031 1 view .LVU65
 242 0014 7047     		bx	lr
 243              	.LVL6:
 244              	.L10:
1023:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 245              		.loc 1 1023 7 is_stmt 1 view .LVU66
 246              	.LBB250:
ARM GAS  /tmp/cc42qbQx.s 			page 97


 247              	.LBI250:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 248              		.loc 2 2030 26 view .LVU67
 249              	.LBB251:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 250              		.loc 2 2032 3 view .LVU68
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 251              		.loc 2 2032 11 is_stmt 0 view .LVU69
 252 0016 054B     		ldr	r3, .L15
 253 0018 1868     		ldr	r0, [r3]
 254              	.LVL7:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 255              		.loc 2 2032 11 view .LVU70
 256              	.LBE251:
 257              	.LBE250:
1023:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 258              		.loc 1 1023 10 discriminator 1 view .LVU71
 259 001a 10F00200 		ands	r0, r0, #2
 260 001e F9D0     		beq	.L9
1025:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 261              		.loc 1 1025 23 view .LVU72
 262 0020 48F21200 		movw	r0, #32786
 263              	.LVL8:
1030:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 264              		.loc 1 1030 3 is_stmt 1 view .LVU73
1030:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 265              		.loc 1 1030 10 is_stmt 0 view .LVU74
 266 0024 F6E7     		b	.L9
 267              	.LVL9:
 268              	.L14:
1017:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 269              		.loc 1 1017 23 view .LVU75
 270 0026 4FF40040 		mov	r0, #32768
 271 002a 7047     		bx	lr
 272              	.L16:
 273              		.align	2
 274              	.L15:
 275 002c 00380240 		.word	1073887232
 276              		.cfi_endproc
 277              	.LFE305:
 279              		.section	.text.RCC_GetHCLKClockFreq,"ax",%progbits
 280              		.align	1
 281              		.global	RCC_GetHCLKClockFreq
 282              		.syntax unified
 283              		.thumb
 284              		.thumb_func
 286              	RCC_GetHCLKClockFreq:
 287              	.LVL10:
 288              	.LFB312:
1032:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* CEC */
1033:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1034:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1035:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return USBx clock frequency
1036:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  USBxSource This parameter can be one of the following values:
1037:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_USB_CLKSOURCE
1038:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval USB clock frequency (in Hz)
1039:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 98


1040:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetUSBClockFreq(uint32_t USBxSource)
1041:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1042:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usb_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1043:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1044:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1045:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_USB_CLKSOURCE(USBxSource));
1046:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1047:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* USBCLK clock frequency */
1048:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetUSBClockSource(USBxSource))
1049:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1050:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_USB_CLKSOURCE_PLL:           /* PLL clock used as USB clock source */
1051:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_PLL_IsReady())
1052:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
1053:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usb_frequency = RCC_PLL_GetFreqDomain_48M();
1054:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
1055:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1056:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1057:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_USB_CLKSOURCE_PLLSAI:       /* PLLSAI clock used as USB clock source */
1058:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1059:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_PLLSAI_IsReady())
1060:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
1061:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         usb_frequency = RCC_PLLSAI_GetFreqDomain_48M();
1062:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
1063:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1064:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1065:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1066:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return usb_frequency;
1067:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1068:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1069:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DFSDM1_Channel0)
1070:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1071:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return DFSDMx clock frequency
1072:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  DFSDMxSource This parameter can be one of the following values:
1073:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE
1074:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval DFSDM clock frequency (in Hz)
1075:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1076:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetDFSDMClockFreq(uint32_t DFSDMxSource)
1077:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1078:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1079:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1080:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1081:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_DFSDM_CLKSOURCE(DFSDMxSource));
1082:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1083:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* DFSDM1CLK clock frequency */
1084:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetDFSDMClockSource(DFSDMxSource))
1085:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1086:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DFSDM1_CLKSOURCE_SYSCLK:     /* DFSDM1 Clock is SYSCLK */
1087:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       dfsdm_frequency = RCC_GetSystemClockFreq();
1088:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1089:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1090:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DFSDM1_CLKSOURCE_PCLK2:      /* DFSDM1 Clock is PCLK2 */
1091:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1092:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       dfsdm_frequency = RCC_GetPCLK2ClockFreq(RCC_GetHCLKClockFreq(RCC_GetSystemClockFreq()));
1093:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1094:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1095:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1096:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return dfsdm_frequency;
ARM GAS  /tmp/cc42qbQx.s 			page 99


1097:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1098:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1099:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1100:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return DFSDMx Audio clock frequency
1101:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  DFSDMxSource This parameter can be one of the following values:
1102:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE
1103:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval DFSDM clock frequency (in Hz)
1104:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator is not ready
1105:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1106:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetDFSDMAudioClockFreq(uint32_t DFSDMxSource)
1107:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1108:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1109:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1110:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1111:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_DFSDM_AUDIO_CLKSOURCE(DFSDMxSource));
1112:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1113:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* DFSDM1CLK clock frequency */
1114:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetDFSDMAudioClockSource(DFSDMxSource))
1115:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1116:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1:     /* SAI1 clock used as DFSDM1 audio clock */
1117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       dfsdm_frequency = LL_RCC_GetSAIClockFreq(LL_RCC_SAI1_CLKSOURCE);
1118:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1119:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1120:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2:     /* SAI2 clock used as DFSDM1 audio clock */
1121:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       dfsdm_frequency = LL_RCC_GetSAIClockFreq(LL_RCC_SAI2_CLKSOURCE);
1123:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1124:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1125:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1126:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return dfsdm_frequency;
1127:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1128:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DFSDM1_Channel0 */
1129:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1130:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DSI)
1131:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1132:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return DSI clock frequency
1133:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  DSIxSource This parameter can be one of the following values:
1134:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE
1135:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval DSI clock frequency (in Hz)
1136:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator is not ready
1137:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NA indicates that external clock is used
1138:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1139:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetDSIClockFreq(uint32_t DSIxSource)
1140:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1141:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dsi_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1142:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1143:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1144:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_DSI_CLKSOURCE(DSIxSource));
1145:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1146:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* DSICLK clock frequency */
1147:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetDSIClockSource(DSIxSource))
1148:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1149:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DSI_CLKSOURCE_PLL:     /* DSI Clock is PLL Osc. */
1150:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       if (LL_RCC_PLL_IsReady())
1151:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
1152:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         dsi_frequency = RCC_PLL_GetFreqDomain_DSI();
1153:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
ARM GAS  /tmp/cc42qbQx.s 			page 100


1154:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1155:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1156:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_DSI_CLKSOURCE_PHY:    /* DSI Clock is DSI physical clock. */
1157:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1158:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       dsi_frequency = LL_RCC_PERIPH_FREQUENCY_NA;
1159:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1160:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1161:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1162:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return dsi_frequency;
1163:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1164:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DSI */
1165:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1166:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(LTDC)
1167:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1168:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return LTDC clock frequency
1169:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  LTDCxSource This parameter can be one of the following values:
1170:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_LTDC_CLKSOURCE
1171:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval LTDC clock frequency (in Hz)
1172:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator PLLSAI is not ready
1173:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1174:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetLTDCClockFreq(uint32_t LTDCxSource)
1175:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1176:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t ltdc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1177:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1178:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1179:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_LTDC_CLKSOURCE(LTDCxSource));
1180:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1181:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (LL_RCC_PLLSAI_IsReady())
1182:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1183:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      ltdc_frequency = RCC_PLLSAI_GetFreqDomain_LTDC();
1184:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1185:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1186:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return ltdc_frequency;
1187:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1188:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* LTDC */
1189:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1190:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SPDIFRX)
1191:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1192:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return SPDIFRX clock frequency
1193:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  SPDIFRXxSource This parameter can be one of the following values:
1194:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         @arg @ref LL_RCC_SPDIFRX1_CLKSOURCE
1195:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval SPDIFRX clock frequency (in Hz)
1196:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   *         - @ref  LL_RCC_PERIPH_FREQUENCY_NO indicates that oscillator is not ready
1197:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1198:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t LL_RCC_GetSPDIFRXClockFreq(uint32_t SPDIFRXxSource)
1199:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1200:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t spdifrx_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
1201:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1202:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Check parameter */
1203:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   assert_param(IS_LL_RCC_SPDIFRX_CLKSOURCE(SPDIFRXxSource));
1204:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1205:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   if (LL_RCC_PLLI2S_IsReady())
1206:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1207:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      spdifrx_frequency = RCC_PLLI2S_GetFreqDomain_SPDIFRX();
1208:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1209:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1210:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return spdifrx_frequency;
ARM GAS  /tmp/cc42qbQx.s 			page 101


1211:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1212:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SPDIFRX */
1213:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1214:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1215:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @}
1216:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1217:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1218:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1219:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @}
1220:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1221:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1222:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /** @addtogroup RCC_LL_Private_Functions
1223:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @{
1224:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1225:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1226:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1227:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return SYSTEM clock frequency
1228:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval SYSTEM clock frequency (in Hz)
1229:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1230:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetSystemClockFreq(void)
1231:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1232:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t frequency = 0U;
1233:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1234:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Get SYSCLK source -------------------------------------------------------*/
1235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (LL_RCC_GetSysClkSource())
1236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1237:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_SYS_CLKSOURCE_STATUS_HSI:  /* HSI used as system clock  source */
1238:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       frequency = HSI_VALUE;
1239:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1240:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1241:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_SYS_CLKSOURCE_STATUS_HSE:  /* HSE used as system clock  source */
1242:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       frequency = HSE_VALUE;
1243:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1244:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1245:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_SYS_CLKSOURCE_STATUS_PLL:  /* PLL used as system clock  source */
1246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       frequency = RCC_PLL_GetFreqDomain_SYS();
1247:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1249:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       frequency = HSI_VALUE;
1251:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1252:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1253:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1254:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return frequency;
1255:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1256:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1257:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1258:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return HCLK clock frequency
1259:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  SYSCLK_Frequency SYSCLK clock frequency
1260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval HCLK clock frequency (in Hz)
1261:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1262:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetHCLKClockFreq(uint32_t SYSCLK_Frequency)
1263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 289              		.loc 1 1263 1 is_stmt 1 view -0
 290              		.cfi_startproc
 291              		@ args = 0, pretend = 0, frame = 0
 292              		@ frame_needed = 0, uses_anonymous_args = 0
ARM GAS  /tmp/cc42qbQx.s 			page 102


 293              		@ link register save eliminated.
1264:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* HCLK clock frequency */
1265:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_HCLK_FREQ(SYSCLK_Frequency, LL_RCC_GetAHBPrescaler());
 294              		.loc 1 1265 3 view .LVU77
 295              	.LBB252:
 296              	.LBI252:
2298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 297              		.loc 2 2298 26 view .LVU78
 298              	.LBB253:
2300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 299              		.loc 2 2300 3 view .LVU79
2300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 300              		.loc 2 2300 21 is_stmt 0 view .LVU80
 301 0000 034B     		ldr	r3, .L18
 302 0002 9B68     		ldr	r3, [r3, #8]
 303              	.LBE253:
 304              	.LBE252:
 305              		.loc 1 1265 10 discriminator 1 view .LVU81
 306 0004 C3F30313 		ubfx	r3, r3, #4, #4
 307 0008 024A     		ldr	r2, .L18+4
 308 000a D35C     		ldrb	r3, [r2, r3]	@ zero_extendqisi2
1266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 309              		.loc 1 1266 1 view .LVU82
 310 000c D840     		lsrs	r0, r0, r3
 311              	.LVL11:
 312              		.loc 1 1266 1 view .LVU83
 313 000e 7047     		bx	lr
 314              	.L19:
 315              		.align	2
 316              	.L18:
 317 0010 00380240 		.word	1073887232
 318 0014 00000000 		.word	AHBPrescTable
 319              		.cfi_endproc
 320              	.LFE312:
 322              		.section	.text.RCC_GetPCLK1ClockFreq,"ax",%progbits
 323              		.align	1
 324              		.global	RCC_GetPCLK1ClockFreq
 325              		.syntax unified
 326              		.thumb
 327              		.thumb_func
 329              	RCC_GetPCLK1ClockFreq:
 330              	.LVL12:
 331              	.LFB313:
1267:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1268:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PCLK1 clock frequency
1270:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  HCLK_Frequency HCLK clock frequency
1271:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PCLK1 clock frequency (in Hz)
1272:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1273:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetPCLK1ClockFreq(uint32_t HCLK_Frequency)
1274:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 332              		.loc 1 1274 1 is_stmt 1 view -0
 333              		.cfi_startproc
 334              		@ args = 0, pretend = 0, frame = 0
 335              		@ frame_needed = 0, uses_anonymous_args = 0
 336              		@ link register save eliminated.
1275:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PCLK1 clock frequency */
ARM GAS  /tmp/cc42qbQx.s 			page 103


1276:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PCLK1_FREQ(HCLK_Frequency, LL_RCC_GetAPB1Prescaler());
 337              		.loc 1 1276 3 view .LVU85
 338              	.LBB254:
 339              	.LBI254:
2313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 340              		.loc 2 2313 26 view .LVU86
 341              	.LBB255:
2315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 342              		.loc 2 2315 3 view .LVU87
2315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 343              		.loc 2 2315 21 is_stmt 0 view .LVU88
 344 0000 034B     		ldr	r3, .L21
 345 0002 9B68     		ldr	r3, [r3, #8]
 346              	.LBE255:
 347              	.LBE254:
 348              		.loc 1 1276 10 discriminator 1 view .LVU89
 349 0004 C3F38223 		ubfx	r3, r3, #10, #3
 350 0008 024A     		ldr	r2, .L21+4
 351 000a D35C     		ldrb	r3, [r2, r3]	@ zero_extendqisi2
1277:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 352              		.loc 1 1277 1 view .LVU90
 353 000c D840     		lsrs	r0, r0, r3
 354              	.LVL13:
 355              		.loc 1 1277 1 view .LVU91
 356 000e 7047     		bx	lr
 357              	.L22:
 358              		.align	2
 359              	.L21:
 360 0010 00380240 		.word	1073887232
 361 0014 00000000 		.word	APBPrescTable
 362              		.cfi_endproc
 363              	.LFE313:
 365              		.section	.text.RCC_GetPCLK2ClockFreq,"ax",%progbits
 366              		.align	1
 367              		.global	RCC_GetPCLK2ClockFreq
 368              		.syntax unified
 369              		.thumb
 370              		.thumb_func
 372              	RCC_GetPCLK2ClockFreq:
 373              	.LVL14:
 374              	.LFB314:
1278:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1279:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1280:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PCLK2 clock frequency
1281:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @param  HCLK_Frequency HCLK clock frequency
1282:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PCLK2 clock frequency (in Hz)
1283:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1284:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_GetPCLK2ClockFreq(uint32_t HCLK_Frequency)
1285:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 375              		.loc 1 1285 1 is_stmt 1 view -0
 376              		.cfi_startproc
 377              		@ args = 0, pretend = 0, frame = 0
 378              		@ frame_needed = 0, uses_anonymous_args = 0
 379              		@ link register save eliminated.
1286:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PCLK2 clock frequency */
1287:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PCLK2_FREQ(HCLK_Frequency, LL_RCC_GetAPB2Prescaler());
 380              		.loc 1 1287 3 view .LVU93
ARM GAS  /tmp/cc42qbQx.s 			page 104


 381              	.LBB256:
 382              	.LBI256:
2328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 383              		.loc 2 2328 26 view .LVU94
 384              	.LBB257:
2330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 385              		.loc 2 2330 3 view .LVU95
2330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 386              		.loc 2 2330 21 is_stmt 0 view .LVU96
 387 0000 034B     		ldr	r3, .L24
 388 0002 9B68     		ldr	r3, [r3, #8]
 389              	.LBE257:
 390              	.LBE256:
 391              		.loc 1 1287 10 discriminator 1 view .LVU97
 392 0004 C3F34233 		ubfx	r3, r3, #13, #3
 393 0008 024A     		ldr	r2, .L24+4
 394 000a D35C     		ldrb	r3, [r2, r3]	@ zero_extendqisi2
1288:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 395              		.loc 1 1288 1 view .LVU98
 396 000c D840     		lsrs	r0, r0, r3
 397              	.LVL15:
 398              		.loc 1 1288 1 view .LVU99
 399 000e 7047     		bx	lr
 400              	.L25:
 401              		.align	2
 402              	.L24:
 403 0010 00380240 		.word	1073887232
 404 0014 00000000 		.word	APBPrescTable
 405              		.cfi_endproc
 406              	.LFE314:
 408              		.section	.text.RCC_PLL_GetFreqDomain_SYS,"ax",%progbits
 409              		.align	1
 410              		.global	RCC_PLL_GetFreqDomain_SYS
 411              		.syntax unified
 412              		.thumb
 413              		.thumb_func
 415              	RCC_PLL_GetFreqDomain_SYS:
 416              	.LFB315:
1289:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1290:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1291:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLL clock frequency used for system domain
1292:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLL clock frequency (in Hz)
1293:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1294:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_SYS(void)
1295:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 417              		.loc 1 1295 1 is_stmt 1 view -0
 418              		.cfi_startproc
 419              		@ args = 0, pretend = 0, frame = 0
 420              		@ frame_needed = 0, uses_anonymous_args = 0
 421              		@ link register save eliminated.
1296:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 422              		.loc 1 1296 3 view .LVU101
 423              	.LVL16:
1297:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1298:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLL_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLN
1299:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      SYSCLK = PLL_VCO / PLLP
1300:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
ARM GAS  /tmp/cc42qbQx.s 			page 105


1301:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 424              		.loc 1 1301 3 view .LVU102
 425              	.LBB258:
 426              	.LBI258:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 427              		.loc 2 3461 26 view .LVU103
 428              	.LBB259:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 429              		.loc 2 3463 3 view .LVU104
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 430              		.loc 2 3463 21 is_stmt 0 view .LVU105
 431 0000 0D4B     		ldr	r3, .L29
 432 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 433              		.loc 2 3463 10 view .LVU106
 434 0004 03F48003 		and	r3, r3, #4194304
 435              	.LVL17:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 436              		.loc 2 3463 10 view .LVU107
 437              	.LBE259:
 438              	.LBE258:
1302:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1303:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 439              		.loc 1 1303 3 is_stmt 1 view .LVU108
 440 0008 9BB9     		cbnz	r3, .L28
1304:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1305:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLL clock source */
1306:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 441              		.loc 1 1306 20 is_stmt 0 view .LVU109
 442 000a 0C48     		ldr	r0, .L29+4
 443              	.L27:
 444              	.LVL18:
1307:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1308:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1309:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLL clock source */
1310:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1311:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1312:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1313:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1315:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1316:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1317:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLCLK_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 445              		.loc 1 1317 3 is_stmt 1 view .LVU110
 446              	.LBB260:
 447              	.LBI260:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 448              		.loc 2 3601 26 view .LVU111
 449              	.LBB261:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 450              		.loc 2 3603 3 view .LVU112
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 451              		.loc 2 3603 21 is_stmt 0 view .LVU113
 452 000c 0A4B     		ldr	r3, .L29
 453              	.LVL19:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 454              		.loc 2 3603 21 view .LVU114
ARM GAS  /tmp/cc42qbQx.s 			page 106


 455 000e 5A68     		ldr	r2, [r3, #4]
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 456              		.loc 2 3603 10 view .LVU115
 457 0010 02F03F02 		and	r2, r2, #63
 458              	.LBE261:
 459              	.LBE260:
 460              		.loc 1 1317 10 discriminator 1 view .LVU116
 461 0014 B0FBF2F0 		udiv	r0, r0, r2
 462              	.LVL20:
 463              	.LBB262:
 464              	.LBI262:
3471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 465              		.loc 2 3471 26 is_stmt 1 view .LVU117
 466              	.LBB263:
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 467              		.loc 2 3473 3 view .LVU118
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 468              		.loc 2 3473 21 is_stmt 0 view .LVU119
 469 0018 5A68     		ldr	r2, [r3, #4]
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 470              		.loc 2 3473 10 view .LVU120
 471 001a C2F38812 		ubfx	r2, r2, #6, #9
 472              	.LBE263:
 473              	.LBE262:
 474              		.loc 1 1317 10 discriminator 2 view .LVU121
 475 001e 02FB00F0 		mul	r0, r2, r0
 476              	.LBB264:
 477              	.LBI264:
3485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 478              		.loc 2 3485 26 is_stmt 1 view .LVU122
 479              	.LBB265:
3487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 480              		.loc 2 3487 3 view .LVU123
3487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 481              		.loc 2 3487 21 is_stmt 0 view .LVU124
 482 0022 5B68     		ldr	r3, [r3, #4]
 483              	.LBE265:
 484              	.LBE264:
 485              		.loc 1 1317 10 discriminator 3 view .LVU125
 486 0024 C3F30143 		ubfx	r3, r3, #16, #2
 487 0028 0133     		adds	r3, r3, #1
 488 002a 5B00     		lsls	r3, r3, #1
1318:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLL_GetN(), LL_RCC_PLL_GetP());
1319:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 489              		.loc 1 1319 1 view .LVU126
 490 002c B0FBF3F0 		udiv	r0, r0, r3
 491 0030 7047     		bx	lr
 492              	.LVL21:
 493              	.L28:
1310:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 494              		.loc 1 1310 20 view .LVU127
 495 0032 0348     		ldr	r0, .L29+8
 496 0034 EAE7     		b	.L27
 497              	.L30:
 498 0036 00BF     		.align	2
 499              	.L29:
 500 0038 00380240 		.word	1073887232
ARM GAS  /tmp/cc42qbQx.s 			page 107


 501 003c 0024F400 		.word	16000000
 502 0040 40787D01 		.word	25000000
 503              		.cfi_endproc
 504              	.LFE315:
 506              		.section	.text.RCC_GetSystemClockFreq,"ax",%progbits
 507              		.align	1
 508              		.global	RCC_GetSystemClockFreq
 509              		.syntax unified
 510              		.thumb
 511              		.thumb_func
 513              	RCC_GetSystemClockFreq:
 514              	.LFB311:
1231:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t frequency = 0U;
 515              		.loc 1 1231 1 is_stmt 1 view -0
 516              		.cfi_startproc
 517              		@ args = 0, pretend = 0, frame = 0
 518              		@ frame_needed = 0, uses_anonymous_args = 0
 519 0000 08B5     		push	{r3, lr}
 520              	.LCFI2:
 521              		.cfi_def_cfa_offset 8
 522              		.cfi_offset 3, -8
 523              		.cfi_offset 14, -4
1232:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 524              		.loc 1 1232 3 view .LVU129
 525              	.LVL22:
1235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 526              		.loc 1 1235 3 view .LVU130
 527              	.LBB266:
 528              	.LBI266:
2227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 529              		.loc 2 2227 26 view .LVU131
 530              	.LBB267:
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 531              		.loc 2 2229 3 view .LVU132
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 532              		.loc 2 2229 21 is_stmt 0 view .LVU133
 533 0002 074B     		ldr	r3, .L36
 534 0004 9B68     		ldr	r3, [r3, #8]
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 535              		.loc 2 2229 10 view .LVU134
 536 0006 03F00C03 		and	r3, r3, #12
 537              	.LBE267:
 538              	.LBE266:
1235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 539              		.loc 1 1235 3 discriminator 1 view .LVU135
 540 000a 042B     		cmp	r3, #4
 541 000c 04D0     		beq	.L33
 542 000e 082B     		cmp	r3, #8
 543 0010 04D1     		bne	.L34
1246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 544              		.loc 1 1246 7 is_stmt 1 view .LVU136
1246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 545              		.loc 1 1246 19 is_stmt 0 view .LVU137
 546 0012 FFF7FEFF 		bl	RCC_PLL_GetFreqDomain_SYS
 547              	.LVL23:
1247:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 548              		.loc 1 1247 7 is_stmt 1 view .LVU138
ARM GAS  /tmp/cc42qbQx.s 			page 108


 549              	.L31:
1255:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 550              		.loc 1 1255 1 is_stmt 0 view .LVU139
 551 0016 08BD     		pop	{r3, pc}
 552              	.LVL24:
 553              	.L33:
1242:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 554              		.loc 1 1242 17 view .LVU140
 555 0018 0248     		ldr	r0, .L36+4
 556 001a FCE7     		b	.L31
 557              	.L34:
1235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 558              		.loc 1 1235 3 discriminator 1 view .LVU141
 559 001c 0248     		ldr	r0, .L36+8
 560              	.LVL25:
1254:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 561              		.loc 1 1254 3 is_stmt 1 view .LVU142
1254:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 562              		.loc 1 1254 10 is_stmt 0 view .LVU143
 563 001e FAE7     		b	.L31
 564              	.L37:
 565              		.align	2
 566              	.L36:
 567 0020 00380240 		.word	1073887232
 568 0024 40787D01 		.word	25000000
 569 0028 0024F400 		.word	16000000
 570              		.cfi_endproc
 571              	.LFE311:
 573              		.section	.text.LL_RCC_GetSystemClocksFreq,"ax",%progbits
 574              		.align	1
 575              		.global	LL_RCC_GetSystemClocksFreq
 576              		.syntax unified
 577              		.thumb
 578              		.thumb_func
 580              	LL_RCC_GetSystemClocksFreq:
 581              	.LVL26:
 582              	.LFB296:
 258:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Get SYSCLK frequency */
 583              		.loc 1 258 1 is_stmt 1 view -0
 584              		.cfi_startproc
 585              		@ args = 0, pretend = 0, frame = 0
 586              		@ frame_needed = 0, uses_anonymous_args = 0
 258:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* Get SYSCLK frequency */
 587              		.loc 1 258 1 is_stmt 0 view .LVU145
 588 0000 10B5     		push	{r4, lr}
 589              	.LCFI3:
 590              		.cfi_def_cfa_offset 8
 591              		.cfi_offset 4, -8
 592              		.cfi_offset 14, -4
 593 0002 0446     		mov	r4, r0
 260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 594              		.loc 1 260 3 is_stmt 1 view .LVU146
 260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 595              		.loc 1 260 34 is_stmt 0 view .LVU147
 596 0004 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 597              	.LVL27:
 260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
ARM GAS  /tmp/cc42qbQx.s 			page 109


 598              		.loc 1 260 32 discriminator 1 view .LVU148
 599 0008 2060     		str	r0, [r4]
 263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 600              		.loc 1 263 3 is_stmt 1 view .LVU149
 263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 601              		.loc 1 263 34 is_stmt 0 view .LVU150
 602 000a FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 603              	.LVL28:
 263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 604              		.loc 1 263 32 discriminator 1 view .LVU151
 605 000e 6060     		str	r0, [r4, #4]
 266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 606              		.loc 1 266 3 is_stmt 1 view .LVU152
 266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 607              		.loc 1 266 34 is_stmt 0 view .LVU153
 608 0010 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 609              	.LVL29:
 266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 610              		.loc 1 266 32 discriminator 1 view .LVU154
 611 0014 A060     		str	r0, [r4, #8]
 269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 612              		.loc 1 269 3 is_stmt 1 view .LVU155
 269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 613              		.loc 1 269 34 is_stmt 0 view .LVU156
 614 0016 6068     		ldr	r0, [r4, #4]
 615 0018 FFF7FEFF 		bl	RCC_GetPCLK2ClockFreq
 616              	.LVL30:
 269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 617              		.loc 1 269 32 discriminator 1 view .LVU157
 618 001c E060     		str	r0, [r4, #12]
 270:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 619              		.loc 1 270 1 view .LVU158
 620 001e 10BD     		pop	{r4, pc}
 270:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 621              		.loc 1 270 1 view .LVU159
 622              		.cfi_endproc
 623              	.LFE296:
 625              		.section	.text.LL_RCC_GetUSARTClockFreq,"ax",%progbits
 626              		.align	1
 627              		.global	LL_RCC_GetUSARTClockFreq
 628              		.syntax unified
 629              		.thumb
 630              		.thumb_func
 632              	LL_RCC_GetUSARTClockFreq:
 633              	.LVL31:
 634              	.LFB297:
 283:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 635              		.loc 1 283 1 is_stmt 1 view -0
 636              		.cfi_startproc
 637              		@ args = 0, pretend = 0, frame = 0
 638              		@ frame_needed = 0, uses_anonymous_args = 0
 283:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 639              		.loc 1 283 1 is_stmt 0 view .LVU161
 640 0000 08B5     		push	{r3, lr}
 641              	.LCFI4:
 642              		.cfi_def_cfa_offset 8
 643              		.cfi_offset 3, -8
ARM GAS  /tmp/cc42qbQx.s 			page 110


 644              		.cfi_offset 14, -4
 284:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 645              		.loc 1 284 3 is_stmt 1 view .LVU162
 646              	.LVL32:
 287:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 647              		.loc 1 287 3 view .LVU163
 289:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 648              		.loc 1 289 3 view .LVU164
 289:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 649              		.loc 1 289 6 is_stmt 0 view .LVU165
 650 0002 0328     		cmp	r0, #3
 651 0004 08D0     		beq	.L67
 318:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 652              		.loc 1 318 8 is_stmt 1 view .LVU166
 318:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 653              		.loc 1 318 11 is_stmt 0 view .LVU167
 654 0006 0C28     		cmp	r0, #12
 655 0008 2ED0     		beq	.L68
 347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 656              		.loc 1 347 8 is_stmt 1 view .LVU168
 347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 657              		.loc 1 347 11 is_stmt 0 view .LVU169
 658 000a B0F5406F 		cmp	r0, #3072
 659 000e 53D0     		beq	.L69
 378:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 660              		.loc 1 378 5 is_stmt 1 view .LVU170
 378:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 661              		.loc 1 378 8 is_stmt 0 view .LVU171
 662 0010 3028     		cmp	r0, #48
 663 0012 7AD0     		beq	.L70
 284:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 664              		.loc 1 284 12 view .LVU172
 665 0014 0020     		movs	r0, #0
 666              	.LVL33:
 667              	.L40:
 409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 668              		.loc 1 409 1 view .LVU173
 669 0016 08BD     		pop	{r3, pc}
 670              	.LVL34:
 671              	.L67:
 292:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 672              		.loc 1 292 5 is_stmt 1 view .LVU174
 673              	.LBB268:
 674              	.LBI268:
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 675              		.loc 2 2664 26 view .LVU175
 676              	.LBB269:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 677              		.loc 2 2666 3 view .LVU176
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 678              		.loc 2 2666 21 is_stmt 0 view .LVU177
 679 0018 514B     		ldr	r3, .L71
 680 001a D3F89030 		ldr	r3, [r3, #144]
 681 001e 0340     		ands	r3, r3, r0
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 682              		.loc 2 2666 10 view .LVU178
 683 0020 43EA0043 		orr	r3, r3, r0, lsl #16
ARM GAS  /tmp/cc42qbQx.s 			page 111


 684              	.LVL35:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 685              		.loc 2 2666 10 view .LVU179
 686              	.LBE269:
 687              	.LBE268:
 292:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 688              		.loc 1 292 5 discriminator 1 view .LVU180
 689 0024 4F4A     		ldr	r2, .L71+4
 690 0026 9342     		cmp	r3, r2
 691 0028 08D0     		beq	.L42
 692 002a B3F1031F 		cmp	r3, #196611
 693 002e 0CD0     		beq	.L43
 694 0030 013A     		subs	r2, r2, #1
 695 0032 9342     		cmp	r3, r2
 696 0034 11D1     		bne	.L44
 295:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 697              		.loc 1 295 9 is_stmt 1 view .LVU181
 295:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 698              		.loc 1 295 27 is_stmt 0 view .LVU182
 699 0036 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 700              	.LVL36:
 296:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 701              		.loc 1 296 9 is_stmt 1 view .LVU183
 702 003a ECE7     		b	.L40
 703              	.LVL37:
 704              	.L42:
 299:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 705              		.loc 1 299 9 view .LVU184
 706              	.LBB270:
 707              	.LBI270:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 708              		.loc 2 2030 26 view .LVU185
 709              	.LBB271:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 710              		.loc 2 2032 3 view .LVU186
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 711              		.loc 2 2032 11 is_stmt 0 view .LVU187
 712 003c 484B     		ldr	r3, .L71
 713 003e 1868     		ldr	r0, [r3]
 714              	.LVL38:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 715              		.loc 2 2032 11 view .LVU188
 716              	.LBE271:
 717              	.LBE270:
 299:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 718              		.loc 1 299 12 discriminator 1 view .LVU189
 719 0040 10F00200 		ands	r0, r0, #2
 720 0044 E7D0     		beq	.L40
 301:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 721              		.loc 1 301 27 view .LVU190
 722 0046 4848     		ldr	r0, .L71+8
 723 0048 E5E7     		b	.L40
 724              	.LVL39:
 725              	.L43:
 306:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 726              		.loc 1 306 9 is_stmt 1 view .LVU191
 727              	.LBB272:
ARM GAS  /tmp/cc42qbQx.s 			page 112


 728              	.LBI272:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 729              		.loc 2 2154 26 view .LVU192
 730              	.LBB273:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 731              		.loc 2 2156 3 view .LVU193
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 732              		.loc 2 2156 11 is_stmt 0 view .LVU194
 733 004a 454B     		ldr	r3, .L71
 734 004c 186F     		ldr	r0, [r3, #112]
 735              	.LVL40:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 736              		.loc 2 2156 11 view .LVU195
 737              	.LBE273:
 738              	.LBE272:
 306:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 739              		.loc 1 306 12 discriminator 1 view .LVU196
 740 004e 10F00200 		ands	r0, r0, #2
 741 0052 E0D0     		beq	.L40
 308:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 742              		.loc 1 308 27 view .LVU197
 743 0054 4FF40040 		mov	r0, #32768
 744 0058 DDE7     		b	.L40
 745              	.LVL41:
 746              	.L44:
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 747              		.loc 1 314 9 is_stmt 1 view .LVU198
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 748              		.loc 1 314 27 is_stmt 0 view .LVU199
 749 005a FFF7FEFF 		bl	RCC_GetSystemClockFreq
 750              	.LVL42:
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 751              		.loc 1 314 27 discriminator 1 view .LVU200
 752 005e FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 753              	.LVL43:
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 754              		.loc 1 314 27 discriminator 2 view .LVU201
 755 0062 FFF7FEFF 		bl	RCC_GetPCLK2ClockFreq
 756              	.LVL44:
 315:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 757              		.loc 1 315 9 is_stmt 1 view .LVU202
 758 0066 D6E7     		b	.L40
 759              	.LVL45:
 760              	.L68:
 321:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 761              		.loc 1 321 5 view .LVU203
 762              	.LBB274:
 763              	.LBI274:
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 764              		.loc 2 2664 26 view .LVU204
 765              	.LBB275:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 766              		.loc 2 2666 3 view .LVU205
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 767              		.loc 2 2666 21 is_stmt 0 view .LVU206
 768 0068 3D4B     		ldr	r3, .L71
 769 006a D3F89030 		ldr	r3, [r3, #144]
ARM GAS  /tmp/cc42qbQx.s 			page 113


 770 006e 0340     		ands	r3, r3, r0
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 771              		.loc 2 2666 10 view .LVU207
 772 0070 43EA0043 		orr	r3, r3, r0, lsl #16
 773              	.LVL46:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 774              		.loc 2 2666 10 view .LVU208
 775              	.LBE275:
 776              	.LBE274:
 321:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 777              		.loc 1 321 5 discriminator 1 view .LVU209
 778 0074 3D4A     		ldr	r2, .L71+12
 779 0076 9342     		cmp	r3, r2
 780 0078 08D0     		beq	.L47
 781 007a B3F10C1F 		cmp	r3, #786444
 782 007e 0CD0     		beq	.L48
 783 0080 043A     		subs	r2, r2, #4
 784 0082 9342     		cmp	r3, r2
 785 0084 11D1     		bne	.L49
 324:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 786              		.loc 1 324 9 is_stmt 1 view .LVU210
 324:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 787              		.loc 1 324 27 is_stmt 0 view .LVU211
 788 0086 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 789              	.LVL47:
 325:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 790              		.loc 1 325 9 is_stmt 1 view .LVU212
 791 008a C4E7     		b	.L40
 792              	.LVL48:
 793              	.L47:
 328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 794              		.loc 1 328 9 view .LVU213
 795              	.LBB276:
 796              	.LBI276:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 797              		.loc 2 2030 26 view .LVU214
 798              	.LBB277:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 799              		.loc 2 2032 3 view .LVU215
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 800              		.loc 2 2032 11 is_stmt 0 view .LVU216
 801 008c 344B     		ldr	r3, .L71
 802 008e 1868     		ldr	r0, [r3]
 803              	.LVL49:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 804              		.loc 2 2032 11 view .LVU217
 805              	.LBE277:
 806              	.LBE276:
 328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 807              		.loc 1 328 12 discriminator 1 view .LVU218
 808 0090 10F00200 		ands	r0, r0, #2
 809 0094 BFD0     		beq	.L40
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 810              		.loc 1 330 27 view .LVU219
 811 0096 3448     		ldr	r0, .L71+8
 812 0098 BDE7     		b	.L40
 813              	.LVL50:
ARM GAS  /tmp/cc42qbQx.s 			page 114


 814              	.L48:
 335:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 815              		.loc 1 335 9 is_stmt 1 view .LVU220
 816              	.LBB278:
 817              	.LBI278:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 818              		.loc 2 2154 26 view .LVU221
 819              	.LBB279:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 820              		.loc 2 2156 3 view .LVU222
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 821              		.loc 2 2156 11 is_stmt 0 view .LVU223
 822 009a 314B     		ldr	r3, .L71
 823 009c 186F     		ldr	r0, [r3, #112]
 824              	.LVL51:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 825              		.loc 2 2156 11 view .LVU224
 826              	.LBE279:
 827              	.LBE278:
 335:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 828              		.loc 1 335 12 discriminator 1 view .LVU225
 829 009e 10F00200 		ands	r0, r0, #2
 830 00a2 B8D0     		beq	.L40
 337:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 831              		.loc 1 337 27 view .LVU226
 832 00a4 4FF40040 		mov	r0, #32768
 833 00a8 B5E7     		b	.L40
 834              	.LVL52:
 835              	.L49:
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 836              		.loc 1 343 9 is_stmt 1 view .LVU227
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 837              		.loc 1 343 27 is_stmt 0 view .LVU228
 838 00aa FFF7FEFF 		bl	RCC_GetSystemClockFreq
 839              	.LVL53:
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 840              		.loc 1 343 27 discriminator 1 view .LVU229
 841 00ae FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 842              	.LVL54:
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 843              		.loc 1 343 27 discriminator 2 view .LVU230
 844 00b2 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 845              	.LVL55:
 344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 846              		.loc 1 344 9 is_stmt 1 view .LVU231
 847 00b6 AEE7     		b	.L40
 848              	.LVL56:
 849              	.L69:
 350:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 850              		.loc 1 350 5 view .LVU232
 851              	.LBB280:
 852              	.LBI280:
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 853              		.loc 2 2664 26 view .LVU233
 854              	.LBB281:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 855              		.loc 2 2666 3 view .LVU234
ARM GAS  /tmp/cc42qbQx.s 			page 115


2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 856              		.loc 2 2666 21 is_stmt 0 view .LVU235
 857 00b8 294B     		ldr	r3, .L71
 858 00ba D3F89030 		ldr	r3, [r3, #144]
 859 00be 0340     		ands	r3, r3, r0
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 860              		.loc 2 2666 10 view .LVU236
 861 00c0 43EA0043 		orr	r3, r3, r0, lsl #16
 862              	.LVL57:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 863              		.loc 2 2666 10 view .LVU237
 864              	.LBE281:
 865              	.LBE280:
 350:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 866              		.loc 1 350 5 discriminator 1 view .LVU238
 867 00c4 2A4A     		ldr	r2, .L71+16
 868 00c6 9342     		cmp	r3, r2
 869 00c8 09D0     		beq	.L51
 870 00ca B3F10C2F 		cmp	r3, #201329664
 871 00ce 0DD0     		beq	.L52
 872 00d0 A2F58062 		sub	r2, r2, #1024
 873 00d4 9342     		cmp	r3, r2
 874 00d6 11D1     		bne	.L53
 353:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 875              		.loc 1 353 9 is_stmt 1 view .LVU239
 353:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 876              		.loc 1 353 27 is_stmt 0 view .LVU240
 877 00d8 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 878              	.LVL58:
 354:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 879              		.loc 1 354 9 is_stmt 1 view .LVU241
 880 00dc 9BE7     		b	.L40
 881              	.LVL59:
 882              	.L51:
 357:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 883              		.loc 1 357 9 view .LVU242
 884              	.LBB282:
 885              	.LBI282:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 886              		.loc 2 2030 26 view .LVU243
 887              	.LBB283:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 888              		.loc 2 2032 3 view .LVU244
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 889              		.loc 2 2032 11 is_stmt 0 view .LVU245
 890 00de 204B     		ldr	r3, .L71
 891 00e0 1868     		ldr	r0, [r3]
 892              	.LVL60:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 893              		.loc 2 2032 11 view .LVU246
 894              	.LBE283:
 895              	.LBE282:
 357:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 896              		.loc 1 357 12 discriminator 1 view .LVU247
 897 00e2 10F00200 		ands	r0, r0, #2
 898 00e6 96D0     		beq	.L40
 359:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
ARM GAS  /tmp/cc42qbQx.s 			page 116


 899              		.loc 1 359 27 view .LVU248
 900 00e8 1F48     		ldr	r0, .L71+8
 901 00ea 94E7     		b	.L40
 902              	.LVL61:
 903              	.L52:
 364:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 904              		.loc 1 364 9 is_stmt 1 view .LVU249
 905              	.LBB284:
 906              	.LBI284:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 907              		.loc 2 2154 26 view .LVU250
 908              	.LBB285:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 909              		.loc 2 2156 3 view .LVU251
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 910              		.loc 2 2156 11 is_stmt 0 view .LVU252
 911 00ec 1C4B     		ldr	r3, .L71
 912 00ee 186F     		ldr	r0, [r3, #112]
 913              	.LVL62:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 914              		.loc 2 2156 11 view .LVU253
 915              	.LBE285:
 916              	.LBE284:
 364:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 917              		.loc 1 364 12 discriminator 1 view .LVU254
 918 00f0 10F00200 		ands	r0, r0, #2
 919 00f4 8FD0     		beq	.L40
 366:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 920              		.loc 1 366 27 view .LVU255
 921 00f6 4FF40040 		mov	r0, #32768
 922 00fa 8CE7     		b	.L40
 923              	.LVL63:
 924              	.L53:
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 925              		.loc 1 372 9 is_stmt 1 view .LVU256
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 926              		.loc 1 372 27 is_stmt 0 view .LVU257
 927 00fc FFF7FEFF 		bl	RCC_GetSystemClockFreq
 928              	.LVL64:
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 929              		.loc 1 372 27 discriminator 1 view .LVU258
 930 0100 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 931              	.LVL65:
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 932              		.loc 1 372 27 discriminator 2 view .LVU259
 933 0104 FFF7FEFF 		bl	RCC_GetPCLK2ClockFreq
 934              	.LVL66:
 373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 935              		.loc 1 373 9 is_stmt 1 view .LVU260
 936 0108 85E7     		b	.L40
 937              	.LVL67:
 938              	.L70:
 381:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 939              		.loc 1 381 7 view .LVU261
 940              	.LBB286:
 941              	.LBI286:
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
ARM GAS  /tmp/cc42qbQx.s 			page 117


 942              		.loc 2 2664 26 view .LVU262
 943              	.LBB287:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 944              		.loc 2 2666 3 view .LVU263
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 945              		.loc 2 2666 21 is_stmt 0 view .LVU264
 946 010a 154B     		ldr	r3, .L71
 947 010c D3F89030 		ldr	r3, [r3, #144]
 948 0110 0340     		ands	r3, r3, r0
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 949              		.loc 2 2666 10 view .LVU265
 950 0112 43EA0043 		orr	r3, r3, r0, lsl #16
 951              	.LVL68:
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 952              		.loc 2 2666 10 view .LVU266
 953              	.LBE287:
 954              	.LBE286:
 381:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 955              		.loc 1 381 7 discriminator 1 view .LVU267
 956 0116 174A     		ldr	r2, .L71+20
 957 0118 9342     		cmp	r3, r2
 958 011a 08D0     		beq	.L54
 959 011c B3F1301F 		cmp	r3, #3145776
 960 0120 0DD0     		beq	.L55
 961 0122 103A     		subs	r2, r2, #16
 962 0124 9342     		cmp	r3, r2
 963 0126 13D1     		bne	.L56
 384:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 964              		.loc 1 384 11 is_stmt 1 view .LVU268
 384:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 965              		.loc 1 384 29 is_stmt 0 view .LVU269
 966 0128 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 967              	.LVL69:
 385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 968              		.loc 1 385 11 is_stmt 1 view .LVU270
 969 012c 73E7     		b	.L40
 970              	.LVL70:
 971              	.L54:
 388:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 972              		.loc 1 388 11 view .LVU271
 973              	.LBB288:
 974              	.LBI288:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 975              		.loc 2 2030 26 view .LVU272
 976              	.LBB289:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 977              		.loc 2 2032 3 view .LVU273
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 978              		.loc 2 2032 11 is_stmt 0 view .LVU274
 979 012e 0C4B     		ldr	r3, .L71
 980 0130 1868     		ldr	r0, [r3]
 981              	.LVL71:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 982              		.loc 2 2032 11 view .LVU275
 983              	.LBE289:
 984              	.LBE288:
 388:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
ARM GAS  /tmp/cc42qbQx.s 			page 118


 985              		.loc 1 388 14 discriminator 1 view .LVU276
 986 0132 10F00200 		ands	r0, r0, #2
 987 0136 3FF46EAF 		beq	.L40
 390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 988              		.loc 1 390 29 view .LVU277
 989 013a 0B48     		ldr	r0, .L71+8
 990 013c 6BE7     		b	.L40
 991              	.LVL72:
 992              	.L55:
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 993              		.loc 1 395 11 is_stmt 1 view .LVU278
 994              	.LBB290:
 995              	.LBI290:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 996              		.loc 2 2154 26 view .LVU279
 997              	.LBB291:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 998              		.loc 2 2156 3 view .LVU280
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 999              		.loc 2 2156 11 is_stmt 0 view .LVU281
 1000 013e 084B     		ldr	r3, .L71
 1001 0140 186F     		ldr	r0, [r3, #112]
 1002              	.LVL73:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1003              		.loc 2 2156 11 view .LVU282
 1004              	.LBE291:
 1005              	.LBE290:
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1006              		.loc 1 395 14 discriminator 1 view .LVU283
 1007 0142 10F00200 		ands	r0, r0, #2
 1008 0146 3FF466AF 		beq	.L40
 397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 1009              		.loc 1 397 29 view .LVU284
 1010 014a 4FF40040 		mov	r0, #32768
 1011              	.LVL74:
 408:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1012              		.loc 1 408 3 is_stmt 1 view .LVU285
 408:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1013              		.loc 1 408 10 is_stmt 0 view .LVU286
 1014 014e 62E7     		b	.L40
 1015              	.LVL75:
 1016              	.L56:
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1017              		.loc 1 403 11 is_stmt 1 view .LVU287
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1018              		.loc 1 403 29 is_stmt 0 view .LVU288
 1019 0150 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1020              	.LVL76:
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1021              		.loc 1 403 29 discriminator 1 view .LVU289
 1022 0154 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1023              	.LVL77:
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1024              		.loc 1 403 29 discriminator 2 view .LVU290
 1025 0158 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1026              	.LVL78:
 404:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
ARM GAS  /tmp/cc42qbQx.s 			page 119


 1027              		.loc 1 404 11 is_stmt 1 view .LVU291
 1028 015c 5BE7     		b	.L40
 1029              	.L72:
 1030 015e 00BF     		.align	2
 1031              	.L71:
 1032 0160 00380240 		.word	1073887232
 1033 0164 02000300 		.word	196610
 1034 0168 0024F400 		.word	16000000
 1035 016c 08000C00 		.word	786440
 1036 0170 0008000C 		.word	201328640
 1037 0174 20003000 		.word	3145760
 1038              		.cfi_endproc
 1039              	.LFE297:
 1041              		.section	.text.LL_RCC_GetUARTClockFreq,"ax",%progbits
 1042              		.align	1
 1043              		.global	LL_RCC_GetUARTClockFreq
 1044              		.syntax unified
 1045              		.thumb
 1046              		.thumb_func
 1048              	LL_RCC_GetUARTClockFreq:
 1049              	.LVL79:
 1050              	.LFB298:
 422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t uart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1051              		.loc 1 422 1 view -0
 1052              		.cfi_startproc
 1053              		@ args = 0, pretend = 0, frame = 0
 1054              		@ frame_needed = 0, uses_anonymous_args = 0
 422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t uart_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1055              		.loc 1 422 1 is_stmt 0 view .LVU293
 1056 0000 08B5     		push	{r3, lr}
 1057              	.LCFI5:
 1058              		.cfi_def_cfa_offset 8
 1059              		.cfi_offset 3, -8
 1060              		.cfi_offset 14, -4
 423:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1061              		.loc 1 423 3 is_stmt 1 view .LVU294
 1062              	.LVL80:
 426:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1063              		.loc 1 426 3 view .LVU295
 428:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1064              		.loc 1 428 3 view .LVU296
 428:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1065              		.loc 1 428 6 is_stmt 0 view .LVU297
 1066 0002 C028     		cmp	r0, #192
 1067 0004 0AD0     		beq	.L100
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1068              		.loc 1 457 8 is_stmt 1 view .LVU298
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1069              		.loc 1 457 11 is_stmt 0 view .LVU299
 1070 0006 B0F5407F 		cmp	r0, #768
 1071 000a 2FD0     		beq	.L101
 486:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1072              		.loc 1 486 8 is_stmt 1 view .LVU300
 486:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1073              		.loc 1 486 11 is_stmt 0 view .LVU301
 1074 000c B0F5405F 		cmp	r0, #12288
 1075 0010 55D0     		beq	.L102
ARM GAS  /tmp/cc42qbQx.s 			page 120


 517:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1076              		.loc 1 517 5 is_stmt 1 view .LVU302
 517:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1077              		.loc 1 517 8 is_stmt 0 view .LVU303
 1078 0012 B0F5404F 		cmp	r0, #49152
 1079 0016 7BD0     		beq	.L103
 423:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1080              		.loc 1 423 12 view .LVU304
 1081 0018 0020     		movs	r0, #0
 1082              	.LVL81:
 1083              	.L73:
 548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1084              		.loc 1 548 1 view .LVU305
 1085 001a 08BD     		pop	{r3, pc}
 1086              	.LVL82:
 1087              	.L100:
 431:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1088              		.loc 1 431 5 is_stmt 1 view .LVU306
 1089              	.LBB292:
 1090              	.LBI292:
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1091              		.loc 2 2698 26 view .LVU307
 1092              	.LBB293:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1093              		.loc 2 2700 3 view .LVU308
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1094              		.loc 2 2700 21 is_stmt 0 view .LVU309
 1095 001c 524B     		ldr	r3, .L104
 1096 001e D3F89030 		ldr	r3, [r3, #144]
 1097 0022 0340     		ands	r3, r3, r0
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1098              		.loc 2 2700 10 view .LVU310
 1099 0024 43EA0043 		orr	r3, r3, r0, lsl #16
 1100              	.LVL83:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1101              		.loc 2 2700 10 view .LVU311
 1102              	.LBE293:
 1103              	.LBE292:
 431:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1104              		.loc 1 431 5 discriminator 1 view .LVU312
 1105 0028 504A     		ldr	r2, .L104+4
 1106 002a 9342     		cmp	r3, r2
 1107 002c 08D0     		beq	.L75
 1108 002e B3F1C01F 		cmp	r3, #12583104
 1109 0032 0CD0     		beq	.L76
 1110 0034 403A     		subs	r2, r2, #64
 1111 0036 9342     		cmp	r3, r2
 1112 0038 11D1     		bne	.L77
 434:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1113              		.loc 1 434 9 is_stmt 1 view .LVU313
 434:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1114              		.loc 1 434 26 is_stmt 0 view .LVU314
 1115 003a FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1116              	.LVL84:
 435:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1117              		.loc 1 435 9 is_stmt 1 view .LVU315
 1118 003e ECE7     		b	.L73
ARM GAS  /tmp/cc42qbQx.s 			page 121


 1119              	.LVL85:
 1120              	.L75:
 438:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1121              		.loc 1 438 9 view .LVU316
 1122              	.LBB294:
 1123              	.LBI294:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1124              		.loc 2 2030 26 view .LVU317
 1125              	.LBB295:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1126              		.loc 2 2032 3 view .LVU318
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1127              		.loc 2 2032 11 is_stmt 0 view .LVU319
 1128 0040 494B     		ldr	r3, .L104
 1129 0042 1868     		ldr	r0, [r3]
 1130              	.LVL86:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1131              		.loc 2 2032 11 view .LVU320
 1132              	.LBE295:
 1133              	.LBE294:
 438:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1134              		.loc 1 438 12 discriminator 1 view .LVU321
 1135 0044 10F00200 		ands	r0, r0, #2
 1136 0048 E7D0     		beq	.L73
 440:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1137              		.loc 1 440 26 view .LVU322
 1138 004a 4948     		ldr	r0, .L104+8
 1139 004c E5E7     		b	.L73
 1140              	.LVL87:
 1141              	.L76:
 445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1142              		.loc 1 445 9 is_stmt 1 view .LVU323
 1143              	.LBB296:
 1144              	.LBI296:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1145              		.loc 2 2154 26 view .LVU324
 1146              	.LBB297:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1147              		.loc 2 2156 3 view .LVU325
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1148              		.loc 2 2156 11 is_stmt 0 view .LVU326
 1149 004e 464B     		ldr	r3, .L104
 1150 0050 186F     		ldr	r0, [r3, #112]
 1151              	.LVL88:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1152              		.loc 2 2156 11 view .LVU327
 1153              	.LBE297:
 1154              	.LBE296:
 445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1155              		.loc 1 445 12 discriminator 1 view .LVU328
 1156 0052 10F00200 		ands	r0, r0, #2
 1157 0056 E0D0     		beq	.L73
 447:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1158              		.loc 1 447 26 view .LVU329
 1159 0058 4FF40040 		mov	r0, #32768
 1160 005c DDE7     		b	.L73
 1161              	.LVL89:
ARM GAS  /tmp/cc42qbQx.s 			page 122


 1162              	.L77:
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1163              		.loc 1 453 9 is_stmt 1 view .LVU330
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1164              		.loc 1 453 26 is_stmt 0 view .LVU331
 1165 005e FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1166              	.LVL90:
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1167              		.loc 1 453 26 discriminator 1 view .LVU332
 1168 0062 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1169              	.LVL91:
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1170              		.loc 1 453 26 discriminator 2 view .LVU333
 1171 0066 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1172              	.LVL92:
 454:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1173              		.loc 1 454 9 is_stmt 1 view .LVU334
 1174 006a D6E7     		b	.L73
 1175              	.LVL93:
 1176              	.L101:
 460:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1177              		.loc 1 460 5 view .LVU335
 1178              	.LBB298:
 1179              	.LBI298:
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1180              		.loc 2 2698 26 view .LVU336
 1181              	.LBB299:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1182              		.loc 2 2700 3 view .LVU337
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1183              		.loc 2 2700 21 is_stmt 0 view .LVU338
 1184 006c 3E4B     		ldr	r3, .L104
 1185 006e D3F89030 		ldr	r3, [r3, #144]
 1186 0072 0340     		ands	r3, r3, r0
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1187              		.loc 2 2700 10 view .LVU339
 1188 0074 43EA0043 		orr	r3, r3, r0, lsl #16
 1189              	.LVL94:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1190              		.loc 2 2700 10 view .LVU340
 1191              	.LBE299:
 1192              	.LBE298:
 460:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1193              		.loc 1 460 5 discriminator 1 view .LVU341
 1194 0078 3E4A     		ldr	r2, .L104+12
 1195 007a 9342     		cmp	r3, r2
 1196 007c 09D0     		beq	.L80
 1197 007e B3F1032F 		cmp	r3, #50332416
 1198 0082 0DD0     		beq	.L81
 1199 0084 A2F58072 		sub	r2, r2, #256
 1200 0088 9342     		cmp	r3, r2
 1201 008a 11D1     		bne	.L82
 463:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1202              		.loc 1 463 9 is_stmt 1 view .LVU342
 463:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1203              		.loc 1 463 26 is_stmt 0 view .LVU343
 1204 008c FFF7FEFF 		bl	RCC_GetSystemClockFreq
ARM GAS  /tmp/cc42qbQx.s 			page 123


 1205              	.LVL95:
 464:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1206              		.loc 1 464 9 is_stmt 1 view .LVU344
 1207 0090 C3E7     		b	.L73
 1208              	.LVL96:
 1209              	.L80:
 467:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1210              		.loc 1 467 9 view .LVU345
 1211              	.LBB300:
 1212              	.LBI300:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1213              		.loc 2 2030 26 view .LVU346
 1214              	.LBB301:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1215              		.loc 2 2032 3 view .LVU347
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1216              		.loc 2 2032 11 is_stmt 0 view .LVU348
 1217 0092 354B     		ldr	r3, .L104
 1218 0094 1868     		ldr	r0, [r3]
 1219              	.LVL97:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1220              		.loc 2 2032 11 view .LVU349
 1221              	.LBE301:
 1222              	.LBE300:
 467:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1223              		.loc 1 467 12 discriminator 1 view .LVU350
 1224 0096 10F00200 		ands	r0, r0, #2
 1225 009a BED0     		beq	.L73
 469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1226              		.loc 1 469 26 view .LVU351
 1227 009c 3448     		ldr	r0, .L104+8
 1228 009e BCE7     		b	.L73
 1229              	.LVL98:
 1230              	.L81:
 474:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1231              		.loc 1 474 9 is_stmt 1 view .LVU352
 1232              	.LBB302:
 1233              	.LBI302:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1234              		.loc 2 2154 26 view .LVU353
 1235              	.LBB303:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1236              		.loc 2 2156 3 view .LVU354
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1237              		.loc 2 2156 11 is_stmt 0 view .LVU355
 1238 00a0 314B     		ldr	r3, .L104
 1239 00a2 186F     		ldr	r0, [r3, #112]
 1240              	.LVL99:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1241              		.loc 2 2156 11 view .LVU356
 1242              	.LBE303:
 1243              	.LBE302:
 474:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1244              		.loc 1 474 12 discriminator 1 view .LVU357
 1245 00a4 10F00200 		ands	r0, r0, #2
 1246 00a8 B7D0     		beq	.L73
 476:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
ARM GAS  /tmp/cc42qbQx.s 			page 124


 1247              		.loc 1 476 26 view .LVU358
 1248 00aa 4FF40040 		mov	r0, #32768
 1249 00ae B4E7     		b	.L73
 1250              	.LVL100:
 1251              	.L82:
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1252              		.loc 1 482 9 is_stmt 1 view .LVU359
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1253              		.loc 1 482 26 is_stmt 0 view .LVU360
 1254 00b0 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1255              	.LVL101:
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1256              		.loc 1 482 26 discriminator 1 view .LVU361
 1257 00b4 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1258              	.LVL102:
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1259              		.loc 1 482 26 discriminator 2 view .LVU362
 1260 00b8 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1261              	.LVL103:
 483:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1262              		.loc 1 483 9 is_stmt 1 view .LVU363
 1263 00bc ADE7     		b	.L73
 1264              	.LVL104:
 1265              	.L102:
 489:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1266              		.loc 1 489 5 view .LVU364
 1267              	.LBB304:
 1268              	.LBI304:
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1269              		.loc 2 2698 26 view .LVU365
 1270              	.LBB305:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1271              		.loc 2 2700 3 view .LVU366
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1272              		.loc 2 2700 21 is_stmt 0 view .LVU367
 1273 00be 2A4B     		ldr	r3, .L104
 1274 00c0 D3F89030 		ldr	r3, [r3, #144]
 1275 00c4 0340     		ands	r3, r3, r0
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1276              		.loc 2 2700 10 view .LVU368
 1277 00c6 43EA0043 		orr	r3, r3, r0, lsl #16
 1278              	.LVL105:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1279              		.loc 2 2700 10 view .LVU369
 1280              	.LBE305:
 1281              	.LBE304:
 489:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1282              		.loc 1 489 5 discriminator 1 view .LVU370
 1283 00ca 2B4A     		ldr	r2, .L104+16
 1284 00cc 9342     		cmp	r3, r2
 1285 00ce 09D0     		beq	.L84
 1286 00d0 B3F1302F 		cmp	r3, #805318656
 1287 00d4 0DD0     		beq	.L85
 1288 00d6 A2F58052 		sub	r2, r2, #4096
 1289 00da 9342     		cmp	r3, r2
 1290 00dc 11D1     		bne	.L86
 492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
ARM GAS  /tmp/cc42qbQx.s 			page 125


 1291              		.loc 1 492 9 is_stmt 1 view .LVU371
 492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1292              		.loc 1 492 26 is_stmt 0 view .LVU372
 1293 00de FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1294              	.LVL106:
 493:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1295              		.loc 1 493 9 is_stmt 1 view .LVU373
 1296 00e2 9AE7     		b	.L73
 1297              	.LVL107:
 1298              	.L84:
 496:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1299              		.loc 1 496 9 view .LVU374
 1300              	.LBB306:
 1301              	.LBI306:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1302              		.loc 2 2030 26 view .LVU375
 1303              	.LBB307:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1304              		.loc 2 2032 3 view .LVU376
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1305              		.loc 2 2032 11 is_stmt 0 view .LVU377
 1306 00e4 204B     		ldr	r3, .L104
 1307 00e6 1868     		ldr	r0, [r3]
 1308              	.LVL108:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1309              		.loc 2 2032 11 view .LVU378
 1310              	.LBE307:
 1311              	.LBE306:
 496:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1312              		.loc 1 496 12 discriminator 1 view .LVU379
 1313 00e8 10F00200 		ands	r0, r0, #2
 1314 00ec 95D0     		beq	.L73
 498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1315              		.loc 1 498 26 view .LVU380
 1316 00ee 2048     		ldr	r0, .L104+8
 1317 00f0 93E7     		b	.L73
 1318              	.LVL109:
 1319              	.L85:
 503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1320              		.loc 1 503 9 is_stmt 1 view .LVU381
 1321              	.LBB308:
 1322              	.LBI308:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1323              		.loc 2 2154 26 view .LVU382
 1324              	.LBB309:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1325              		.loc 2 2156 3 view .LVU383
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1326              		.loc 2 2156 11 is_stmt 0 view .LVU384
 1327 00f2 1D4B     		ldr	r3, .L104
 1328 00f4 186F     		ldr	r0, [r3, #112]
 1329              	.LVL110:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1330              		.loc 2 2156 11 view .LVU385
 1331              	.LBE309:
 1332              	.LBE308:
 503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
ARM GAS  /tmp/cc42qbQx.s 			page 126


 1333              		.loc 1 503 12 discriminator 1 view .LVU386
 1334 00f6 10F00200 		ands	r0, r0, #2
 1335 00fa 8ED0     		beq	.L73
 505:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1336              		.loc 1 505 26 view .LVU387
 1337 00fc 4FF40040 		mov	r0, #32768
 1338 0100 8BE7     		b	.L73
 1339              	.LVL111:
 1340              	.L86:
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1341              		.loc 1 511 9 is_stmt 1 view .LVU388
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1342              		.loc 1 511 26 is_stmt 0 view .LVU389
 1343 0102 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1344              	.LVL112:
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1345              		.loc 1 511 26 discriminator 1 view .LVU390
 1346 0106 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1347              	.LVL113:
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1348              		.loc 1 511 26 discriminator 2 view .LVU391
 1349 010a FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1350              	.LVL114:
 512:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1351              		.loc 1 512 9 is_stmt 1 view .LVU392
 1352 010e 84E7     		b	.L73
 1353              	.LVL115:
 1354              	.L103:
 520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 1355              		.loc 1 520 7 view .LVU393
 1356              	.LBB310:
 1357              	.LBI310:
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1358              		.loc 2 2698 26 view .LVU394
 1359              	.LBB311:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1360              		.loc 2 2700 3 view .LVU395
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1361              		.loc 2 2700 21 is_stmt 0 view .LVU396
 1362 0110 154B     		ldr	r3, .L104
 1363 0112 D3F89030 		ldr	r3, [r3, #144]
 1364 0116 0340     		ands	r3, r3, r0
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1365              		.loc 2 2700 10 view .LVU397
 1366 0118 43EA0043 		orr	r3, r3, r0, lsl #16
 1367              	.LVL116:
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1368              		.loc 2 2700 10 view .LVU398
 1369              	.LBE311:
 1370              	.LBE310:
 520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 1371              		.loc 1 520 7 discriminator 1 view .LVU399
 1372 011c 174A     		ldr	r2, .L104+20
 1373 011e 9342     		cmp	r3, r2
 1374 0120 09D0     		beq	.L87
 1375 0122 B3F1C02F 		cmp	r3, #-1073692672
 1376 0126 0ED0     		beq	.L88
ARM GAS  /tmp/cc42qbQx.s 			page 127


 1377 0128 A2F58042 		sub	r2, r2, #16384
 1378 012c 9342     		cmp	r3, r2
 1379 012e 13D1     		bne	.L89
 523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1380              		.loc 1 523 11 is_stmt 1 view .LVU400
 523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1381              		.loc 1 523 28 is_stmt 0 view .LVU401
 1382 0130 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1383              	.LVL117:
 524:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1384              		.loc 1 524 11 is_stmt 1 view .LVU402
 1385 0134 71E7     		b	.L73
 1386              	.LVL118:
 1387              	.L87:
 527:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1388              		.loc 1 527 11 view .LVU403
 1389              	.LBB312:
 1390              	.LBI312:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1391              		.loc 2 2030 26 view .LVU404
 1392              	.LBB313:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1393              		.loc 2 2032 3 view .LVU405
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1394              		.loc 2 2032 11 is_stmt 0 view .LVU406
 1395 0136 0C4B     		ldr	r3, .L104
 1396 0138 1868     		ldr	r0, [r3]
 1397              	.LVL119:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1398              		.loc 2 2032 11 view .LVU407
 1399              	.LBE313:
 1400              	.LBE312:
 527:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1401              		.loc 1 527 14 discriminator 1 view .LVU408
 1402 013a 10F00200 		ands	r0, r0, #2
 1403 013e 3FF46CAF 		beq	.L73
 529:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 1404              		.loc 1 529 28 view .LVU409
 1405 0142 0B48     		ldr	r0, .L104+8
 1406 0144 69E7     		b	.L73
 1407              	.LVL120:
 1408              	.L88:
 534:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1409              		.loc 1 534 11 is_stmt 1 view .LVU410
 1410              	.LBB314:
 1411              	.LBI314:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1412              		.loc 2 2154 26 view .LVU411
 1413              	.LBB315:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1414              		.loc 2 2156 3 view .LVU412
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1415              		.loc 2 2156 11 is_stmt 0 view .LVU413
 1416 0146 084B     		ldr	r3, .L104
 1417 0148 186F     		ldr	r0, [r3, #112]
 1418              	.LVL121:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/cc42qbQx.s 			page 128


 1419              		.loc 2 2156 11 view .LVU414
 1420              	.LBE315:
 1421              	.LBE314:
 534:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1422              		.loc 1 534 14 discriminator 1 view .LVU415
 1423 014a 10F00200 		ands	r0, r0, #2
 1424 014e 3FF464AF 		beq	.L73
 536:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 1425              		.loc 1 536 28 view .LVU416
 1426 0152 4FF40040 		mov	r0, #32768
 1427              	.LVL122:
 547:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1428              		.loc 1 547 3 is_stmt 1 view .LVU417
 547:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1429              		.loc 1 547 10 is_stmt 0 view .LVU418
 1430 0156 60E7     		b	.L73
 1431              	.LVL123:
 1432              	.L89:
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1433              		.loc 1 542 11 is_stmt 1 view .LVU419
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1434              		.loc 1 542 28 is_stmt 0 view .LVU420
 1435 0158 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1436              	.LVL124:
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1437              		.loc 1 542 28 discriminator 1 view .LVU421
 1438 015c FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1439              	.LVL125:
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1440              		.loc 1 542 28 discriminator 2 view .LVU422
 1441 0160 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1442              	.LVL126:
 543:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 1443              		.loc 1 543 11 is_stmt 1 view .LVU423
 1444 0164 59E7     		b	.L73
 1445              	.L105:
 1446 0166 00BF     		.align	2
 1447              	.L104:
 1448 0168 00380240 		.word	1073887232
 1449 016c 8000C000 		.word	12583040
 1450 0170 0024F400 		.word	16000000
 1451 0174 00020003 		.word	50332160
 1452 0178 00200030 		.word	805314560
 1453 017c 008000C0 		.word	-1073709056
 1454              		.cfi_endproc
 1455              	.LFE298:
 1457              		.section	.text.LL_RCC_GetI2CClockFreq,"ax",%progbits
 1458              		.align	1
 1459              		.global	LL_RCC_GetI2CClockFreq
 1460              		.syntax unified
 1461              		.thumb
 1462              		.thumb_func
 1464              	LL_RCC_GetI2CClockFreq:
 1465              	.LVL127:
 1466              	.LFB299:
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2c_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1467              		.loc 1 563 1 view -0
ARM GAS  /tmp/cc42qbQx.s 			page 129


 1468              		.cfi_startproc
 1469              		@ args = 0, pretend = 0, frame = 0
 1470              		@ frame_needed = 0, uses_anonymous_args = 0
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2c_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1471              		.loc 1 563 1 is_stmt 0 view .LVU425
 1472 0000 08B5     		push	{r3, lr}
 1473              	.LCFI6:
 1474              		.cfi_def_cfa_offset 8
 1475              		.cfi_offset 3, -8
 1476              		.cfi_offset 14, -4
 564:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1477              		.loc 1 564 3 is_stmt 1 view .LVU426
 1478              	.LVL128:
 567:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1479              		.loc 1 567 3 view .LVU427
 569:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1480              		.loc 1 569 3 view .LVU428
 569:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1481              		.loc 1 569 6 is_stmt 0 view .LVU429
 1482 0002 B0F5403F 		cmp	r0, #196608
 1483 0006 0AD0     		beq	.L133
 591:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1484              		.loc 1 591 8 is_stmt 1 view .LVU430
 591:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1485              		.loc 1 591 11 is_stmt 0 view .LVU431
 1486 0008 B0F5402F 		cmp	r0, #786432
 1487 000c 24D0     		beq	.L134
 613:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1488              		.loc 1 613 8 is_stmt 1 view .LVU432
 613:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1489              		.loc 1 613 11 is_stmt 0 view .LVU433
 1490 000e B0F5401F 		cmp	r0, #3145728
 1491 0012 3ED0     		beq	.L135
 638:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1492              		.loc 1 638 5 is_stmt 1 view .LVU434
 638:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1493              		.loc 1 638 8 is_stmt 0 view .LVU435
 1494 0014 B0F5400F 		cmp	r0, #12582912
 1495 0018 58D0     		beq	.L136
 564:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1496              		.loc 1 564 12 view .LVU436
 1497 001a 0020     		movs	r0, #0
 1498              	.LVL129:
 1499              	.L106:
 669:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1500              		.loc 1 669 1 view .LVU437
 1501 001c 08BD     		pop	{r3, pc}
 1502              	.LVL130:
 1503              	.L133:
 572:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1504              		.loc 1 572 5 is_stmt 1 view .LVU438
 1505              	.LBB316:
 1506              	.LBI316:
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1507              		.loc 2 2730 26 view .LVU439
 1508              	.LBB317:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/cc42qbQx.s 			page 130


 1509              		.loc 2 2732 3 view .LVU440
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1510              		.loc 2 2732 22 is_stmt 0 view .LVU441
 1511 001e 3A4B     		ldr	r3, .L137
 1512 0020 D3F89030 		ldr	r3, [r3, #144]
 1513 0024 0340     		ands	r3, r3, r0
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1514              		.loc 2 2732 10 view .LVU442
 1515 0026 40EA1340 		orr	r0, r0, r3, lsr #16
 1516              	.LVL131:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1517              		.loc 2 2732 10 view .LVU443
 1518              	.LBE317:
 1519              	.LBE316:
 572:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1520              		.loc 1 572 5 discriminator 1 view .LVU444
 1521 002a 384B     		ldr	r3, .L137+4
 1522 002c 9842     		cmp	r0, r3
 1523 002e 09D0     		beq	.L108
 1524 0030 0133     		adds	r3, r3, #1
 1525 0032 9842     		cmp	r0, r3
 1526 0034 09D0     		beq	.L109
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1527              		.loc 1 587 9 is_stmt 1 view .LVU445
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1528              		.loc 1 587 25 is_stmt 0 view .LVU446
 1529 0036 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1530              	.LVL132:
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1531              		.loc 1 587 25 discriminator 1 view .LVU447
 1532 003a FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1533              	.LVL133:
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1534              		.loc 1 587 25 discriminator 2 view .LVU448
 1535 003e FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1536              	.LVL134:
 588:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1537              		.loc 1 588 9 is_stmt 1 view .LVU449
 1538 0042 EBE7     		b	.L106
 1539              	.LVL135:
 1540              	.L108:
 575:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1541              		.loc 1 575 9 view .LVU450
 575:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1542              		.loc 1 575 25 is_stmt 0 view .LVU451
 1543 0044 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1544              	.LVL136:
 576:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1545              		.loc 1 576 9 is_stmt 1 view .LVU452
 1546 0048 E8E7     		b	.L106
 1547              	.LVL137:
 1548              	.L109:
 579:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1549              		.loc 1 579 9 view .LVU453
 1550              	.LBB318:
 1551              	.LBI318:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
ARM GAS  /tmp/cc42qbQx.s 			page 131


 1552              		.loc 2 2030 26 view .LVU454
 1553              	.LBB319:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1554              		.loc 2 2032 3 view .LVU455
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1555              		.loc 2 2032 11 is_stmt 0 view .LVU456
 1556 004a 2F4B     		ldr	r3, .L137
 1557 004c 1868     		ldr	r0, [r3]
 1558              	.LBE319:
 1559              	.LBE318:
 579:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1560              		.loc 1 579 12 discriminator 1 view .LVU457
 1561 004e 10F00200 		ands	r0, r0, #2
 1562 0052 E3D0     		beq	.L106
 581:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1563              		.loc 1 581 25 view .LVU458
 1564 0054 2E48     		ldr	r0, .L137+8
 1565 0056 E1E7     		b	.L106
 1566              	.LVL138:
 1567              	.L134:
 594:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1568              		.loc 1 594 5 is_stmt 1 view .LVU459
 1569              	.LBB320:
 1570              	.LBI320:
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1571              		.loc 2 2730 26 view .LVU460
 1572              	.LBB321:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1573              		.loc 2 2732 3 view .LVU461
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1574              		.loc 2 2732 22 is_stmt 0 view .LVU462
 1575 0058 2B4B     		ldr	r3, .L137
 1576 005a D3F89030 		ldr	r3, [r3, #144]
 1577 005e 0340     		ands	r3, r3, r0
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1578              		.loc 2 2732 10 view .LVU463
 1579 0060 40EA1340 		orr	r0, r0, r3, lsr #16
 1580              	.LVL139:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1581              		.loc 2 2732 10 view .LVU464
 1582              	.LBE321:
 1583              	.LBE320:
 594:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1584              		.loc 1 594 5 discriminator 1 view .LVU465
 1585 0064 2B4B     		ldr	r3, .L137+12
 1586 0066 9842     		cmp	r0, r3
 1587 0068 09D0     		beq	.L113
 1588 006a 0433     		adds	r3, r3, #4
 1589 006c 9842     		cmp	r0, r3
 1590 006e 09D0     		beq	.L114
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1591              		.loc 1 609 9 is_stmt 1 view .LVU466
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1592              		.loc 1 609 25 is_stmt 0 view .LVU467
 1593 0070 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1594              	.LVL140:
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
ARM GAS  /tmp/cc42qbQx.s 			page 132


 1595              		.loc 1 609 25 discriminator 1 view .LVU468
 1596 0074 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1597              	.LVL141:
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1598              		.loc 1 609 25 discriminator 2 view .LVU469
 1599 0078 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1600              	.LVL142:
 610:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1601              		.loc 1 610 9 is_stmt 1 view .LVU470
 1602 007c CEE7     		b	.L106
 1603              	.LVL143:
 1604              	.L113:
 597:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1605              		.loc 1 597 9 view .LVU471
 597:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1606              		.loc 1 597 25 is_stmt 0 view .LVU472
 1607 007e FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1608              	.LVL144:
 598:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1609              		.loc 1 598 9 is_stmt 1 view .LVU473
 1610 0082 CBE7     		b	.L106
 1611              	.LVL145:
 1612              	.L114:
 601:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1613              		.loc 1 601 9 view .LVU474
 1614              	.LBB322:
 1615              	.LBI322:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1616              		.loc 2 2030 26 view .LVU475
 1617              	.LBB323:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1618              		.loc 2 2032 3 view .LVU476
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1619              		.loc 2 2032 11 is_stmt 0 view .LVU477
 1620 0084 204B     		ldr	r3, .L137
 1621 0086 1868     		ldr	r0, [r3]
 1622              	.LBE323:
 1623              	.LBE322:
 601:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1624              		.loc 1 601 12 discriminator 1 view .LVU478
 1625 0088 10F00200 		ands	r0, r0, #2
 1626 008c C6D0     		beq	.L106
 603:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1627              		.loc 1 603 25 view .LVU479
 1628 008e 2048     		ldr	r0, .L137+8
 1629 0090 C4E7     		b	.L106
 1630              	.LVL146:
 1631              	.L135:
 616:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1632              		.loc 1 616 5 is_stmt 1 view .LVU480
 1633              	.LBB324:
 1634              	.LBI324:
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1635              		.loc 2 2730 26 view .LVU481
 1636              	.LBB325:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1637              		.loc 2 2732 3 view .LVU482
ARM GAS  /tmp/cc42qbQx.s 			page 133


2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1638              		.loc 2 2732 22 is_stmt 0 view .LVU483
 1639 0092 1D4B     		ldr	r3, .L137
 1640 0094 D3F89030 		ldr	r3, [r3, #144]
 1641 0098 0340     		ands	r3, r3, r0
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1642              		.loc 2 2732 10 view .LVU484
 1643 009a 40EA1340 		orr	r0, r0, r3, lsr #16
 1644              	.LVL147:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1645              		.loc 2 2732 10 view .LVU485
 1646              	.LBE325:
 1647              	.LBE324:
 616:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1648              		.loc 1 616 5 discriminator 1 view .LVU486
 1649 009e 1E4B     		ldr	r3, .L137+16
 1650 00a0 9842     		cmp	r0, r3
 1651 00a2 09D0     		beq	.L117
 1652 00a4 1033     		adds	r3, r3, #16
 1653 00a6 9842     		cmp	r0, r3
 1654 00a8 09D0     		beq	.L118
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1655              		.loc 1 631 9 is_stmt 1 view .LVU487
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1656              		.loc 1 631 25 is_stmt 0 view .LVU488
 1657 00aa FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1658              	.LVL148:
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1659              		.loc 1 631 25 discriminator 1 view .LVU489
 1660 00ae FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1661              	.LVL149:
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1662              		.loc 1 631 25 discriminator 2 view .LVU490
 1663 00b2 FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1664              	.LVL150:
 632:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1665              		.loc 1 632 9 is_stmt 1 view .LVU491
 1666 00b6 B1E7     		b	.L106
 1667              	.LVL151:
 1668              	.L117:
 619:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1669              		.loc 1 619 9 view .LVU492
 619:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1670              		.loc 1 619 25 is_stmt 0 view .LVU493
 1671 00b8 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1672              	.LVL152:
 620:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1673              		.loc 1 620 9 is_stmt 1 view .LVU494
 1674 00bc AEE7     		b	.L106
 1675              	.LVL153:
 1676              	.L118:
 623:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1677              		.loc 1 623 9 view .LVU495
 1678              	.LBB326:
 1679              	.LBI326:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1680              		.loc 2 2030 26 view .LVU496
ARM GAS  /tmp/cc42qbQx.s 			page 134


 1681              	.LBB327:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1682              		.loc 2 2032 3 view .LVU497
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1683              		.loc 2 2032 11 is_stmt 0 view .LVU498
 1684 00be 124B     		ldr	r3, .L137
 1685 00c0 1868     		ldr	r0, [r3]
 1686              	.LBE327:
 1687              	.LBE326:
 623:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1688              		.loc 1 623 12 discriminator 1 view .LVU499
 1689 00c2 10F00200 		ands	r0, r0, #2
 1690 00c6 A9D0     		beq	.L106
 625:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1691              		.loc 1 625 25 view .LVU500
 1692 00c8 1148     		ldr	r0, .L137+8
 1693 00ca A7E7     		b	.L106
 1694              	.LVL154:
 1695              	.L136:
 641:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 1696              		.loc 1 641 7 is_stmt 1 view .LVU501
 1697              	.LBB328:
 1698              	.LBI328:
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1699              		.loc 2 2730 26 view .LVU502
 1700              	.LBB329:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1701              		.loc 2 2732 3 view .LVU503
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1702              		.loc 2 2732 22 is_stmt 0 view .LVU504
 1703 00cc 0E4B     		ldr	r3, .L137
 1704 00ce D3F89030 		ldr	r3, [r3, #144]
 1705 00d2 0340     		ands	r3, r3, r0
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1706              		.loc 2 2732 10 view .LVU505
 1707 00d4 40EA1340 		orr	r0, r0, r3, lsr #16
 1708              	.LVL155:
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1709              		.loc 2 2732 10 view .LVU506
 1710              	.LBE329:
 1711              	.LBE328:
 641:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 1712              		.loc 1 641 7 discriminator 1 view .LVU507
 1713 00d8 104B     		ldr	r3, .L137+20
 1714 00da 9842     		cmp	r0, r3
 1715 00dc 09D0     		beq	.L120
 1716 00de 4033     		adds	r3, r3, #64
 1717 00e0 9842     		cmp	r0, r3
 1718 00e2 09D0     		beq	.L121
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1719              		.loc 1 656 11 is_stmt 1 view .LVU508
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1720              		.loc 1 656 27 is_stmt 0 view .LVU509
 1721 00e4 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1722              	.LVL156:
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1723              		.loc 1 656 27 discriminator 1 view .LVU510
ARM GAS  /tmp/cc42qbQx.s 			page 135


 1724 00e8 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1725              	.LVL157:
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1726              		.loc 1 656 27 discriminator 2 view .LVU511
 1727 00ec FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1728              	.LVL158:
 657:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 1729              		.loc 1 657 11 is_stmt 1 view .LVU512
 1730 00f0 94E7     		b	.L106
 1731              	.LVL159:
 1732              	.L120:
 644:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1733              		.loc 1 644 11 view .LVU513
 644:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 1734              		.loc 1 644 27 is_stmt 0 view .LVU514
 1735 00f2 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1736              	.LVL160:
 645:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1737              		.loc 1 645 11 is_stmt 1 view .LVU515
 1738 00f6 91E7     		b	.L106
 1739              	.LVL161:
 1740              	.L121:
 648:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1741              		.loc 1 648 11 view .LVU516
 1742              	.LBB330:
 1743              	.LBI330:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1744              		.loc 2 2030 26 view .LVU517
 1745              	.LBB331:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1746              		.loc 2 2032 3 view .LVU518
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1747              		.loc 2 2032 11 is_stmt 0 view .LVU519
 1748 00f8 034B     		ldr	r3, .L137
 1749 00fa 1868     		ldr	r0, [r3]
 1750              	.LBE331:
 1751              	.LBE330:
 648:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           {
 1752              		.loc 1 648 14 discriminator 1 view .LVU520
 1753 00fc 10F00200 		ands	r0, r0, #2
 1754 0100 8CD0     		beq	.L106
 650:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           }
 1755              		.loc 1 650 27 view .LVU521
 1756 0102 0348     		ldr	r0, .L137+8
 1757              	.LVL162:
 668:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1758              		.loc 1 668 3 is_stmt 1 view .LVU522
 668:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1759              		.loc 1 668 10 is_stmt 0 view .LVU523
 1760 0104 8AE7     		b	.L106
 1761              	.L138:
 1762 0106 00BF     		.align	2
 1763              	.L137:
 1764 0108 00380240 		.word	1073887232
 1765 010c 01000300 		.word	196609
 1766 0110 0024F400 		.word	16000000
 1767 0114 04000C00 		.word	786436
ARM GAS  /tmp/cc42qbQx.s 			page 136


 1768 0118 10003000 		.word	3145744
 1769 011c 4000C000 		.word	12582976
 1770              		.cfi_endproc
 1771              	.LFE299:
 1773              		.section	.text.LL_RCC_GetLPTIMClockFreq,"ax",%progbits
 1774              		.align	1
 1775              		.global	LL_RCC_GetLPTIMClockFreq
 1776              		.syntax unified
 1777              		.thumb
 1778              		.thumb_func
 1780              	LL_RCC_GetLPTIMClockFreq:
 1781              	.LVL163:
 1782              	.LFB301:
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t lptim_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1783              		.loc 1 715 1 is_stmt 1 view -0
 1784              		.cfi_startproc
 1785              		@ args = 0, pretend = 0, frame = 0
 1786              		@ frame_needed = 0, uses_anonymous_args = 0
 716:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1787              		.loc 1 716 3 view .LVU525
 719:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1788              		.loc 1 719 3 view .LVU526
 721:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1789              		.loc 1 721 3 view .LVU527
 721:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1790              		.loc 1 721 6 is_stmt 0 view .LVU528
 1791 0000 B0F1407F 		cmp	r0, #50331648
 1792 0004 01D0     		beq	.L152
 716:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1793              		.loc 1 716 12 view .LVU529
 1794 0006 0020     		movs	r0, #0
 1795              	.LVL164:
 755:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1796              		.loc 1 755 1 view .LVU530
 1797 0008 7047     		bx	lr
 1798              	.LVL165:
 1799              	.L152:
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t lptim_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1800              		.loc 1 715 1 view .LVU531
 1801 000a 08B5     		push	{r3, lr}
 1802              	.LCFI7:
 1803              		.cfi_def_cfa_offset 8
 1804              		.cfi_offset 3, -8
 1805              		.cfi_offset 14, -4
 724:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1806              		.loc 1 724 5 is_stmt 1 view .LVU532
 1807              	.LVL166:
 1808              	.LBB332:
 1809              	.LBI332:
2746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1810              		.loc 2 2746 26 view .LVU533
 1811              	.LBB333:
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1812              		.loc 2 2748 3 view .LVU534
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1813              		.loc 2 2748 21 is_stmt 0 view .LVU535
 1814 000c 154B     		ldr	r3, .L153
ARM GAS  /tmp/cc42qbQx.s 			page 137


 1815 000e D3F89030 		ldr	r3, [r3, #144]
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1816              		.loc 2 2748 10 view .LVU536
 1817 0012 03F04073 		and	r3, r3, #50331648
 1818              	.LVL167:
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1819              		.loc 2 2748 10 view .LVU537
 1820              	.LBE333:
 1821              	.LBE332:
 724:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 1822              		.loc 1 724 5 discriminator 1 view .LVU538
 1823 0016 B3F1007F 		cmp	r3, #33554432
 1824 001a 0DD0     		beq	.L141
 1825 001c B3F1407F 		cmp	r3, #50331648
 1826 0020 11D0     		beq	.L142
 1827 0022 B3F1807F 		cmp	r3, #16777216
 1828 0026 16D1     		bne	.L143
 727:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1829              		.loc 1 727 9 is_stmt 1 view .LVU539
 1830              	.LBB334:
 1831              	.LBI334:
2192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1832              		.loc 2 2192 26 view .LVU540
 1833              	.LBB335:
2194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1834              		.loc 2 2194 3 view .LVU541
2194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1835              		.loc 2 2194 11 is_stmt 0 view .LVU542
 1836 0028 0E4B     		ldr	r3, .L153
 1837 002a 586F     		ldr	r0, [r3, #116]
 1838              	.LVL168:
2194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1839              		.loc 2 2194 11 view .LVU543
 1840              	.LBE335:
 1841              	.LBE334:
 727:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1842              		.loc 1 727 12 discriminator 1 view .LVU544
 1843 002c 10F00200 		ands	r0, r0, #2
 1844 0030 17D0     		beq	.L139
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1845              		.loc 1 729 27 view .LVU545
 1846 0032 4FF4FA40 		mov	r0, #32000
 1847 0036 14E0     		b	.L139
 1848              	.LVL169:
 1849              	.L141:
 734:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1850              		.loc 1 734 9 is_stmt 1 view .LVU546
 1851              	.LBB336:
 1852              	.LBI336:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1853              		.loc 2 2030 26 view .LVU547
 1854              	.LBB337:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1855              		.loc 2 2032 3 view .LVU548
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1856              		.loc 2 2032 11 is_stmt 0 view .LVU549
 1857 0038 0A4B     		ldr	r3, .L153
ARM GAS  /tmp/cc42qbQx.s 			page 138


 1858 003a 1868     		ldr	r0, [r3]
 1859              	.LVL170:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1860              		.loc 2 2032 11 view .LVU550
 1861              	.LBE337:
 1862              	.LBE336:
 734:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1863              		.loc 1 734 12 discriminator 1 view .LVU551
 1864 003c 10F00200 		ands	r0, r0, #2
 1865 0040 0FD0     		beq	.L139
 736:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1866              		.loc 1 736 27 view .LVU552
 1867 0042 0948     		ldr	r0, .L153+4
 1868 0044 0DE0     		b	.L139
 1869              	.LVL171:
 1870              	.L142:
 741:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1871              		.loc 1 741 9 is_stmt 1 view .LVU553
 1872              	.LBB338:
 1873              	.LBI338:
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1874              		.loc 2 2154 26 view .LVU554
 1875              	.LBB339:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1876              		.loc 2 2156 3 view .LVU555
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1877              		.loc 2 2156 11 is_stmt 0 view .LVU556
 1878 0046 074B     		ldr	r3, .L153
 1879 0048 186F     		ldr	r0, [r3, #112]
 1880              	.LVL172:
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1881              		.loc 2 2156 11 view .LVU557
 1882              	.LBE339:
 1883              	.LBE338:
 741:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 1884              		.loc 1 741 12 discriminator 1 view .LVU558
 1885 004a 10F00200 		ands	r0, r0, #2
 1886 004e 08D0     		beq	.L139
 743:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 1887              		.loc 1 743 27 view .LVU559
 1888 0050 4FF40040 		mov	r0, #32768
 1889              	.LVL173:
 754:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1890              		.loc 1 754 3 is_stmt 1 view .LVU560
 754:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1891              		.loc 1 754 10 is_stmt 0 view .LVU561
 1892 0054 05E0     		b	.L139
 1893              	.LVL174:
 1894              	.L143:
 749:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1895              		.loc 1 749 9 is_stmt 1 view .LVU562
 749:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1896              		.loc 1 749 27 is_stmt 0 view .LVU563
 1897 0056 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1898              	.LVL175:
 749:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1899              		.loc 1 749 27 discriminator 1 view .LVU564
ARM GAS  /tmp/cc42qbQx.s 			page 139


 1900 005a FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1901              	.LVL176:
 749:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 1902              		.loc 1 749 27 discriminator 2 view .LVU565
 1903 005e FFF7FEFF 		bl	RCC_GetPCLK1ClockFreq
 1904              	.LVL177:
 750:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 1905              		.loc 1 750 9 is_stmt 1 view .LVU566
 1906              	.L139:
 755:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1907              		.loc 1 755 1 is_stmt 0 view .LVU567
 1908 0062 08BD     		pop	{r3, pc}
 1909              	.L154:
 1910              		.align	2
 1911              	.L153:
 1912 0064 00380240 		.word	1073887232
 1913 0068 0024F400 		.word	16000000
 1914              		.cfi_endproc
 1915              	.LFE301:
 1917              		.section	.text.LL_RCC_GetDFSDMClockFreq,"ax",%progbits
 1918              		.align	1
 1919              		.global	LL_RCC_GetDFSDMClockFreq
 1920              		.syntax unified
 1921              		.thumb
 1922              		.thumb_func
 1924              	LL_RCC_GetDFSDMClockFreq:
 1925              	.LVL178:
 1926              	.LFB307:
1077:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1927              		.loc 1 1077 1 is_stmt 1 view -0
 1928              		.cfi_startproc
 1929              		@ args = 0, pretend = 0, frame = 0
 1930              		@ frame_needed = 0, uses_anonymous_args = 0
1077:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 1931              		.loc 1 1077 1 is_stmt 0 view .LVU569
 1932 0000 08B5     		push	{r3, lr}
 1933              	.LCFI8:
 1934              		.cfi_def_cfa_offset 8
 1935              		.cfi_offset 3, -8
 1936              		.cfi_offset 14, -4
1078:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1937              		.loc 1 1078 3 is_stmt 1 view .LVU570
 1938              	.LVL179:
1081:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1939              		.loc 1 1081 3 view .LVU571
1084:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1940              		.loc 1 1084 3 view .LVU572
 1941              	.LBB340:
 1942              	.LBI340:
2891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1943              		.loc 2 2891 26 view .LVU573
 1944              	.LBB341:
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1945              		.loc 2 2893 3 view .LVU574
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1946              		.loc 2 2893 21 is_stmt 0 view .LVU575
 1947 0002 084B     		ldr	r3, .L160
ARM GAS  /tmp/cc42qbQx.s 			page 140


 1948 0004 D3F88C30 		ldr	r3, [r3, #140]
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1949              		.loc 2 2893 10 view .LVU576
 1950 0008 1840     		ands	r0, r0, r3
 1951              	.LVL180:
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1952              		.loc 2 2893 10 view .LVU577
 1953              	.LBE341:
 1954              	.LBE340:
1084:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 1955              		.loc 1 1084 3 discriminator 1 view .LVU578
 1956 000a B0F1007F 		cmp	r0, #33554432
 1957 000e 06D0     		beq	.L159
1092:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1958              		.loc 1 1092 7 is_stmt 1 view .LVU579
1092:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1959              		.loc 1 1092 25 is_stmt 0 view .LVU580
 1960 0010 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1961              	.LVL181:
1092:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1962              		.loc 1 1092 25 discriminator 1 view .LVU581
 1963 0014 FFF7FEFF 		bl	RCC_GetHCLKClockFreq
 1964              	.LVL182:
1092:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1965              		.loc 1 1092 25 discriminator 2 view .LVU582
 1966 0018 FFF7FEFF 		bl	RCC_GetPCLK2ClockFreq
 1967              	.LVL183:
1093:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 1968              		.loc 1 1093 7 is_stmt 1 view .LVU583
1096:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 1969              		.loc 1 1096 3 view .LVU584
 1970              	.L155:
1097:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1971              		.loc 1 1097 1 is_stmt 0 view .LVU585
 1972 001c 08BD     		pop	{r3, pc}
 1973              	.LVL184:
 1974              	.L159:
1087:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1975              		.loc 1 1087 7 is_stmt 1 view .LVU586
1087:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 1976              		.loc 1 1087 25 is_stmt 0 view .LVU587
 1977 001e FFF7FEFF 		bl	RCC_GetSystemClockFreq
 1978              	.LVL185:
1088:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 1979              		.loc 1 1088 7 is_stmt 1 view .LVU588
 1980 0022 FBE7     		b	.L155
 1981              	.L161:
 1982              		.align	2
 1983              	.L160:
 1984 0024 00380240 		.word	1073887232
 1985              		.cfi_endproc
 1986              	.LFE307:
 1988              		.section	.text.RCC_PLL_GetFreqDomain_48M,"ax",%progbits
 1989              		.align	1
 1990              		.global	RCC_PLL_GetFreqDomain_48M
 1991              		.syntax unified
 1992              		.thumb
ARM GAS  /tmp/cc42qbQx.s 			page 141


 1993              		.thumb_func
 1995              	RCC_PLL_GetFreqDomain_48M:
 1996              	.LFB316:
1320:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1321:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1322:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLL clock frequency used for 48 MHz domain
1323:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLL clock frequency (in Hz)
1324:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1325:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_48M(void)
1326:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 1997              		.loc 1 1326 1 view -0
 1998              		.cfi_startproc
 1999              		@ args = 0, pretend = 0, frame = 0
 2000              		@ frame_needed = 0, uses_anonymous_args = 0
 2001              		@ link register save eliminated.
1327:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 2002              		.loc 1 1327 3 view .LVU590
 2003              	.LVL186:
1328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1329:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLL_VCO = (HSE_VALUE or HSI_VALUE / PLLM ) * PLLN
1330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      48M Domain clock = PLL_VCO / PLLQ
1331:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1332:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 2004              		.loc 1 1332 3 view .LVU591
 2005              	.LBB342:
 2006              	.LBI342:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2007              		.loc 2 3461 26 view .LVU592
 2008              	.LBB343:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2009              		.loc 2 3463 3 view .LVU593
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2010              		.loc 2 3463 21 is_stmt 0 view .LVU594
 2011 0000 0C4B     		ldr	r3, .L165
 2012 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2013              		.loc 2 3463 10 view .LVU595
 2014 0004 03F48003 		and	r3, r3, #4194304
 2015              	.LVL187:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2016              		.loc 2 3463 10 view .LVU596
 2017              	.LBE343:
 2018              	.LBE342:
1333:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1334:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 2019              		.loc 1 1334 3 is_stmt 1 view .LVU597
 2020 0008 8BB9     		cbnz	r3, .L164
1335:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1336:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLL clock source */
1337:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 2021              		.loc 1 1337 20 is_stmt 0 view .LVU598
 2022 000a 0B4B     		ldr	r3, .L165+4
 2023              	.LVL188:
 2024              	.L163:
1338:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1339:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1340:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLL clock source */
ARM GAS  /tmp/cc42qbQx.s 			page 142


1341:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1342:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1345:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1346:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1348:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLCLK_48M_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 2025              		.loc 1 1348 3 is_stmt 1 view .LVU599
 2026              	.LBB344:
 2027              	.LBI344:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2028              		.loc 2 3601 26 view .LVU600
 2029              	.LBB345:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2030              		.loc 2 3603 3 view .LVU601
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2031              		.loc 2 3603 21 is_stmt 0 view .LVU602
 2032 000c 094A     		ldr	r2, .L165
 2033 000e 5168     		ldr	r1, [r2, #4]
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2034              		.loc 2 3603 10 view .LVU603
 2035 0010 01F03F01 		and	r1, r1, #63
 2036              	.LBE345:
 2037              	.LBE344:
 2038              		.loc 1 1348 10 discriminator 1 view .LVU604
 2039 0014 B3FBF1F3 		udiv	r3, r3, r1
 2040              	.LVL189:
 2041              	.LBB346:
 2042              	.LBI346:
3471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2043              		.loc 2 3471 26 is_stmt 1 view .LVU605
 2044              	.LBB347:
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2045              		.loc 2 3473 3 view .LVU606
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2046              		.loc 2 3473 21 is_stmt 0 view .LVU607
 2047 0018 5168     		ldr	r1, [r2, #4]
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2048              		.loc 2 3473 10 view .LVU608
 2049 001a C1F38811 		ubfx	r1, r1, #6, #9
 2050              	.LBE347:
 2051              	.LBE346:
 2052              		.loc 1 1348 10 discriminator 2 view .LVU609
 2053 001e 01FB03F3 		mul	r3, r1, r3
 2054              	.LBB348:
 2055              	.LBI348:
3510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2056              		.loc 2 3510 26 is_stmt 1 view .LVU610
 2057              	.LBB349:
3512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2058              		.loc 2 3512 3 view .LVU611
3512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2059              		.loc 2 3512 21 is_stmt 0 view .LVU612
 2060 0022 5068     		ldr	r0, [r2, #4]
 2061              	.LBE349:
 2062              	.LBE348:
ARM GAS  /tmp/cc42qbQx.s 			page 143


 2063              		.loc 1 1348 10 discriminator 3 view .LVU613
 2064 0024 C0F30360 		ubfx	r0, r0, #24, #4
1349:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLL_GetN(), LL_RCC_PLL_GetQ());
1350:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2065              		.loc 1 1350 1 view .LVU614
 2066 0028 B3FBF0F0 		udiv	r0, r3, r0
 2067 002c 7047     		bx	lr
 2068              	.LVL190:
 2069              	.L164:
1341:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2070              		.loc 1 1341 20 view .LVU615
 2071 002e 034B     		ldr	r3, .L165+8
 2072              	.LVL191:
1341:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2073              		.loc 1 1341 20 view .LVU616
 2074 0030 ECE7     		b	.L163
 2075              	.L166:
 2076 0032 00BF     		.align	2
 2077              	.L165:
 2078 0034 00380240 		.word	1073887232
 2079 0038 0024F400 		.word	16000000
 2080 003c 40787D01 		.word	25000000
 2081              		.cfi_endproc
 2082              	.LFE316:
 2084              		.section	.text.RCC_PLLSAI_GetFreqDomain_SAI,"ax",%progbits
 2085              		.align	1
 2086              		.global	RCC_PLLSAI_GetFreqDomain_SAI
 2087              		.syntax unified
 2088              		.thumb
 2089              		.thumb_func
 2091              	RCC_PLLSAI_GetFreqDomain_SAI:
 2092              	.LFB317:
1351:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1352:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(DSI)
1353:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1354:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLL clock frequency used for DSI clock
1355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLL clock frequency (in Hz)
1356:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1357:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLL_GetFreqDomain_DSI(void)
1358:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
1359:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
1360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1361:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLL_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLN
1362:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      DSICLK = PLL_VCO / PLLR
1363:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1364:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
1365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1366:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
1367:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1368:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLL clock source */
1369:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1371:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLL clock source */
1373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1374:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1375:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
ARM GAS  /tmp/cc42qbQx.s 			page 144


1376:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLCLK_DSI_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
1378:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLL_GetN(), LL_RCC_PLL_GetR());
1379:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
1380:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DSI */
1381:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1382:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1383:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLSAI clock frequency used for SAI1 and SAI2 domains
1384:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLSAI clock frequency (in Hz)
1385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1386:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_SAI(void)
1387:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 2093              		.loc 1 1387 1 is_stmt 1 view -0
 2094              		.cfi_startproc
 2095              		@ args = 0, pretend = 0, frame = 0
 2096              		@ frame_needed = 0, uses_anonymous_args = 0
 2097              		@ link register save eliminated.
1388:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 2098              		.loc 1 1388 3 view .LVU618
 2099              	.LVL192:
1389:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLSAI_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLSAIN
1391:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      SAI1 and SAI2 domains clock  = (PLLSAI_VCO / PLLSAIQ) / PLLSAIDIVQ
1392:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1393:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 2100              		.loc 1 1393 3 view .LVU619
 2101              	.LBB350:
 2102              	.LBI350:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2103              		.loc 2 3461 26 view .LVU620
 2104              	.LBB351:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2105              		.loc 2 3463 3 view .LVU621
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2106              		.loc 2 3463 21 is_stmt 0 view .LVU622
 2107 0000 104B     		ldr	r3, .L170
 2108 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2109              		.loc 2 3463 10 view .LVU623
 2110 0004 03F48003 		and	r3, r3, #4194304
 2111              	.LVL193:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2112              		.loc 2 3463 10 view .LVU624
 2113              	.LBE351:
 2114              	.LBE350:
1394:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 2115              		.loc 1 1395 3 is_stmt 1 view .LVU625
 2116 0008 CBB9     		cbnz	r3, .L169
1396:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLSAI clock source */
1398:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 2117              		.loc 1 1398 20 is_stmt 0 view .LVU626
 2118 000a 0F48     		ldr	r0, .L170+4
 2119              	.L168:
 2120              	.LVL194:
1399:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
ARM GAS  /tmp/cc42qbQx.s 			page 145


1400:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1401:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLSAI clock source */
1402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1404:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1405:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1406:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1407:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1408:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLSAI_SAI_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 2121              		.loc 1 1409 3 is_stmt 1 view .LVU627
 2122              	.LBB352:
 2123              	.LBI352:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2124              		.loc 2 3601 26 view .LVU628
 2125              	.LBB353:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2126              		.loc 2 3603 3 view .LVU629
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2127              		.loc 2 3603 21 is_stmt 0 view .LVU630
 2128 000c 0D4A     		ldr	r2, .L170
 2129 000e 5368     		ldr	r3, [r2, #4]
 2130              	.LVL195:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2131              		.loc 2 3603 10 view .LVU631
 2132 0010 03F03F03 		and	r3, r3, #63
 2133              	.LBE353:
 2134              	.LBE352:
 2135              		.loc 1 1409 10 discriminator 1 view .LVU632
 2136 0014 B0FBF3F0 		udiv	r0, r0, r3
 2137              	.LVL196:
 2138              	.LBB354:
 2139              	.LBI354:
4182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLSAI used for SAI1 and SAI2 domain clock
4186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
4187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
4188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLQ can be written only when PLLSAI is disabled
4189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This can be selected for SAI1 and SAI2
4190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLSAI_ConfigDomain_SAI\n
4191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLSAI_ConfigDomain_SAI\n
4192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIN       LL_RCC_PLLSAI_ConfigDomain_SAI\n
4193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIQ       LL_RCC_PLLSAI_ConfigDomain_SAI\n
4194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1     PLLSAIDIVQ    LL_RCC_PLLSAI_ConfigDomain_SAI
4195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
4196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
4197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
4198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
4199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
4200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
4201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
4202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
4203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
4204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
4205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
ARM GAS  /tmp/cc42qbQx.s 			page 146


4206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
4207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
4208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
4209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
4210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
4211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
4212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
4213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
4214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
4215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
4216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
4217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
4218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
4219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
4220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
4221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
4222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
4223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
4224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
4225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
4226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
4227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
4228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
4229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
4230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
4231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
4232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
4233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
4234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
4235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
4236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
4237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
4238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
4239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
4240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
4241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
4242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
4243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
4244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
4245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
4246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
4247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
4248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
4249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
4250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
4251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
4252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
4253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
4254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
4255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
4256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
4257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
4258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
4259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
4260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
4261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
4262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLQ This parameter can be one of the following values:
ARM GAS  /tmp/cc42qbQx.s 			page 147


4263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_2
4264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_3
4265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_4
4266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_5
4267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_6
4268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_7
4269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_8
4270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_9
4271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_10
4272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_11
4273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_12
4274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_13
4275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_14
4276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_15
4277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLDIVQ This parameter can be one of the following values:
4278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_1
4279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_2
4280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_3
4281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_4
4282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_5
4283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_6
4284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_7
4285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_8
4286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_9
4287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_10
4288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_11
4289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_12
4290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_13
4291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_14
4292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_15
4293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_16
4294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_17
4295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_18
4296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_19
4297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_20
4298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_21
4299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_22
4300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_23
4301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_24
4302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_25
4303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_26
4304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_27
4305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_28
4306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_29
4307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_30
4308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_31
4309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_32
4310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_ConfigDomain_SAI(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
4313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
4315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIN | RCC_PLLSAICFGR_PLLSAIQ, PLLN << RCC_PLLSAICF
4316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLSAIDIVQ, PLLDIVQ);
4317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/cc42qbQx.s 			page 148


4320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief Configure PLLSAI used for 48Mhz domain clock
4321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
4322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
4323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLP can be written only when PLLSAI is disabled
4324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for USB, RNG, SDMMC1
4325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLSAI_ConfigDomain_48M\n
4326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLSAI_ConfigDomain_48M\n
4327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIN       LL_RCC_PLLSAI_ConfigDomain_48M\n
4328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIP       LL_RCC_PLLSAI_ConfigDomain_48M
4329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
4330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
4331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
4332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
4333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
4334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
4335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
4336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
4337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
4338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
4339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
4340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
4341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
4342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
4343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
4344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
4345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
4346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
4347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
4348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
4349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
4350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
4351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
4352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
4353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
4354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
4355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
4356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
4357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
4358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
4359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
4360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
4361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
4362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
4363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
4364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
4365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
4366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
4367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
4368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
4369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
4370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
4371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
4372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
4373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
4374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
4375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
4376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
ARM GAS  /tmp/cc42qbQx.s 			page 149


4377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
4378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
4379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
4380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
4381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
4382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
4383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
4384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
4385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
4386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
4387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
4388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
4389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
4390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
4391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
4392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
4393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
4394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
4395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
4396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLP This parameter can be one of the following values:
4397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_2
4398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_4
4399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_6
4400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_8
4401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_ConfigDomain_48M(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
4404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
4406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIN | RCC_PLLSAICFGR_PLLSAIP, PLLN << RCC_PLLSAICF
4407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(LTDC)
4410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLSAI used for LTDC domain clock
4412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
4413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
4414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLR can be written only when PLLSAI is disabled
4415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for LTDC
4416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLSAI_ConfigDomain_LTDC\n
4417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLSAI_ConfigDomain_LTDC\n
4418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIN       LL_RCC_PLLSAI_ConfigDomain_LTDC\n
4419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLSAICFGR   PLLSAIR       LL_RCC_PLLSAI_ConfigDomain_LTDC\n
4420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1     PLLSAIDIVR    LL_RCC_PLLSAI_ConfigDomain_LTDC
4421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
4422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
4423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
4424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
4425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
4426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
4427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
4428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
4429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
4430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
4431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
4432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
4433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
ARM GAS  /tmp/cc42qbQx.s 			page 150


4434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
4435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
4436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
4437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
4438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
4439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
4440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
4441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
4442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
4443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
4444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
4445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
4446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
4447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
4448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
4449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
4450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
4451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
4452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
4453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
4454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
4455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
4456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
4457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
4458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
4459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
4460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
4461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
4462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
4463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
4464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
4465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
4466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
4467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
4468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
4469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
4470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
4471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
4472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
4473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
4474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
4475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
4476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
4477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
4478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
4479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
4480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
4481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
4482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
4483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
4484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
4485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
4486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
4487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
4488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLR This parameter can be one of the following values:
4489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_2
4490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_3
ARM GAS  /tmp/cc42qbQx.s 			page 151


4491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_4
4492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_5
4493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_6
4494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_7
4495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLDIVR This parameter can be one of the following values:
4496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_2
4497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_4
4498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_8
4499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_16
4500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_ConfigDomain_LTDC(uint32_t Source, uint32_t PLLM, uint32_t PLLN,
4503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
4505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIN | RCC_PLLSAICFGR_PLLSAIR, PLLN << RCC_PLLSAICF
4506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLSAIDIVR, PLLDIVR);
4507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LTDC */
4509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL multiplication factor for VCO
4512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLSAICFGR  PLLSAIN      LL_RCC_PLLSAI_GetN
4513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between 50 and 432
4514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetN(void)
 2140              		.loc 2 4515 26 is_stmt 1 view .LVU633
 2141              	.LBB355:
4516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIN) >> RCC_PLLSAICFGR_PLLSAIN_Pos
 2142              		.loc 2 4517 3 view .LVU634
 2143              		.loc 2 4517 21 is_stmt 0 view .LVU635
 2144 0018 D2F88830 		ldr	r3, [r2, #136]
 2145              		.loc 2 4517 10 view .LVU636
 2146 001c C3F38813 		ubfx	r3, r3, #6, #9
 2147              	.LBE355:
 2148              	.LBE354:
 2149              		.loc 1 1409 10 discriminator 2 view .LVU637
 2150 0020 03FB00F0 		mul	r0, r3, r0
 2151              	.LBB356:
 2152              	.LBI356:
4518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL division factor for PLLSAIQ
4522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLSAICFGR  PLLSAIQ      LL_RCC_PLLSAI_GetQ
4523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_2
4525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_3
4526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_4
4527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_5
4528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_6
4529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_7
4530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_8
4531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_9
4532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_10
4533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_11
4534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_12
ARM GAS  /tmp/cc42qbQx.s 			page 152


4535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_13
4536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_14
4537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_15
4538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetQ(void)
 2153              		.loc 2 4539 26 is_stmt 1 view .LVU638
 2154              	.LBB357:
4540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIQ));
 2155              		.loc 2 4541 3 view .LVU639
 2156              		.loc 2 4541 21 is_stmt 0 view .LVU640
 2157 0024 D2F88830 		ldr	r3, [r2, #136]
 2158              	.LBE357:
 2159              	.LBE356:
 2160              		.loc 1 1409 10 discriminator 3 view .LVU641
 2161 0028 C3F30363 		ubfx	r3, r3, #24, #4
 2162              	.LBB358:
 2163              	.LBI358:
4542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLSAICFGR_PLLSAIR)
4545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL division factor for PLLSAIR
4547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLSAICLK (SAI clock)
4548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLSAICFGR  PLLSAIR      LL_RCC_PLLSAI_GetR
4549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_2
4551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_3
4552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_4
4553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_5
4554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_6
4555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_7
4556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetR(void)
4558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIR));
4560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLSAICFGR_PLLSAIR */
4562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL division factor for PLLSAIP
4565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLL48MCLK (48M domain clock)
4566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLSAICFGR  PLLSAIP      LL_RCC_PLLSAI_GetP
4567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_2
4569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_4
4570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_6
4571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_8
4572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetP(void)
4574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLSAICFGR, RCC_PLLSAICFGR_PLLSAIP));
4576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL division factor for PLLSAIDIVQ
4580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used PLLSAI1CLK, PLLSAI2CLK selected (SAI1 and SAI2 clock)
ARM GAS  /tmp/cc42qbQx.s 			page 153


4581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1   PLLSAIDIVQ      LL_RCC_PLLSAI_GetDIVQ
4582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_1
4584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_2
4585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_3
4586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_4
4587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_5
4588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_6
4589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_7
4590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_8
4591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_9
4592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_10
4593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_11
4594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_12
4595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_13
4596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_14
4597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_15
4598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_16
4599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_17
4600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_18
4601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_19
4602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_20
4603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_21
4604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_22
4605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_23
4606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_24
4607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_25
4608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_26
4609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_27
4610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_28
4611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_29
4612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_30
4613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_31
4614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_32
4615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetDIVQ(void)
 2164              		.loc 2 4616 26 is_stmt 1 view .LVU642
 2165              	.LBB359:
4617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLSAIDIVQ));
 2166              		.loc 2 4618 3 view .LVU643
 2167              		.loc 2 4618 21 is_stmt 0 view .LVU644
 2168 002c D2F88C20 		ldr	r2, [r2, #140]
 2169              	.LBE359:
 2170              	.LBE358:
 2171              		.loc 1 1409 10 discriminator 4 view .LVU645
 2172 0030 C2F30422 		ubfx	r2, r2, #8, #5
 2173 0034 02FB0333 		mla	r3, r2, r3, r3
1410:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLSAI_GetN(), LL_RCC_PLLSAI_GetQ(), LL_RCC_PLLSAI_G
1411:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2174              		.loc 1 1411 1 view .LVU646
 2175 0038 B0FBF3F0 		udiv	r0, r0, r3
 2176 003c 7047     		bx	lr
 2177              	.LVL197:
 2178              	.L169:
1402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2179              		.loc 1 1402 20 view .LVU647
ARM GAS  /tmp/cc42qbQx.s 			page 154


 2180 003e 0348     		ldr	r0, .L170+8
 2181 0040 E4E7     		b	.L168
 2182              	.L171:
 2183 0042 00BF     		.align	2
 2184              	.L170:
 2185 0044 00380240 		.word	1073887232
 2186 0048 0024F400 		.word	16000000
 2187 004c 40787D01 		.word	25000000
 2188              		.cfi_endproc
 2189              	.LFE317:
 2191              		.section	.text.RCC_PLLSAI_GetFreqDomain_48M,"ax",%progbits
 2192              		.align	1
 2193              		.global	RCC_PLLSAI_GetFreqDomain_48M
 2194              		.syntax unified
 2195              		.thumb
 2196              		.thumb_func
 2198              	RCC_PLLSAI_GetFreqDomain_48M:
 2199              	.LFB318:
1412:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1413:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1414:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLSAI clock frequency used for 48Mhz domain
1415:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLSAI clock frequency (in Hz)
1416:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1417:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_48M(void)
1418:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 2200              		.loc 1 1418 1 is_stmt 1 view -0
 2201              		.cfi_startproc
 2202              		@ args = 0, pretend = 0, frame = 0
 2203              		@ frame_needed = 0, uses_anonymous_args = 0
 2204              		@ link register save eliminated.
1419:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 2205              		.loc 1 1419 3 view .LVU649
 2206              	.LVL198:
1420:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1421:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLSAI_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLSAIN
1422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      48M Domain clock  = PLLSAI_VCO / PLLSAIP
1423:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1424:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 2207              		.loc 1 1424 3 view .LVU650
 2208              	.LBB360:
 2209              	.LBI360:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2210              		.loc 2 3461 26 view .LVU651
 2211              	.LBB361:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2212              		.loc 2 3463 3 view .LVU652
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2213              		.loc 2 3463 21 is_stmt 0 view .LVU653
 2214 0000 0E4B     		ldr	r3, .L175
 2215 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2216              		.loc 2 3463 10 view .LVU654
 2217 0004 03F48003 		and	r3, r3, #4194304
 2218              	.LVL199:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2219              		.loc 2 3463 10 view .LVU655
 2220              	.LBE361:
ARM GAS  /tmp/cc42qbQx.s 			page 155


 2221              	.LBE360:
1425:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1426:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 2222              		.loc 1 1426 3 is_stmt 1 view .LVU656
 2223 0008 ABB9     		cbnz	r3, .L174
1427:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1428:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLSAI clock source */
1429:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 2224              		.loc 1 1429 20 is_stmt 0 view .LVU657
 2225 000a 0D48     		ldr	r0, .L175+4
 2226              	.L173:
 2227              	.LVL200:
1430:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1431:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1432:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLSAI clock source */
1433:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1434:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1435:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1436:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1437:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1438:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1439:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1440:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLSAI_48M_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 2228              		.loc 1 1440 3 is_stmt 1 view .LVU658
 2229              	.LBB362:
 2230              	.LBI362:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2231              		.loc 2 3601 26 view .LVU659
 2232              	.LBB363:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2233              		.loc 2 3603 3 view .LVU660
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2234              		.loc 2 3603 21 is_stmt 0 view .LVU661
 2235 000c 0B4B     		ldr	r3, .L175
 2236              	.LVL201:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2237              		.loc 2 3603 21 view .LVU662
 2238 000e 5A68     		ldr	r2, [r3, #4]
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2239              		.loc 2 3603 10 view .LVU663
 2240 0010 02F03F02 		and	r2, r2, #63
 2241              	.LBE363:
 2242              	.LBE362:
 2243              		.loc 1 1440 10 discriminator 1 view .LVU664
 2244 0014 B0FBF2F0 		udiv	r0, r0, r2
 2245              	.LVL202:
 2246              	.LBB364:
 2247              	.LBI364:
4515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2248              		.loc 2 4515 26 is_stmt 1 view .LVU665
 2249              	.LBB365:
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2250              		.loc 2 4517 3 view .LVU666
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2251              		.loc 2 4517 21 is_stmt 0 view .LVU667
 2252 0018 D3F88820 		ldr	r2, [r3, #136]
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/cc42qbQx.s 			page 156


 2253              		.loc 2 4517 10 view .LVU668
 2254 001c C2F38812 		ubfx	r2, r2, #6, #9
 2255              	.LBE365:
 2256              	.LBE364:
 2257              		.loc 1 1440 10 discriminator 2 view .LVU669
 2258 0020 02FB00F0 		mul	r0, r2, r0
 2259              	.LBB366:
 2260              	.LBI366:
4573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2261              		.loc 2 4573 26 is_stmt 1 view .LVU670
 2262              	.LBB367:
4575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2263              		.loc 2 4575 3 view .LVU671
4575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2264              		.loc 2 4575 21 is_stmt 0 view .LVU672
 2265 0024 D3F88830 		ldr	r3, [r3, #136]
 2266              	.LBE367:
 2267              	.LBE366:
 2268              		.loc 1 1440 10 discriminator 3 view .LVU673
 2269 0028 C3F30143 		ubfx	r3, r3, #16, #2
 2270 002c 0133     		adds	r3, r3, #1
 2271 002e 5B00     		lsls	r3, r3, #1
1441:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLSAI_GetN(), LL_RCC_PLLSAI_GetP());
1442:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2272              		.loc 1 1442 1 view .LVU674
 2273 0030 B0FBF3F0 		udiv	r0, r0, r3
 2274 0034 7047     		bx	lr
 2275              	.LVL203:
 2276              	.L174:
1433:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2277              		.loc 1 1433 20 view .LVU675
 2278 0036 0348     		ldr	r0, .L175+8
 2279 0038 E8E7     		b	.L173
 2280              	.L176:
 2281 003a 00BF     		.align	2
 2282              	.L175:
 2283 003c 00380240 		.word	1073887232
 2284 0040 0024F400 		.word	16000000
 2285 0044 40787D01 		.word	25000000
 2286              		.cfi_endproc
 2287              	.LFE318:
 2289              		.section	.text.LL_RCC_GetSDMMCClockFreq,"ax",%progbits
 2290              		.align	1
 2291              		.global	LL_RCC_GetSDMMCClockFreq
 2292              		.syntax unified
 2293              		.thumb
 2294              		.thumb_func
 2296              	LL_RCC_GetSDMMCClockFreq:
 2297              	.LVL204:
 2298              	.LFB303:
 886:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sdmmc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2299              		.loc 1 886 1 is_stmt 1 view -0
 2300              		.cfi_startproc
 2301              		@ args = 0, pretend = 0, frame = 0
 2302              		@ frame_needed = 0, uses_anonymous_args = 0
 886:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sdmmc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2303              		.loc 1 886 1 is_stmt 0 view .LVU677
ARM GAS  /tmp/cc42qbQx.s 			page 157


 2304 0000 08B5     		push	{r3, lr}
 2305              	.LCFI9:
 2306              		.cfi_def_cfa_offset 8
 2307              		.cfi_offset 3, -8
 2308              		.cfi_offset 14, -4
 887:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2309              		.loc 1 887 3 is_stmt 1 view .LVU678
 2310              	.LVL205:
 890:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2311              		.loc 1 890 3 view .LVU679
 892:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2312              		.loc 1 892 3 view .LVU680
 892:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2313              		.loc 1 892 6 is_stmt 0 view .LVU681
 2314 0002 B0F1805F 		cmp	r0, #268435456
 2315 0006 16D0     		beq	.L185
 927:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      {
 2316              		.loc 1 927 6 is_stmt 1 view .LVU682
 2317              	.LVL206:
 2318              	.LBB368:
 2319              	.LBI368:
2790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2320              		.loc 2 2790 26 view .LVU683
 2321              	.LBB369:
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2322              		.loc 2 2792 3 view .LVU684
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2323              		.loc 2 2792 21 is_stmt 0 view .LVU685
 2324 0008 214B     		ldr	r3, .L186
 2325 000a D3F89030 		ldr	r3, [r3, #144]
 2326 000e 0340     		ands	r3, r3, r0
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2327              		.loc 2 2792 10 view .LVU686
 2328 0010 40EA1340 		orr	r0, r0, r3, lsr #16
 2329              	.LVL207:
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2330              		.loc 2 2792 10 view .LVU687
 2331              	.LBE369:
 2332              	.LBE368:
 927:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      {
 2333              		.loc 1 927 6 discriminator 1 view .LVU688
 2334 0014 B0F1005F 		cmp	r0, #536870912
 2335 0018 37D1     		bne	.L182
 930:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****          {
 2336              		.loc 1 930 10 is_stmt 1 view .LVU689
 2337              	.LVL208:
 2338              	.LBB370:
 2339              	.LBI370:
2804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2340              		.loc 2 2804 26 view .LVU690
 2341              	.LBB371:
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2342              		.loc 2 2806 3 view .LVU691
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2343              		.loc 2 2806 21 is_stmt 0 view .LVU692
 2344 001a 1D4B     		ldr	r3, .L186
 2345 001c D3F89030 		ldr	r3, [r3, #144]
ARM GAS  /tmp/cc42qbQx.s 			page 158


 2346              	.LVL209:
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2347              		.loc 2 2806 21 view .LVU693
 2348              	.LBE371:
 2349              	.LBE370:
 2350 0020 13F0006F 		tst	r3, #134217728
 2351 0024 29D1     		bne	.L183
 933:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 2352              		.loc 1 933 14 is_stmt 1 view .LVU694
 2353              	.LBB372:
 2354              	.LBI372:
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2355              		.loc 2 3153 26 view .LVU695
 2356              	.LBB373:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2357              		.loc 2 3155 3 view .LVU696
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2358              		.loc 2 3155 11 is_stmt 0 view .LVU697
 2359 0026 1A4B     		ldr	r3, .L186
 2360 0028 1868     		ldr	r0, [r3]
 2361              	.LBE373:
 2362              	.LBE372:
 933:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 2363              		.loc 1 933 17 discriminator 1 view .LVU698
 2364 002a 10F00070 		ands	r0, r0, #33554432
 2365 002e 2ED0     		beq	.L177
 935:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2366              		.loc 1 935 16 is_stmt 1 view .LVU699
 935:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2367              		.loc 1 935 34 is_stmt 0 view .LVU700
 2368 0030 FFF7FEFF 		bl	RCC_PLL_GetFreqDomain_48M
 2369              	.LVL210:
 935:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2370              		.loc 1 935 34 view .LVU701
 2371 0034 2BE0     		b	.L177
 2372              	.LVL211:
 2373              	.L185:
 895:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 2374              		.loc 1 895 5 is_stmt 1 view .LVU702
 2375              	.LBB374:
 2376              	.LBI374:
2790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2377              		.loc 2 2790 26 view .LVU703
 2378              	.LBB375:
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2379              		.loc 2 2792 3 view .LVU704
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2380              		.loc 2 2792 21 is_stmt 0 view .LVU705
 2381 0036 164B     		ldr	r3, .L186
 2382 0038 D3F89030 		ldr	r3, [r3, #144]
 2383 003c 0340     		ands	r3, r3, r0
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2384              		.loc 2 2792 10 view .LVU706
 2385 003e 40EA1340 		orr	r0, r0, r3, lsr #16
 2386              	.LVL212:
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2387              		.loc 2 2792 10 view .LVU707
ARM GAS  /tmp/cc42qbQx.s 			page 159


 2388              	.LBE375:
 2389              	.LBE374:
 895:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 2390              		.loc 1 895 5 discriminator 1 view .LVU708
 2391 0042 B0F1805F 		cmp	r0, #268435456
 2392 0046 15D1     		bne	.L179
 898:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 2393              		.loc 1 898 9 is_stmt 1 view .LVU709
 2394              	.LVL213:
 2395              	.LBB376:
 2396              	.LBI376:
2804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2397              		.loc 2 2804 26 view .LVU710
 2398              	.LBB377:
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2399              		.loc 2 2806 3 view .LVU711
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2400              		.loc 2 2806 21 is_stmt 0 view .LVU712
 2401 0048 114B     		ldr	r3, .L186
 2402 004a D3F89030 		ldr	r3, [r3, #144]
 2403              	.LVL214:
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2404              		.loc 2 2806 21 view .LVU713
 2405              	.LBE377:
 2406              	.LBE376:
 2407 004e 13F0006F 		tst	r3, #134217728
 2408 0052 07D1     		bne	.L180
 901:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 2409              		.loc 1 901 13 is_stmt 1 view .LVU714
 2410              	.LBB378:
 2411              	.LBI378:
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2412              		.loc 2 3153 26 view .LVU715
 2413              	.LBB379:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2414              		.loc 2 3155 3 view .LVU716
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2415              		.loc 2 3155 11 is_stmt 0 view .LVU717
 2416 0054 0E4B     		ldr	r3, .L186
 2417 0056 1868     		ldr	r0, [r3]
 2418              	.LBE379:
 2419              	.LBE378:
 901:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 2420              		.loc 1 901 16 discriminator 1 view .LVU718
 2421 0058 10F00070 		ands	r0, r0, #33554432
 2422 005c 17D0     		beq	.L177
 903:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2423              		.loc 1 903 15 is_stmt 1 view .LVU719
 903:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2424              		.loc 1 903 33 is_stmt 0 view .LVU720
 2425 005e FFF7FEFF 		bl	RCC_PLL_GetFreqDomain_48M
 2426              	.LVL215:
 903:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2427              		.loc 1 903 33 view .LVU721
 2428 0062 14E0     		b	.L177
 2429              	.LVL216:
 2430              	.L180:
ARM GAS  /tmp/cc42qbQx.s 			page 160


 909:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 2431              		.loc 1 909 13 is_stmt 1 view .LVU722
 2432              	.LBB380:
 2433              	.LBI380:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2434              		.loc 2 4179 26 view .LVU723
 2435              	.LBB381:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2436              		.loc 2 4181 3 view .LVU724
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2437              		.loc 2 4181 11 is_stmt 0 view .LVU725
 2438 0064 0A4B     		ldr	r3, .L186
 2439 0066 1868     		ldr	r0, [r3]
 2440              	.LBE381:
 2441              	.LBE380:
 909:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             {
 2442              		.loc 1 909 16 discriminator 1 view .LVU726
 2443 0068 10F00050 		ands	r0, r0, #536870912
 2444 006c 0FD0     		beq	.L177
 911:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2445              		.loc 1 911 15 is_stmt 1 view .LVU727
 911:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2446              		.loc 1 911 33 is_stmt 0 view .LVU728
 2447 006e FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_48M
 2448              	.LVL217:
 911:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****             }
 2449              		.loc 1 911 33 view .LVU729
 2450 0072 0CE0     		b	.L177
 2451              	.LVL218:
 2452              	.L179:
 919:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2453              		.loc 1 919 7 is_stmt 1 view .LVU730
 919:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2454              		.loc 1 919 25 is_stmt 0 view .LVU731
 2455 0074 FFF7FEFF 		bl	RCC_GetSystemClockFreq
 2456              	.LVL219:
 920:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     }
 2457              		.loc 1 920 7 is_stmt 1 view .LVU732
 2458 0078 09E0     		b	.L177
 2459              	.LVL220:
 2460              	.L183:
 941:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 2461              		.loc 1 941 14 view .LVU733
 2462              	.LBB382:
 2463              	.LBI382:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2464              		.loc 2 4179 26 view .LVU734
 2465              	.LBB383:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2466              		.loc 2 4181 3 view .LVU735
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2467              		.loc 2 4181 11 is_stmt 0 view .LVU736
 2468 007a 054B     		ldr	r3, .L186
 2469 007c 1868     		ldr	r0, [r3]
 2470              	.LBE383:
 2471              	.LBE382:
 941:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
ARM GAS  /tmp/cc42qbQx.s 			page 161


 2472              		.loc 1 941 17 discriminator 1 view .LVU737
 2473 007e 10F00050 		ands	r0, r0, #536870912
 2474 0082 04D0     		beq	.L177
 943:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2475              		.loc 1 943 16 is_stmt 1 view .LVU738
 943:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2476              		.loc 1 943 34 is_stmt 0 view .LVU739
 2477 0084 FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_48M
 2478              	.LVL221:
 943:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 2479              		.loc 1 943 34 view .LVU740
 2480 0088 01E0     		b	.L177
 2481              	.LVL222:
 2482              	.L182:
 951:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        break;
 2483              		.loc 1 951 8 is_stmt 1 view .LVU741
 951:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****        break;
 2484              		.loc 1 951 26 is_stmt 0 view .LVU742
 2485 008a FFF7FEFF 		bl	RCC_GetSystemClockFreq
 2486              	.LVL223:
 952:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      }
 2487              		.loc 1 952 8 is_stmt 1 view .LVU743
 957:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2488              		.loc 1 957 3 view .LVU744
 2489              	.L177:
 958:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2490              		.loc 1 958 1 is_stmt 0 view .LVU745
 2491 008e 08BD     		pop	{r3, pc}
 2492              	.L187:
 2493              		.align	2
 2494              	.L186:
 2495 0090 00380240 		.word	1073887232
 2496              		.cfi_endproc
 2497              	.LFE303:
 2499              		.section	.text.LL_RCC_GetRNGClockFreq,"ax",%progbits
 2500              		.align	1
 2501              		.global	LL_RCC_GetRNGClockFreq
 2502              		.syntax unified
 2503              		.thumb
 2504              		.thumb_func
 2506              	LL_RCC_GetRNGClockFreq:
 2507              	.LVL224:
 2508              	.LFB304:
 968:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t rng_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2509              		.loc 1 968 1 is_stmt 1 view -0
 2510              		.cfi_startproc
 2511              		@ args = 0, pretend = 0, frame = 0
 2512              		@ frame_needed = 0, uses_anonymous_args = 0
 968:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t rng_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2513              		.loc 1 968 1 is_stmt 0 view .LVU747
 2514 0000 08B5     		push	{r3, lr}
 2515              	.LCFI10:
 2516              		.cfi_def_cfa_offset 8
 2517              		.cfi_offset 3, -8
 2518              		.cfi_offset 14, -4
 969:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2519              		.loc 1 969 3 is_stmt 1 view .LVU748
ARM GAS  /tmp/cc42qbQx.s 			page 162


 2520              	.LVL225:
 972:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2521              		.loc 1 972 3 view .LVU749
 975:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2522              		.loc 1 975 3 view .LVU750
 2523              	.LBB384:
 2524              	.LBI384:
2818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2525              		.loc 2 2818 26 view .LVU751
 2526              	.LBB385:
2820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2527              		.loc 2 2820 3 view .LVU752
2820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2528              		.loc 2 2820 21 is_stmt 0 view .LVU753
 2529 0002 0B4B     		ldr	r3, .L193
 2530 0004 D3F89030 		ldr	r3, [r3, #144]
 2531              	.LVL226:
2820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2532              		.loc 2 2820 21 view .LVU754
 2533              	.LBE385:
 2534              	.LBE384:
 975:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2535              		.loc 1 975 3 discriminator 1 view .LVU755
 2536 0008 1842     		tst	r0, r3
 2537 000a 08D1     		bne	.L189
 978:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2538              		.loc 1 978 7 is_stmt 1 view .LVU756
 2539              	.LBB386:
 2540              	.LBI386:
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2541              		.loc 2 3153 26 view .LVU757
 2542              	.LBB387:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2543              		.loc 2 3155 3 view .LVU758
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2544              		.loc 2 3155 11 is_stmt 0 view .LVU759
 2545 000c 084B     		ldr	r3, .L193
 2546 000e 1868     		ldr	r0, [r3]
 2547              	.LVL227:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2548              		.loc 2 3155 11 view .LVU760
 2549              	.LBE387:
 2550              	.LBE386:
 978:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2551              		.loc 1 978 10 discriminator 1 view .LVU761
 2552 0010 10F00070 		ands	r0, r0, #33554432
 2553 0014 00D1     		bne	.L192
 2554              	.LVL228:
 2555              	.L188:
 994:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2556              		.loc 1 994 1 view .LVU762
 2557 0016 08BD     		pop	{r3, pc}
 2558              	.LVL229:
 2559              	.L192:
 980:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2560              		.loc 1 980 9 is_stmt 1 view .LVU763
 980:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
ARM GAS  /tmp/cc42qbQx.s 			page 163


 2561              		.loc 1 980 25 is_stmt 0 view .LVU764
 2562 0018 FFF7FEFF 		bl	RCC_PLL_GetFreqDomain_48M
 2563              	.LVL230:
 980:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2564              		.loc 1 980 25 view .LVU765
 2565 001c FBE7     		b	.L188
 2566              	.LVL231:
 2567              	.L189:
 986:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2568              		.loc 1 986 7 is_stmt 1 view .LVU766
 2569              	.LBB388:
 2570              	.LBI388:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2571              		.loc 2 4179 26 view .LVU767
 2572              	.LBB389:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2573              		.loc 2 4181 3 view .LVU768
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2574              		.loc 2 4181 11 is_stmt 0 view .LVU769
 2575 001e 044B     		ldr	r3, .L193
 2576 0020 1868     		ldr	r0, [r3]
 2577              	.LVL232:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2578              		.loc 2 4181 11 view .LVU770
 2579              	.LBE389:
 2580              	.LBE388:
 986:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2581              		.loc 1 986 10 discriminator 1 view .LVU771
 2582 0022 10F00050 		ands	r0, r0, #536870912
 2583 0026 F6D0     		beq	.L188
 988:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2584              		.loc 1 988 9 is_stmt 1 view .LVU772
 988:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2585              		.loc 1 988 25 is_stmt 0 view .LVU773
 2586 0028 FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_48M
 2587              	.LVL233:
 993:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2588              		.loc 1 993 3 is_stmt 1 view .LVU774
 993:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2589              		.loc 1 993 10 is_stmt 0 view .LVU775
 2590 002c F3E7     		b	.L188
 2591              	.L194:
 2592 002e 00BF     		.align	2
 2593              	.L193:
 2594 0030 00380240 		.word	1073887232
 2595              		.cfi_endproc
 2596              	.LFE304:
 2598              		.section	.text.LL_RCC_GetUSBClockFreq,"ax",%progbits
 2599              		.align	1
 2600              		.global	LL_RCC_GetUSBClockFreq
 2601              		.syntax unified
 2602              		.thumb
 2603              		.thumb_func
 2605              	LL_RCC_GetUSBClockFreq:
 2606              	.LVL234:
 2607              	.LFB306:
1041:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usb_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
ARM GAS  /tmp/cc42qbQx.s 			page 164


 2608              		.loc 1 1041 1 is_stmt 1 view -0
 2609              		.cfi_startproc
 2610              		@ args = 0, pretend = 0, frame = 0
 2611              		@ frame_needed = 0, uses_anonymous_args = 0
1041:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t usb_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2612              		.loc 1 1041 1 is_stmt 0 view .LVU777
 2613 0000 08B5     		push	{r3, lr}
 2614              	.LCFI11:
 2615              		.cfi_def_cfa_offset 8
 2616              		.cfi_offset 3, -8
 2617              		.cfi_offset 14, -4
1042:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2618              		.loc 1 1042 3 is_stmt 1 view .LVU778
 2619              	.LVL235:
1045:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2620              		.loc 1 1045 3 view .LVU779
1048:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2621              		.loc 1 1048 3 view .LVU780
 2622              	.LBB390:
 2623              	.LBI390:
2832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2624              		.loc 2 2832 26 view .LVU781
 2625              	.LBB391:
2834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2626              		.loc 2 2834 3 view .LVU782
2834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2627              		.loc 2 2834 21 is_stmt 0 view .LVU783
 2628 0002 0B4B     		ldr	r3, .L200
 2629 0004 D3F89030 		ldr	r3, [r3, #144]
 2630              	.LVL236:
2834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2631              		.loc 2 2834 21 view .LVU784
 2632              	.LBE391:
 2633              	.LBE390:
1048:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2634              		.loc 1 1048 3 discriminator 1 view .LVU785
 2635 0008 1842     		tst	r0, r3
 2636 000a 08D1     		bne	.L196
1051:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2637              		.loc 1 1051 7 is_stmt 1 view .LVU786
 2638              	.LBB392:
 2639              	.LBI392:
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2640              		.loc 2 3153 26 view .LVU787
 2641              	.LBB393:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2642              		.loc 2 3155 3 view .LVU788
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2643              		.loc 2 3155 11 is_stmt 0 view .LVU789
 2644 000c 084B     		ldr	r3, .L200
 2645 000e 1868     		ldr	r0, [r3]
 2646              	.LVL237:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2647              		.loc 2 3155 11 view .LVU790
 2648              	.LBE393:
 2649              	.LBE392:
1051:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
ARM GAS  /tmp/cc42qbQx.s 			page 165


 2650              		.loc 1 1051 10 discriminator 1 view .LVU791
 2651 0010 10F00070 		ands	r0, r0, #33554432
 2652 0014 00D1     		bne	.L199
 2653              	.LVL238:
 2654              	.L195:
1067:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2655              		.loc 1 1067 1 view .LVU792
 2656 0016 08BD     		pop	{r3, pc}
 2657              	.LVL239:
 2658              	.L199:
1053:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2659              		.loc 1 1053 9 is_stmt 1 view .LVU793
1053:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2660              		.loc 1 1053 25 is_stmt 0 view .LVU794
 2661 0018 FFF7FEFF 		bl	RCC_PLL_GetFreqDomain_48M
 2662              	.LVL240:
1053:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2663              		.loc 1 1053 25 view .LVU795
 2664 001c FBE7     		b	.L195
 2665              	.LVL241:
 2666              	.L196:
1059:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2667              		.loc 1 1059 7 is_stmt 1 view .LVU796
 2668              	.LBB394:
 2669              	.LBI394:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2670              		.loc 2 4179 26 view .LVU797
 2671              	.LBB395:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2672              		.loc 2 4181 3 view .LVU798
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2673              		.loc 2 4181 11 is_stmt 0 view .LVU799
 2674 001e 044B     		ldr	r3, .L200
 2675 0020 1868     		ldr	r0, [r3]
 2676              	.LVL242:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2677              		.loc 2 4181 11 view .LVU800
 2678              	.LBE395:
 2679              	.LBE394:
1059:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 2680              		.loc 1 1059 10 discriminator 1 view .LVU801
 2681 0022 10F00050 		ands	r0, r0, #536870912
 2682 0026 F6D0     		beq	.L195
1061:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2683              		.loc 1 1061 9 is_stmt 1 view .LVU802
1061:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       }
 2684              		.loc 1 1061 25 is_stmt 0 view .LVU803
 2685 0028 FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_48M
 2686              	.LVL243:
1066:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2687              		.loc 1 1066 3 is_stmt 1 view .LVU804
1066:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2688              		.loc 1 1066 10 is_stmt 0 view .LVU805
 2689 002c F3E7     		b	.L195
 2690              	.L201:
 2691 002e 00BF     		.align	2
 2692              	.L200:
ARM GAS  /tmp/cc42qbQx.s 			page 166


 2693 0030 00380240 		.word	1073887232
 2694              		.cfi_endproc
 2695              	.LFE306:
 2697              		.section	.text.RCC_PLLSAI_GetFreqDomain_LTDC,"ax",%progbits
 2698              		.align	1
 2699              		.global	RCC_PLLSAI_GetFreqDomain_LTDC
 2700              		.syntax unified
 2701              		.thumb
 2702              		.thumb_func
 2704              	RCC_PLLSAI_GetFreqDomain_LTDC:
 2705              	.LFB319:
1443:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1444:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(LTDC)
1445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1446:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLSAI clock frequency used for LTDC domain
1447:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLSAI clock frequency (in Hz)
1448:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1449:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLSAI_GetFreqDomain_LTDC(void)
1450:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 2706              		.loc 1 1450 1 is_stmt 1 view -0
 2707              		.cfi_startproc
 2708              		@ args = 0, pretend = 0, frame = 0
 2709              		@ frame_needed = 0, uses_anonymous_args = 0
 2710              		@ link register save eliminated.
1451:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 2711              		.loc 1 1451 3 view .LVU807
 2712              	.LVL244:
1452:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLSAI_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLSAIN
1454:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      LTDC Domain clock  = (PLLSAI_VCO / PLLSAIR) / PLLSAIDIVR
1455:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1456:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 2713              		.loc 1 1456 3 view .LVU808
 2714              	.LBB396:
 2715              	.LBI396:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2716              		.loc 2 3461 26 view .LVU809
 2717              	.LBB397:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2718              		.loc 2 3463 3 view .LVU810
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2719              		.loc 2 3463 21 is_stmt 0 view .LVU811
 2720 0000 114B     		ldr	r3, .L205
 2721 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2722              		.loc 2 3463 10 view .LVU812
 2723 0004 03F48003 		and	r3, r3, #4194304
 2724              	.LVL245:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2725              		.loc 2 3463 10 view .LVU813
 2726              	.LBE397:
 2727              	.LBE396:
1457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1458:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 2728              		.loc 1 1458 3 is_stmt 1 view .LVU814
 2729 0008 DBB9     		cbnz	r3, .L204
1459:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
ARM GAS  /tmp/cc42qbQx.s 			page 167


1460:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLSAI clock source */
1461:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 2730              		.loc 1 1461 20 is_stmt 0 view .LVU815
 2731 000a 1048     		ldr	r0, .L205+4
 2732              	.L203:
 2733              	.LVL246:
1462:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1463:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1464:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLSAI clock source */
1465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1466:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1467:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1468:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1470:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1471:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1472:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLSAI_LTDC_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 2734              		.loc 1 1472 3 is_stmt 1 view .LVU816
 2735              	.LBB398:
 2736              	.LBI398:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2737              		.loc 2 3601 26 view .LVU817
 2738              	.LBB399:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2739              		.loc 2 3603 3 view .LVU818
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2740              		.loc 2 3603 21 is_stmt 0 view .LVU819
 2741 000c 0E4A     		ldr	r2, .L205
 2742 000e 5368     		ldr	r3, [r2, #4]
 2743              	.LVL247:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2744              		.loc 2 3603 10 view .LVU820
 2745 0010 03F03F03 		and	r3, r3, #63
 2746              	.LBE399:
 2747              	.LBE398:
 2748              		.loc 1 1472 10 discriminator 1 view .LVU821
 2749 0014 B0FBF3F0 		udiv	r0, r0, r3
 2750              	.LVL248:
 2751              	.LBB400:
 2752              	.LBI400:
4515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2753              		.loc 2 4515 26 is_stmt 1 view .LVU822
 2754              	.LBB401:
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2755              		.loc 2 4517 3 view .LVU823
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2756              		.loc 2 4517 21 is_stmt 0 view .LVU824
 2757 0018 D2F88830 		ldr	r3, [r2, #136]
4517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2758              		.loc 2 4517 10 view .LVU825
 2759 001c C3F38813 		ubfx	r3, r3, #6, #9
 2760              	.LBE401:
 2761              	.LBE400:
 2762              		.loc 1 1472 10 discriminator 2 view .LVU826
 2763 0020 03FB00F0 		mul	r0, r3, r0
 2764              	.LBB402:
 2765              	.LBI402:
ARM GAS  /tmp/cc42qbQx.s 			page 168


4557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2766              		.loc 2 4557 26 is_stmt 1 view .LVU827
 2767              	.LBB403:
4559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2768              		.loc 2 4559 3 view .LVU828
4559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2769              		.loc 2 4559 21 is_stmt 0 view .LVU829
 2770 0024 D2F88830 		ldr	r3, [r2, #136]
 2771              	.LBE403:
 2772              	.LBE402:
 2773              		.loc 1 1472 10 discriminator 3 view .LVU830
 2774 0028 C3F30273 		ubfx	r3, r3, #28, #3
 2775              	.LBB404:
 2776              	.LBI404:
4619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_DCKCFGR1_PLLSAIDIVR)
4622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIPLL division factor for PLLSAIDIVR
4624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for LTDC domain clock
4625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1  PLLSAIDIVR      LL_RCC_PLLSAI_GetDIVR
4626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_2
4628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_4
4629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_8
4630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_16
4631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_GetDIVR(void)
 2777              		.loc 2 4632 26 is_stmt 1 view .LVU831
 2778              	.LBB405:
4633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLSAIDIVR));
 2779              		.loc 2 4634 3 view .LVU832
 2780              		.loc 2 4634 21 is_stmt 0 view .LVU833
 2781 002c D2F88C20 		ldr	r2, [r2, #140]
 2782              	.LBE405:
 2783              	.LBE404:
 2784              		.loc 1 1472 10 discriminator 4 view .LVU834
 2785 0030 C2F30142 		ubfx	r2, r2, #16, #2
 2786 0034 0649     		ldr	r1, .L205+8
 2787 0036 8A5C     		ldrb	r2, [r1, r2]	@ zero_extendqisi2
 2788 0038 02FB03F3 		mul	r3, r2, r3
1473:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLSAI_GetN(), LL_RCC_PLLSAI_GetR(), LL_RCC_PLLSAI_G
1474:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2789              		.loc 1 1474 1 view .LVU835
 2790 003c B0FBF3F0 		udiv	r0, r0, r3
 2791 0040 7047     		bx	lr
 2792              	.LVL249:
 2793              	.L204:
1465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2794              		.loc 1 1465 20 view .LVU836
 2795 0042 0448     		ldr	r0, .L205+12
 2796 0044 E2E7     		b	.L203
 2797              	.L206:
 2798 0046 00BF     		.align	2
 2799              	.L205:
 2800 0048 00380240 		.word	1073887232
ARM GAS  /tmp/cc42qbQx.s 			page 169


 2801 004c 0024F400 		.word	16000000
 2802 0050 00000000 		.word	aRCC_PLLSAIDIVRPrescTable
 2803 0054 40787D01 		.word	25000000
 2804              		.cfi_endproc
 2805              	.LFE319:
 2807              		.section	.text.LL_RCC_GetLTDCClockFreq,"ax",%progbits
 2808              		.align	1
 2809              		.global	LL_RCC_GetLTDCClockFreq
 2810              		.syntax unified
 2811              		.thumb
 2812              		.thumb_func
 2814              	LL_RCC_GetLTDCClockFreq:
 2815              	.LVL250:
 2816              	.LFB309:
1175:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t ltdc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2817              		.loc 1 1175 1 is_stmt 1 view -0
 2818              		.cfi_startproc
 2819              		@ args = 0, pretend = 0, frame = 0
 2820              		@ frame_needed = 0, uses_anonymous_args = 0
1175:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t ltdc_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2821              		.loc 1 1175 1 is_stmt 0 view .LVU838
 2822 0000 08B5     		push	{r3, lr}
 2823              	.LCFI12:
 2824              		.cfi_def_cfa_offset 8
 2825              		.cfi_offset 3, -8
 2826              		.cfi_offset 14, -4
1176:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2827              		.loc 1 1176 3 is_stmt 1 view .LVU839
 2828              	.LVL251:
1179:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2829              		.loc 1 1179 3 view .LVU840
1181:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2830              		.loc 1 1181 3 view .LVU841
 2831              	.LBB406:
 2832              	.LBI406:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2833              		.loc 2 4179 26 view .LVU842
 2834              	.LBB407:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2835              		.loc 2 4181 3 view .LVU843
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2836              		.loc 2 4181 11 is_stmt 0 view .LVU844
 2837 0002 044B     		ldr	r3, .L211
 2838 0004 1868     		ldr	r0, [r3]
 2839              	.LVL252:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2840              		.loc 2 4181 11 view .LVU845
 2841              	.LBE407:
 2842              	.LBE406:
1181:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2843              		.loc 1 1181 6 discriminator 1 view .LVU846
 2844 0006 10F00050 		ands	r0, r0, #536870912
 2845 000a 00D1     		bne	.L210
 2846              	.LVL253:
 2847              	.L207:
1187:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* LTDC */
 2848              		.loc 1 1187 1 view .LVU847
ARM GAS  /tmp/cc42qbQx.s 			page 170


 2849 000c 08BD     		pop	{r3, pc}
 2850              	.LVL254:
 2851              	.L210:
1183:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 2852              		.loc 1 1183 6 is_stmt 1 view .LVU848
1183:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 2853              		.loc 1 1183 23 is_stmt 0 view .LVU849
 2854 000e FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_LTDC
 2855              	.LVL255:
1186:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2856              		.loc 1 1186 3 is_stmt 1 view .LVU850
1186:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2857              		.loc 1 1186 10 is_stmt 0 view .LVU851
 2858 0012 FBE7     		b	.L207
 2859              	.L212:
 2860              		.align	2
 2861              	.L211:
 2862 0014 00380240 		.word	1073887232
 2863              		.cfi_endproc
 2864              	.LFE309:
 2866              		.section	.text.RCC_PLLI2S_GetFreqDomain_SAI,"ax",%progbits
 2867              		.align	1
 2868              		.global	RCC_PLLI2S_GetFreqDomain_SAI
 2869              		.syntax unified
 2870              		.thumb
 2871              		.thumb_func
 2873              	RCC_PLLI2S_GetFreqDomain_SAI:
 2874              	.LFB320:
1475:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* LTDC */
1476:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1477:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1478:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLI2S clock frequency used for SAI1 and SAI2 domains
1479:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLI2S clock frequency (in Hz)
1480:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1481:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_SAI(void)
1482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 2875              		.loc 1 1482 1 is_stmt 1 view -0
 2876              		.cfi_startproc
 2877              		@ args = 0, pretend = 0, frame = 0
 2878              		@ frame_needed = 0, uses_anonymous_args = 0
 2879              		@ link register save eliminated.
1483:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 2880              		.loc 1 1483 3 view .LVU853
 2881              	.LVL256:
1484:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1485:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLI2S_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLI2SN
1486:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      SAI1 and SAI2 domains clock  = (PLLI2S_VCO / PLLI2SQ) / PLLI2SDIVQ
1487:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1488:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 2882              		.loc 1 1488 3 view .LVU854
 2883              	.LBB408:
 2884              	.LBI408:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2885              		.loc 2 3461 26 view .LVU855
 2886              	.LBB409:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2887              		.loc 2 3463 3 view .LVU856
ARM GAS  /tmp/cc42qbQx.s 			page 171


3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2888              		.loc 2 3463 21 is_stmt 0 view .LVU857
 2889 0000 104B     		ldr	r3, .L216
 2890 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2891              		.loc 2 3463 10 view .LVU858
 2892 0004 03F48003 		and	r3, r3, #4194304
 2893              	.LVL257:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2894              		.loc 2 3463 10 view .LVU859
 2895              	.LBE409:
 2896              	.LBE408:
1489:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1490:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 2897              		.loc 1 1490 3 is_stmt 1 view .LVU860
 2898 0008 CBB9     		cbnz	r3, .L215
1491:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLI2S clock source */
1493:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 2899              		.loc 1 1493 20 is_stmt 0 view .LVU861
 2900 000a 0F48     		ldr	r0, .L216+4
 2901              	.L214:
 2902              	.LVL258:
1494:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1496:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLI2S clock source */
1497:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1499:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1500:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1501:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1502:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLI2S_SAI_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 2903              		.loc 1 1504 3 is_stmt 1 view .LVU862
 2904              	.LBB410:
 2905              	.LBI410:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2906              		.loc 2 3601 26 view .LVU863
 2907              	.LBB411:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2908              		.loc 2 3603 3 view .LVU864
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2909              		.loc 2 3603 21 is_stmt 0 view .LVU865
 2910 000c 0D4A     		ldr	r2, .L216
 2911 000e 5368     		ldr	r3, [r2, #4]
 2912              	.LVL259:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2913              		.loc 2 3603 10 view .LVU866
 2914 0010 03F03F03 		and	r3, r3, #63
 2915              	.LBE411:
 2916              	.LBE410:
 2917              		.loc 1 1504 10 discriminator 1 view .LVU867
 2918 0014 B0FBF3F0 		udiv	r0, r0, r3
 2919              	.LVL260:
 2920              	.LBB412:
 2921              	.LBI412:
ARM GAS  /tmp/cc42qbQx.s 			page 172


4040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2922              		.loc 2 4040 26 is_stmt 1 view .LVU868
 2923              	.LBB413:
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2924              		.loc 2 4042 3 view .LVU869
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2925              		.loc 2 4042 21 is_stmt 0 view .LVU870
 2926 0018 D2F88430 		ldr	r3, [r2, #132]
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2927              		.loc 2 4042 10 view .LVU871
 2928 001c C3F38813 		ubfx	r3, r3, #6, #9
 2929              	.LBE413:
 2930              	.LBE412:
 2931              		.loc 1 1504 10 discriminator 2 view .LVU872
 2932 0020 03FB00F0 		mul	r0, r3, r0
 2933              	.LBB414:
 2934              	.LBI414:
4064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2935              		.loc 2 4064 26 is_stmt 1 view .LVU873
 2936              	.LBB415:
4066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2937              		.loc 2 4066 3 view .LVU874
4066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2938              		.loc 2 4066 21 is_stmt 0 view .LVU875
 2939 0024 D2F88430 		ldr	r3, [r2, #132]
 2940              	.LBE415:
 2941              	.LBE414:
 2942              		.loc 1 1504 10 discriminator 3 view .LVU876
 2943 0028 C3F30363 		ubfx	r3, r3, #24, #4
 2944              	.LBB416:
 2945              	.LBI416:
4141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 2946              		.loc 2 4141 26 is_stmt 1 view .LVU877
 2947              	.LBB417:
4143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2948              		.loc 2 4143 3 view .LVU878
4143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2949              		.loc 2 4143 21 is_stmt 0 view .LVU879
 2950 002c D2F88C20 		ldr	r2, [r2, #140]
4143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 2951              		.loc 2 4143 10 view .LVU880
 2952 0030 02F01F02 		and	r2, r2, #31
 2953              	.LBE417:
 2954              	.LBE416:
 2955              		.loc 1 1504 10 discriminator 4 view .LVU881
 2956 0034 02FB0333 		mla	r3, r2, r3, r3
1505:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLI2S_GetN(), LL_RCC_PLLI2S_GetQ(), LL_RCC_PLLI2S_G
1506:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 2957              		.loc 1 1506 1 view .LVU882
 2958 0038 B0FBF3F0 		udiv	r0, r0, r3
 2959 003c 7047     		bx	lr
 2960              	.LVL261:
 2961              	.L215:
1497:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 2962              		.loc 1 1497 20 view .LVU883
 2963 003e 0348     		ldr	r0, .L216+8
 2964 0040 E4E7     		b	.L214
ARM GAS  /tmp/cc42qbQx.s 			page 173


 2965              	.L217:
 2966 0042 00BF     		.align	2
 2967              	.L216:
 2968 0044 00380240 		.word	1073887232
 2969 0048 0024F400 		.word	16000000
 2970 004c 40787D01 		.word	25000000
 2971              		.cfi_endproc
 2972              	.LFE320:
 2974              		.section	.text.LL_RCC_GetSAIClockFreq,"ax",%progbits
 2975              		.align	1
 2976              		.global	LL_RCC_GetSAIClockFreq
 2977              		.syntax unified
 2978              		.thumb
 2979              		.thumb_func
 2981              	LL_RCC_GetSAIClockFreq:
 2982              	.LVL262:
 2983              	.LFB302:
 766:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sai_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2984              		.loc 1 766 1 is_stmt 1 view -0
 2985              		.cfi_startproc
 2986              		@ args = 0, pretend = 0, frame = 0
 2987              		@ frame_needed = 0, uses_anonymous_args = 0
 766:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t sai_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 2988              		.loc 1 766 1 is_stmt 0 view .LVU885
 2989 0000 08B5     		push	{r3, lr}
 2990              	.LCFI13:
 2991              		.cfi_def_cfa_offset 8
 2992              		.cfi_offset 3, -8
 2993              		.cfi_offset 14, -4
 767:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2994              		.loc 1 767 3 is_stmt 1 view .LVU886
 2995              	.LVL263:
 770:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 2996              		.loc 1 770 3 view .LVU887
 772:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2997              		.loc 1 772 3 view .LVU888
 772:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 2998              		.loc 1 772 6 is_stmt 0 view .LVU889
 2999 0002 B0F5401F 		cmp	r0, #3145728
 3000 0006 04D0     		beq	.L239
 822:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3001              		.loc 1 822 5 is_stmt 1 view .LVU890
 822:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3002              		.loc 1 822 8 is_stmt 0 view .LVU891
 3003 0008 B0F5400F 		cmp	r0, #12582912
 3004 000c 3BD0     		beq	.L240
 767:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3005              		.loc 1 767 12 view .LVU892
 3006 000e 0020     		movs	r0, #0
 3007              	.LVL264:
 3008              	.L218:
 873:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3009              		.loc 1 873 1 view .LVU893
 3010 0010 08BD     		pop	{r3, pc}
 3011              	.LVL265:
 3012              	.L239:
 775:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
ARM GAS  /tmp/cc42qbQx.s 			page 174


 3013              		.loc 1 775 5 is_stmt 1 view .LVU894
 3014              	.LBB418:
 3015              	.LBI418:
2770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3016              		.loc 2 2770 26 view .LVU895
 3017              	.LBB419:
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3018              		.loc 2 2772 3 view .LVU896
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3019              		.loc 2 2772 21 is_stmt 0 view .LVU897
 3020 0012 3D4B     		ldr	r3, .L245
 3021 0014 D3F88C30 		ldr	r3, [r3, #140]
 3022 0018 0340     		ands	r3, r3, r0
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3023              		.loc 2 2772 10 view .LVU898
 3024 001a 40EA1340 		orr	r0, r0, r3, lsr #16
 3025              	.LVL266:
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3026              		.loc 2 2772 10 view .LVU899
 3027              	.LBE419:
 3028              	.LBE418:
 775:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3029              		.loc 1 775 5 discriminator 1 view .LVU900
 3030 001e 3B4B     		ldr	r3, .L245+4
 3031 0020 9842     		cmp	r0, r3
 3032 0022 6AD0     		beq	.L231
 3033 0024 0FD8     		bhi	.L221
 3034 0026 B0F5401F 		cmp	r0, #3145728
 3035 002a 1DD0     		beq	.L222
 3036 002c 103B     		subs	r3, r3, #16
 3037 002e 9842     		cmp	r0, r3
 3038 0030 07D1     		bne	.L241
 785:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3039              		.loc 1 785 9 is_stmt 1 view .LVU901
 3040              	.LBB420:
 3041              	.LBI420:
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3042              		.loc 2 3711 26 view .LVU902
 3043              	.LBB421:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3044              		.loc 2 3713 3 view .LVU903
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3045              		.loc 2 3713 11 is_stmt 0 view .LVU904
 3046 0032 354B     		ldr	r3, .L245
 3047 0034 1868     		ldr	r0, [r3]
 3048              	.LBE421:
 3049              	.LBE420:
 785:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3050              		.loc 1 785 12 discriminator 1 view .LVU905
 3051 0036 10F00060 		ands	r0, r0, #134217728
 3052 003a E9D0     		beq	.L218
 787:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3053              		.loc 1 787 11 is_stmt 1 view .LVU906
 787:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3054              		.loc 1 787 27 is_stmt 0 view .LVU907
 3055 003c FFF7FEFF 		bl	RCC_PLLI2S_GetFreqDomain_SAI
 3056              	.LVL267:
ARM GAS  /tmp/cc42qbQx.s 			page 175


 787:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3057              		.loc 1 787 27 view .LVU908
 3058 0040 E6E7     		b	.L218
 3059              	.LVL268:
 3060              	.L241:
 775:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3061              		.loc 1 775 5 discriminator 1 view .LVU909
 3062 0042 0020     		movs	r0, #0
 3063 0044 E4E7     		b	.L218
 3064              	.L221:
 3065 0046 B0F1301F 		cmp	r0, #3145776
 3066 004a 0BD1     		bne	.L242
 793:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3067              		.loc 1 793 9 is_stmt 1 view .LVU910
 3068              	.LBB422:
 3069              	.LBI422:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3070              		.loc 2 3461 26 view .LVU911
 3071              	.LBB423:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3072              		.loc 2 3463 3 view .LVU912
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3073              		.loc 2 3463 21 is_stmt 0 view .LVU913
 3074 004c 2E4B     		ldr	r3, .L245
 3075 004e 5B68     		ldr	r3, [r3, #4]
 3076              	.LBE423:
 3077              	.LBE422:
 3078 0050 13F4800F 		tst	r3, #4194304
 3079 0054 10D0     		beq	.L225
 796:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3080              		.loc 1 796 14 is_stmt 1 view .LVU914
 3081              	.LBB424:
 3082              	.LBI424:
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3083              		.loc 2 1992 26 view .LVU915
 3084              	.LBB425:
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3085              		.loc 2 1994 3 view .LVU916
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3086              		.loc 2 1994 11 is_stmt 0 view .LVU917
 3087 0056 2C4B     		ldr	r3, .L245
 3088 0058 1868     		ldr	r0, [r3]
 3089              	.LBE425:
 3090              	.LBE424:
 796:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3091              		.loc 1 796 17 discriminator 1 view .LVU918
 3092 005a 10F40030 		ands	r0, r0, #131072
 3093 005e D7D0     		beq	.L218
 798:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 3094              		.loc 1 798 30 view .LVU919
 3095 0060 2B48     		ldr	r0, .L245+8
 3096 0062 D5E7     		b	.L218
 3097              	.L242:
 775:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3098              		.loc 1 775 5 discriminator 1 view .LVU920
 3099 0064 0020     		movs	r0, #0
 3100 0066 D3E7     		b	.L218
ARM GAS  /tmp/cc42qbQx.s 			page 176


 3101              	.L222:
 778:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3102              		.loc 1 778 9 is_stmt 1 view .LVU921
 3103              	.LBB426:
 3104              	.LBI426:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3105              		.loc 2 4179 26 view .LVU922
 3106              	.LBB427:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3107              		.loc 2 4181 3 view .LVU923
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3108              		.loc 2 4181 11 is_stmt 0 view .LVU924
 3109 0068 274B     		ldr	r3, .L245
 3110 006a 1868     		ldr	r0, [r3]
 3111              	.LBE427:
 3112              	.LBE426:
 778:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3113              		.loc 1 778 12 discriminator 1 view .LVU925
 3114 006c 10F00050 		ands	r0, r0, #536870912
 3115 0070 CED0     		beq	.L218
 780:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3116              		.loc 1 780 11 is_stmt 1 view .LVU926
 780:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3117              		.loc 1 780 27 is_stmt 0 view .LVU927
 3118 0072 FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_SAI
 3119              	.LVL269:
 780:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3120              		.loc 1 780 27 view .LVU928
 3121 0076 CBE7     		b	.L218
 3122              	.LVL270:
 3123              	.L225:
 804:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3124              		.loc 1 804 14 is_stmt 1 view .LVU929
 3125              	.LBB428:
 3126              	.LBI428:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3127              		.loc 2 2030 26 view .LVU930
 3128              	.LBB429:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3129              		.loc 2 2032 3 view .LVU931
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3130              		.loc 2 2032 11 is_stmt 0 view .LVU932
 3131 0078 234B     		ldr	r3, .L245
 3132 007a 1868     		ldr	r0, [r3]
 3133              	.LBE429:
 3134              	.LBE428:
 804:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3135              		.loc 1 804 17 discriminator 1 view .LVU933
 3136 007c 10F00200 		ands	r0, r0, #2
 3137 0080 C6D0     		beq	.L218
 806:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 3138              		.loc 1 806 30 view .LVU934
 3139 0082 2448     		ldr	r0, .L245+12
 3140 0084 C4E7     		b	.L218
 3141              	.LVL271:
 3142              	.L240:
 825:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
ARM GAS  /tmp/cc42qbQx.s 			page 177


 3143              		.loc 1 825 7 is_stmt 1 view .LVU935
 3144              	.LBB430:
 3145              	.LBI430:
2770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3146              		.loc 2 2770 26 view .LVU936
 3147              	.LBB431:
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3148              		.loc 2 2772 3 view .LVU937
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3149              		.loc 2 2772 21 is_stmt 0 view .LVU938
 3150 0086 204B     		ldr	r3, .L245
 3151 0088 D3F88C30 		ldr	r3, [r3, #140]
 3152 008c 0340     		ands	r3, r3, r0
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3153              		.loc 2 2772 10 view .LVU939
 3154 008e 40EA1340 		orr	r0, r0, r3, lsr #16
 3155              	.LVL272:
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3156              		.loc 2 2772 10 view .LVU940
 3157              	.LBE431:
 3158              	.LBE430:
 825:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 3159              		.loc 1 825 7 discriminator 1 view .LVU941
 3160 0092 214B     		ldr	r3, .L245+16
 3161 0094 9842     		cmp	r0, r3
 3162 0096 33D0     		beq	.L235
 3163 0098 0FD8     		bhi	.L226
 3164 009a B0F5400F 		cmp	r0, #12582912
 3165 009e 1DD0     		beq	.L227
 3166 00a0 403B     		subs	r3, r3, #64
 3167 00a2 9842     		cmp	r0, r3
 3168 00a4 07D1     		bne	.L243
 835:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3169              		.loc 1 835 9 is_stmt 1 view .LVU942
 3170              	.LBB432:
 3171              	.LBI432:
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3172              		.loc 2 3711 26 view .LVU943
 3173              	.LBB433:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3174              		.loc 2 3713 3 view .LVU944
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3175              		.loc 2 3713 11 is_stmt 0 view .LVU945
 3176 00a6 184B     		ldr	r3, .L245
 3177 00a8 1868     		ldr	r0, [r3]
 3178              	.LBE433:
 3179              	.LBE432:
 835:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3180              		.loc 1 835 12 discriminator 1 view .LVU946
 3181 00aa 10F00060 		ands	r0, r0, #134217728
 3182 00ae AFD0     		beq	.L218
 837:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3183              		.loc 1 837 11 is_stmt 1 view .LVU947
 837:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3184              		.loc 1 837 27 is_stmt 0 view .LVU948
 3185 00b0 FFF7FEFF 		bl	RCC_PLLI2S_GetFreqDomain_SAI
 3186              	.LVL273:
ARM GAS  /tmp/cc42qbQx.s 			page 178


 837:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3187              		.loc 1 837 27 view .LVU949
 3188 00b4 ACE7     		b	.L218
 3189              	.LVL274:
 3190              	.L243:
 825:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 3191              		.loc 1 825 7 discriminator 1 view .LVU950
 3192 00b6 0020     		movs	r0, #0
 3193 00b8 AAE7     		b	.L218
 3194              	.L226:
 3195 00ba B0F1C01F 		cmp	r0, #12583104
 3196 00be 0BD1     		bne	.L244
 843:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3197              		.loc 1 843 9 is_stmt 1 view .LVU951
 3198              	.LBB434:
 3199              	.LBI434:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3200              		.loc 2 3461 26 view .LVU952
 3201              	.LBB435:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3202              		.loc 2 3463 3 view .LVU953
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3203              		.loc 2 3463 21 is_stmt 0 view .LVU954
 3204 00c0 114B     		ldr	r3, .L245
 3205 00c2 5B68     		ldr	r3, [r3, #4]
 3206              	.LBE435:
 3207              	.LBE434:
 3208 00c4 13F4800F 		tst	r3, #4194304
 3209 00c8 10D0     		beq	.L230
 846:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3210              		.loc 1 846 14 is_stmt 1 view .LVU955
 3211              	.LBB436:
 3212              	.LBI436:
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3213              		.loc 2 1992 26 view .LVU956
 3214              	.LBB437:
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3215              		.loc 2 1994 3 view .LVU957
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3216              		.loc 2 1994 11 is_stmt 0 view .LVU958
 3217 00ca 0F4B     		ldr	r3, .L245
 3218 00cc 1868     		ldr	r0, [r3]
 3219              	.LBE437:
 3220              	.LBE436:
 846:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3221              		.loc 1 846 17 discriminator 1 view .LVU959
 3222 00ce 10F40030 		ands	r0, r0, #131072
 3223 00d2 9DD0     		beq	.L218
 848:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 3224              		.loc 1 848 30 view .LVU960
 3225 00d4 0E48     		ldr	r0, .L245+8
 3226 00d6 9BE7     		b	.L218
 3227              	.L244:
 825:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       {
 3228              		.loc 1 825 7 discriminator 1 view .LVU961
 3229 00d8 0020     		movs	r0, #0
 3230 00da 99E7     		b	.L218
ARM GAS  /tmp/cc42qbQx.s 			page 179


 3231              	.L227:
 828:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3232              		.loc 1 828 9 is_stmt 1 view .LVU962
 3233              	.LBB438:
 3234              	.LBI438:
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3235              		.loc 2 4179 26 view .LVU963
 3236              	.LBB439:
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3237              		.loc 2 4181 3 view .LVU964
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3238              		.loc 2 4181 11 is_stmt 0 view .LVU965
 3239 00dc 0A4B     		ldr	r3, .L245
 3240 00de 1868     		ldr	r0, [r3]
 3241              	.LBE439:
 3242              	.LBE438:
 828:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3243              		.loc 1 828 12 discriminator 1 view .LVU966
 3244 00e0 10F00050 		ands	r0, r0, #536870912
 3245 00e4 94D0     		beq	.L218
 830:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3246              		.loc 1 830 11 is_stmt 1 view .LVU967
 830:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3247              		.loc 1 830 27 is_stmt 0 view .LVU968
 3248 00e6 FFF7FEFF 		bl	RCC_PLLSAI_GetFreqDomain_SAI
 3249              	.LVL275:
 830:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3250              		.loc 1 830 27 view .LVU969
 3251 00ea 91E7     		b	.L218
 3252              	.LVL276:
 3253              	.L230:
 854:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3254              		.loc 1 854 14 is_stmt 1 view .LVU970
 3255              	.LBB440:
 3256              	.LBI440:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3257              		.loc 2 2030 26 view .LVU971
 3258              	.LBB441:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3259              		.loc 2 2032 3 view .LVU972
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3260              		.loc 2 2032 11 is_stmt 0 view .LVU973
 3261 00ec 064B     		ldr	r3, .L245
 3262 00ee 1868     		ldr	r0, [r3]
 3263              	.LBE441:
 3264              	.LBE440:
 854:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              {
 3265              		.loc 1 854 17 discriminator 1 view .LVU974
 3266 00f0 10F00200 		ands	r0, r0, #2
 3267 00f4 8CD0     		beq	.L218
 856:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****              }
 3268              		.loc 1 856 30 view .LVU975
 3269 00f6 0748     		ldr	r0, .L245+12
 3270              	.LVL277:
 872:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3271              		.loc 1 872 3 is_stmt 1 view .LVU976
 872:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
ARM GAS  /tmp/cc42qbQx.s 			page 180


 3272              		.loc 1 872 10 is_stmt 0 view .LVU977
 3273 00f8 8AE7     		b	.L218
 3274              	.LVL278:
 3275              	.L231:
 813:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 3276              		.loc 1 813 23 view .LVU978
 3277 00fa 4BF68030 		movw	r0, #48000
 3278 00fe 87E7     		b	.L218
 3279              	.L235:
 863:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****           break;
 3280              		.loc 1 863 25 view .LVU979
 3281 0100 4BF68030 		movw	r0, #48000
 3282 0104 84E7     		b	.L218
 3283              	.L246:
 3284 0106 00BF     		.align	2
 3285              	.L245:
 3286 0108 00380240 		.word	1073887232
 3287 010c 20003000 		.word	3145760
 3288 0110 40787D01 		.word	25000000
 3289 0114 0024F400 		.word	16000000
 3290 0118 8000C000 		.word	12583040
 3291              		.cfi_endproc
 3292              	.LFE302:
 3294              		.section	.text.LL_RCC_GetDFSDMAudioClockFreq,"ax",%progbits
 3295              		.align	1
 3296              		.global	LL_RCC_GetDFSDMAudioClockFreq
 3297              		.syntax unified
 3298              		.thumb
 3299              		.thumb_func
 3301              	LL_RCC_GetDFSDMAudioClockFreq:
 3302              	.LVL279:
 3303              	.LFB308:
1107:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3304              		.loc 1 1107 1 is_stmt 1 view -0
 3305              		.cfi_startproc
 3306              		@ args = 0, pretend = 0, frame = 0
 3307              		@ frame_needed = 0, uses_anonymous_args = 0
1107:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t dfsdm_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3308              		.loc 1 1107 1 is_stmt 0 view .LVU981
 3309 0000 08B5     		push	{r3, lr}
 3310              	.LCFI14:
 3311              		.cfi_def_cfa_offset 8
 3312              		.cfi_offset 3, -8
 3313              		.cfi_offset 14, -4
1108:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3314              		.loc 1 1108 3 is_stmt 1 view .LVU982
 3315              	.LVL280:
1111:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3316              		.loc 1 1111 3 view .LVU983
1114:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3317              		.loc 1 1114 3 view .LVU984
 3318              	.LBB442:
 3319              	.LBI442:
2877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3320              		.loc 2 2877 26 view .LVU985
 3321              	.LBB443:
2879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/cc42qbQx.s 			page 181


 3322              		.loc 2 2879 3 view .LVU986
2879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3323              		.loc 2 2879 21 is_stmt 0 view .LVU987
 3324 0002 074B     		ldr	r3, .L251
 3325 0004 D3F88C30 		ldr	r3, [r3, #140]
 3326              	.LVL281:
2879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3327              		.loc 2 2879 21 view .LVU988
 3328              	.LBE443:
 3329              	.LBE442:
1114:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3330              		.loc 1 1114 3 discriminator 1 view .LVU989
 3331 0008 1842     		tst	r0, r3
 3332 000a 04D1     		bne	.L248
1117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3333              		.loc 1 1117 7 is_stmt 1 view .LVU990
1117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3334              		.loc 1 1117 25 is_stmt 0 view .LVU991
 3335 000c 4FF44010 		mov	r0, #3145728
 3336              	.LVL282:
1117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3337              		.loc 1 1117 25 view .LVU992
 3338 0010 FFF7FEFF 		bl	LL_RCC_GetSAIClockFreq
 3339              	.LVL283:
1118:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3340              		.loc 1 1118 7 is_stmt 1 view .LVU993
 3341              	.L247:
1127:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* DFSDM1_Channel0 */
 3342              		.loc 1 1127 1 is_stmt 0 view .LVU994
 3343 0014 08BD     		pop	{r3, pc}
 3344              	.LVL284:
 3345              	.L248:
1122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3346              		.loc 1 1122 7 is_stmt 1 view .LVU995
1122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3347              		.loc 1 1122 25 is_stmt 0 view .LVU996
 3348 0016 4FF44000 		mov	r0, #12582912
 3349              	.LVL285:
1122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3350              		.loc 1 1122 25 view .LVU997
 3351 001a FFF7FEFF 		bl	LL_RCC_GetSAIClockFreq
 3352              	.LVL286:
1123:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 3353              		.loc 1 1123 7 is_stmt 1 view .LVU998
1126:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3354              		.loc 1 1126 3 view .LVU999
1126:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3355              		.loc 1 1126 10 is_stmt 0 view .LVU1000
 3356 001e F9E7     		b	.L247
 3357              	.L252:
 3358              		.align	2
 3359              	.L251:
 3360 0020 00380240 		.word	1073887232
 3361              		.cfi_endproc
 3362              	.LFE308:
 3364              		.section	.text.RCC_PLLI2S_GetFreqDomain_SPDIFRX,"ax",%progbits
 3365              		.align	1
ARM GAS  /tmp/cc42qbQx.s 			page 182


 3366              		.global	RCC_PLLI2S_GetFreqDomain_SPDIFRX
 3367              		.syntax unified
 3368              		.thumb
 3369              		.thumb_func
 3371              	RCC_PLLI2S_GetFreqDomain_SPDIFRX:
 3372              	.LFB321:
1507:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1508:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #if defined(SPDIFRX)
1509:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
1510:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLI2S clock frequency used for SPDIFRX domain
1511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLI2S clock frequency (in Hz)
1512:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1513:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_SPDIFRX(void)
1514:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 3373              		.loc 1 1514 1 is_stmt 1 view -0
 3374              		.cfi_startproc
 3375              		@ args = 0, pretend = 0, frame = 0
 3376              		@ frame_needed = 0, uses_anonymous_args = 0
 3377              		@ link register save eliminated.
1515:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 3378              		.loc 1 1515 3 view .LVU1002
 3379              	.LVL287:
1516:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1517:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLI2S_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLI2SN
1518:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      SPDIFRX Domain clock  = PLLI2S_VCO / PLLI2SP
1519:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 3380              		.loc 1 1520 3 view .LVU1003
 3381              	.LBB444:
 3382              	.LBI444:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3383              		.loc 2 3461 26 view .LVU1004
 3384              	.LBB445:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3385              		.loc 2 3463 3 view .LVU1005
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3386              		.loc 2 3463 21 is_stmt 0 view .LVU1006
 3387 0000 0E4B     		ldr	r3, .L256
 3388 0002 5B68     		ldr	r3, [r3, #4]
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3389              		.loc 2 3463 10 view .LVU1007
 3390 0004 03F48003 		and	r3, r3, #4194304
 3391              	.LVL288:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3392              		.loc 2 3463 10 view .LVU1008
 3393              	.LBE445:
 3394              	.LBE444:
1521:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1522:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 3395              		.loc 1 1522 3 is_stmt 1 view .LVU1009
 3396 0008 ABB9     		cbnz	r3, .L255
1523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1524:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLI2S clock source */
1525:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
 3397              		.loc 1 1525 20 is_stmt 0 view .LVU1010
 3398 000a 0D48     		ldr	r0, .L256+4
 3399              	.L254:
ARM GAS  /tmp/cc42qbQx.s 			page 183


 3400              	.LVL289:
1526:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1527:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1528:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLI2S clock source */
1529:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
1530:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1531:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1532:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1533:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1534:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1535:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1536:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1537:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLI2S_SPDIFRX_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 3401              		.loc 1 1537 3 is_stmt 1 view .LVU1011
 3402              	.LBB446:
 3403              	.LBI446:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3404              		.loc 2 3601 26 view .LVU1012
 3405              	.LBB447:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3406              		.loc 2 3603 3 view .LVU1013
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3407              		.loc 2 3603 21 is_stmt 0 view .LVU1014
 3408 000c 0B4B     		ldr	r3, .L256
 3409              	.LVL290:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3410              		.loc 2 3603 21 view .LVU1015
 3411 000e 5A68     		ldr	r2, [r3, #4]
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3412              		.loc 2 3603 10 view .LVU1016
 3413 0010 02F03F02 		and	r2, r2, #63
 3414              	.LBE447:
 3415              	.LBE446:
 3416              		.loc 1 1537 10 discriminator 1 view .LVU1017
 3417 0014 B0FBF2F0 		udiv	r0, r0, r2
 3418              	.LVL291:
 3419              	.LBB448:
 3420              	.LBI448:
4040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3421              		.loc 2 4040 26 is_stmt 1 view .LVU1018
 3422              	.LBB449:
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3423              		.loc 2 4042 3 view .LVU1019
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3424              		.loc 2 4042 21 is_stmt 0 view .LVU1020
 3425 0018 D3F88420 		ldr	r2, [r3, #132]
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3426              		.loc 2 4042 10 view .LVU1021
 3427 001c C2F38812 		ubfx	r2, r2, #6, #9
 3428              	.LBE449:
 3429              	.LBE448:
 3430              		.loc 1 1537 10 discriminator 2 view .LVU1022
 3431 0020 02FB00F0 		mul	r0, r2, r0
 3432              	.LBB450:
 3433              	.LBI450:
4097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3434              		.loc 2 4097 26 is_stmt 1 view .LVU1023
ARM GAS  /tmp/cc42qbQx.s 			page 184


 3435              	.LBB451:
4099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3436              		.loc 2 4099 3 view .LVU1024
4099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3437              		.loc 2 4099 21 is_stmt 0 view .LVU1025
 3438 0024 D3F88430 		ldr	r3, [r3, #132]
 3439              	.LBE451:
 3440              	.LBE450:
 3441              		.loc 1 1537 10 discriminator 3 view .LVU1026
 3442 0028 C3F30143 		ubfx	r3, r3, #16, #2
 3443 002c 0133     		adds	r3, r3, #1
 3444 002e 5B00     		lsls	r3, r3, #1
1538:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLI2S_GetN(), LL_RCC_PLLI2S_GetP());
1539:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3445              		.loc 1 1539 1 view .LVU1027
 3446 0030 B0FBF3F0 		udiv	r0, r0, r3
 3447 0034 7047     		bx	lr
 3448              	.LVL292:
 3449              	.L255:
1529:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3450              		.loc 1 1529 20 view .LVU1028
 3451 0036 0348     		ldr	r0, .L256+8
 3452 0038 E8E7     		b	.L254
 3453              	.L257:
 3454 003a 00BF     		.align	2
 3455              	.L256:
 3456 003c 00380240 		.word	1073887232
 3457 0040 0024F400 		.word	16000000
 3458 0044 40787D01 		.word	25000000
 3459              		.cfi_endproc
 3460              	.LFE321:
 3462              		.section	.text.LL_RCC_GetSPDIFRXClockFreq,"ax",%progbits
 3463              		.align	1
 3464              		.global	LL_RCC_GetSPDIFRXClockFreq
 3465              		.syntax unified
 3466              		.thumb
 3467              		.thumb_func
 3469              	LL_RCC_GetSPDIFRXClockFreq:
 3470              	.LVL293:
 3471              	.LFB310:
1199:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t spdifrx_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3472              		.loc 1 1199 1 is_stmt 1 view -0
 3473              		.cfi_startproc
 3474              		@ args = 0, pretend = 0, frame = 0
 3475              		@ frame_needed = 0, uses_anonymous_args = 0
1199:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t spdifrx_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3476              		.loc 1 1199 1 is_stmt 0 view .LVU1030
 3477 0000 08B5     		push	{r3, lr}
 3478              	.LCFI15:
 3479              		.cfi_def_cfa_offset 8
 3480              		.cfi_offset 3, -8
 3481              		.cfi_offset 14, -4
1200:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3482              		.loc 1 1200 3 is_stmt 1 view .LVU1031
 3483              	.LVL294:
1203:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3484              		.loc 1 1203 3 view .LVU1032
ARM GAS  /tmp/cc42qbQx.s 			page 185


1205:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3485              		.loc 1 1205 3 view .LVU1033
 3486              	.LBB452:
 3487              	.LBI452:
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3488              		.loc 2 3711 26 view .LVU1034
 3489              	.LBB453:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3490              		.loc 2 3713 3 view .LVU1035
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3491              		.loc 2 3713 11 is_stmt 0 view .LVU1036
 3492 0002 044B     		ldr	r3, .L262
 3493 0004 1868     		ldr	r0, [r3]
 3494              	.LVL295:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3495              		.loc 2 3713 11 view .LVU1037
 3496              	.LBE453:
 3497              	.LBE452:
1205:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3498              		.loc 1 1205 6 discriminator 1 view .LVU1038
 3499 0006 10F00060 		ands	r0, r0, #134217728
 3500 000a 00D1     		bne	.L261
 3501              	.LVL296:
 3502              	.L258:
1211:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SPDIFRX */
 3503              		.loc 1 1211 1 view .LVU1039
 3504 000c 08BD     		pop	{r3, pc}
 3505              	.LVL297:
 3506              	.L261:
1207:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 3507              		.loc 1 1207 6 is_stmt 1 view .LVU1040
1207:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
 3508              		.loc 1 1207 26 is_stmt 0 view .LVU1041
 3509 000e FFF7FEFF 		bl	RCC_PLLI2S_GetFreqDomain_SPDIFRX
 3510              	.LVL298:
1210:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3511              		.loc 1 1210 3 is_stmt 1 view .LVU1042
1210:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3512              		.loc 1 1210 10 is_stmt 0 view .LVU1043
 3513 0012 FBE7     		b	.L258
 3514              	.L263:
 3515              		.align	2
 3516              	.L262:
 3517 0014 00380240 		.word	1073887232
 3518              		.cfi_endproc
 3519              	.LFE310:
 3521              		.section	.text.RCC_PLLI2S_GetFreqDomain_I2S,"ax",%progbits
 3522              		.align	1
 3523              		.global	RCC_PLLI2S_GetFreqDomain_I2S
 3524              		.syntax unified
 3525              		.thumb
 3526              		.thumb_func
 3528              	RCC_PLLI2S_GetFreqDomain_I2S:
 3529              	.LFB322:
1540:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** #endif /* SPDIFRX */
1541:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** /**
ARM GAS  /tmp/cc42qbQx.s 			page 186


1543:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @brief  Return PLLI2S clock frequency used for I2S domain
1544:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   * @retval PLLI2S clock frequency (in Hz)
1545:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1546:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** uint32_t RCC_PLLI2S_GetFreqDomain_I2S(void)
1547:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** {
 3530              		.loc 1 1547 1 is_stmt 1 view -0
 3531              		.cfi_startproc
 3532              		@ args = 0, pretend = 0, frame = 0
 3533              		@ frame_needed = 0, uses_anonymous_args = 0
 3534              		@ link register save eliminated.
1548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t pllinputfreq = 0U, pllsource = 0U;
 3535              		.loc 1 1548 3 view .LVU1045
 3536              	.LVL299:
1549:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1550:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   /* PLLI2S_VCO = (HSE_VALUE or HSI_VALUE / PLLM) * PLLI2SN
1551:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****      I2S Domain clock  = PLLI2S_VCO / PLLI2SR
1552:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   */
1553:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   pllsource = LL_RCC_PLL_GetMainSource();
 3537              		.loc 1 1553 3 view .LVU1046
 3538              	.LBB454:
 3539              	.LBI454:
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3540              		.loc 2 3461 26 view .LVU1047
 3541              	.LBB455:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3542              		.loc 2 3463 3 view .LVU1048
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3543              		.loc 2 3463 21 is_stmt 0 view .LVU1049
 3544 0000 0D4B     		ldr	r3, .L267
 3545 0002 5B68     		ldr	r3, [r3, #4]
 3546              	.LVL300:
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3547              		.loc 2 3463 21 view .LVU1050
 3548              	.LBE455:
 3549              	.LBE454:
1554:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1555:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   switch (pllsource)
 3550              		.loc 1 1555 3 is_stmt 1 view .LVU1051
 3551 0004 13F4800F 		tst	r3, #4194304
 3552 0008 13D0     		beq	.L266
1556:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
1557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSE:  /* HSE used as PLLI2S clock source */
1558:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSE_VALUE;
 3553              		.loc 1 1558 20 is_stmt 0 view .LVU1052
 3554 000a 0C4B     		ldr	r3, .L267+4
 3555              	.LVL301:
 3556              	.L265:
1559:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1560:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
1561:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     case LL_RCC_PLLSOURCE_HSI:  /* HSI used as PLLI2S clock source */
1562:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     default:
1563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       pllinputfreq = HSI_VALUE;
1564:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
1565:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   }
1566:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   return __LL_RCC_CALC_PLLI2S_I2S_FREQ(pllinputfreq, LL_RCC_PLL_GetDivider(),
 3557              		.loc 1 1566 3 is_stmt 1 view .LVU1053
 3558              	.LBB456:
ARM GAS  /tmp/cc42qbQx.s 			page 187


 3559              	.LBI456:
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3560              		.loc 2 3601 26 view .LVU1054
 3561              	.LBB457:
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3562              		.loc 2 3603 3 view .LVU1055
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3563              		.loc 2 3603 21 is_stmt 0 view .LVU1056
 3564 000c 0A4A     		ldr	r2, .L267
 3565 000e 5168     		ldr	r1, [r2, #4]
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3566              		.loc 2 3603 10 view .LVU1057
 3567 0010 01F03F01 		and	r1, r1, #63
 3568              	.LBE457:
 3569              	.LBE456:
 3570              		.loc 1 1566 10 discriminator 1 view .LVU1058
 3571 0014 B3FBF1F3 		udiv	r3, r3, r1
 3572              	.LVL302:
 3573              	.LBB458:
 3574              	.LBI458:
4040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3575              		.loc 2 4040 26 is_stmt 1 view .LVU1059
 3576              	.LBB459:
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3577              		.loc 2 4042 3 view .LVU1060
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3578              		.loc 2 4042 21 is_stmt 0 view .LVU1061
 3579 0018 D2F88410 		ldr	r1, [r2, #132]
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3580              		.loc 2 4042 10 view .LVU1062
 3581 001c C1F38811 		ubfx	r1, r1, #6, #9
 3582              	.LBE459:
 3583              	.LBE458:
 3584              		.loc 1 1566 10 discriminator 2 view .LVU1063
 3585 0020 01FB03F3 		mul	r3, r1, r3
 3586              	.LBB460:
 3587              	.LBI460:
4081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3588              		.loc 2 4081 26 is_stmt 1 view .LVU1064
 3589              	.LBB461:
4083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3590              		.loc 2 4083 3 view .LVU1065
4083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3591              		.loc 2 4083 21 is_stmt 0 view .LVU1066
 3592 0024 D2F88400 		ldr	r0, [r2, #132]
 3593              	.LBE461:
 3594              	.LBE460:
 3595              		.loc 1 1566 10 discriminator 3 view .LVU1067
 3596 0028 C0F30270 		ubfx	r0, r0, #28, #3
1567:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****                                         LL_RCC_PLLI2S_GetN(), LL_RCC_PLLI2S_GetR());
1568:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3597              		.loc 1 1568 1 view .LVU1068
 3598 002c B3FBF0F0 		udiv	r0, r3, r0
 3599 0030 7047     		bx	lr
 3600              	.LVL303:
 3601              	.L266:
1563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
ARM GAS  /tmp/cc42qbQx.s 			page 188


 3602              		.loc 1 1563 20 view .LVU1069
 3603 0032 034B     		ldr	r3, .L267+8
 3604              	.LVL304:
1563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****       break;
 3605              		.loc 1 1563 20 view .LVU1070
 3606 0034 EAE7     		b	.L265
 3607              	.L268:
 3608 0036 00BF     		.align	2
 3609              	.L267:
 3610 0038 00380240 		.word	1073887232
 3611 003c 40787D01 		.word	25000000
 3612 0040 0024F400 		.word	16000000
 3613              		.cfi_endproc
 3614              	.LFE322:
 3616              		.section	.text.LL_RCC_GetI2SClockFreq,"ax",%progbits
 3617              		.align	1
 3618              		.global	LL_RCC_GetI2SClockFreq
 3619              		.syntax unified
 3620              		.thumb
 3621              		.thumb_func
 3623              	LL_RCC_GetI2SClockFreq:
 3624              	.LVL305:
 3625              	.LFB300:
 679:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2s_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3626              		.loc 1 679 1 is_stmt 1 view -0
 3627              		.cfi_startproc
 3628              		@ args = 0, pretend = 0, frame = 0
 3629              		@ frame_needed = 0, uses_anonymous_args = 0
 680:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3630              		.loc 1 680 3 view .LVU1072
 683:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3631              		.loc 1 683 3 view .LVU1073
 685:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3632              		.loc 1 685 3 view .LVU1074
 685:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   {
 3633              		.loc 1 685 6 is_stmt 0 view .LVU1075
 3634 0000 B0F5000F 		cmp	r0, #8388608
 3635 0004 01D0     		beq	.L277
 680:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3636              		.loc 1 680 12 view .LVU1076
 3637 0006 0020     		movs	r0, #0
 3638              	.LVL306:
 705:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3639              		.loc 1 705 1 view .LVU1077
 3640 0008 7047     		bx	lr
 3641              	.LVL307:
 3642              	.L277:
 679:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****   uint32_t i2s_frequency = LL_RCC_PERIPH_FREQUENCY_NO;
 3643              		.loc 1 679 1 view .LVU1078
 3644 000a 08B5     		push	{r3, lr}
 3645              	.LCFI16:
 3646              		.cfi_def_cfa_offset 8
 3647              		.cfi_offset 3, -8
 3648              		.cfi_offset 14, -4
 688:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3649              		.loc 1 688 5 is_stmt 1 view .LVU1079
 3650              	.LVL308:
ARM GAS  /tmp/cc42qbQx.s 			page 189


 3651              	.LBB462:
 3652              	.LBI462:
2862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3653              		.loc 2 2862 26 view .LVU1080
 3654              	.LBB463:
2864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3655              		.loc 2 2864 3 view .LVU1081
2864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3656              		.loc 2 2864 21 is_stmt 0 view .LVU1082
 3657 000c 074B     		ldr	r3, .L279
 3658 000e 9B68     		ldr	r3, [r3, #8]
 3659              	.LVL309:
2864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3660              		.loc 2 2864 21 view .LVU1083
 3661              	.LBE463:
 3662              	.LBE462:
 688:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****     {
 3663              		.loc 1 688 5 discriminator 1 view .LVU1084
 3664 0010 1842     		tst	r0, r3
 3665 0012 08D1     		bne	.L272
 691:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3666              		.loc 1 691 9 is_stmt 1 view .LVU1085
 3667              	.LBB464:
 3668              	.LBI464:
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 3669              		.loc 2 3711 26 view .LVU1086
 3670              	.LBB465:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3671              		.loc 2 3713 3 view .LVU1087
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3672              		.loc 2 3713 11 is_stmt 0 view .LVU1088
 3673 0014 054B     		ldr	r3, .L279
 3674 0016 1868     		ldr	r0, [r3]
 3675              	.LVL310:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 3676              		.loc 2 3713 11 view .LVU1089
 3677              	.LBE465:
 3678              	.LBE464:
 691:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         {
 3679              		.loc 1 691 12 discriminator 1 view .LVU1090
 3680 0018 10F00060 		ands	r0, r0, #134217728
 3681 001c 00D1     		bne	.L278
 3682              	.LVL311:
 3683              	.L269:
 705:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** 
 3684              		.loc 1 705 1 view .LVU1091
 3685 001e 08BD     		pop	{r3, pc}
 3686              	.LVL312:
 3687              	.L278:
 693:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3688              		.loc 1 693 11 is_stmt 1 view .LVU1092
 693:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3689              		.loc 1 693 27 is_stmt 0 view .LVU1093
 3690 0020 FFF7FEFF 		bl	RCC_PLLI2S_GetFreqDomain_I2S
 3691              	.LVL313:
 693:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         }
 3692              		.loc 1 693 27 view .LVU1094
ARM GAS  /tmp/cc42qbQx.s 			page 190


 3693 0024 FBE7     		b	.L269
 3694              	.LVL314:
 3695              	.L272:
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c ****         break;
 3696              		.loc 1 699 23 view .LVU1095
 3697 0026 0248     		ldr	r0, .L279+4
 3698              	.LVL315:
 704:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3699              		.loc 1 704 3 is_stmt 1 view .LVU1096
 704:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_rcc.c **** }
 3700              		.loc 1 704 10 is_stmt 0 view .LVU1097
 3701 0028 F9E7     		b	.L269
 3702              	.L280:
 3703 002a 00BF     		.align	2
 3704              	.L279:
 3705 002c 00380240 		.word	1073887232
 3706 0030 0080BB00 		.word	12288000
 3707              		.cfi_endproc
 3708              	.LFE300:
 3710              		.section	.rodata.aRCC_PLLSAIDIVRPrescTable,"a"
 3711              		.align	2
 3714              	aRCC_PLLSAIDIVRPrescTable:
 3715 0000 02040810 		.ascii	"\002\004\010\020"
 3716              		.text
 3717              	.Letext0:
 3718              		.file 3 "/usr/lib/gcc/arm-none-eabi/13.2.1/include/stdint.h"
 3719              		.file 4 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/system_stm32f7xx.h"
 3720              		.file 5 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/stm32f767xx.h"
 3721              		.file 6 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/stm32f7xx.h"
ARM GAS  /tmp/cc42qbQx.s 			page 191


DEFINED SYMBOLS
                            *ABS*:00000000 stm32f7xx_ll_rcc.c
     /tmp/cc42qbQx.s:20     .text.LL_RCC_DeInit:00000000 $t
     /tmp/cc42qbQx.s:26     .text.LL_RCC_DeInit:00000000 LL_RCC_DeInit
     /tmp/cc42qbQx.s:184    .text.LL_RCC_DeInit:0000008c $d
     /tmp/cc42qbQx.s:191    .text.LL_RCC_GetCECClockFreq:00000000 $t
     /tmp/cc42qbQx.s:197    .text.LL_RCC_GetCECClockFreq:00000000 LL_RCC_GetCECClockFreq
     /tmp/cc42qbQx.s:275    .text.LL_RCC_GetCECClockFreq:0000002c $d
     /tmp/cc42qbQx.s:280    .text.RCC_GetHCLKClockFreq:00000000 $t
     /tmp/cc42qbQx.s:286    .text.RCC_GetHCLKClockFreq:00000000 RCC_GetHCLKClockFreq
     /tmp/cc42qbQx.s:317    .text.RCC_GetHCLKClockFreq:00000010 $d
     /tmp/cc42qbQx.s:323    .text.RCC_GetPCLK1ClockFreq:00000000 $t
     /tmp/cc42qbQx.s:329    .text.RCC_GetPCLK1ClockFreq:00000000 RCC_GetPCLK1ClockFreq
     /tmp/cc42qbQx.s:360    .text.RCC_GetPCLK1ClockFreq:00000010 $d
     /tmp/cc42qbQx.s:366    .text.RCC_GetPCLK2ClockFreq:00000000 $t
     /tmp/cc42qbQx.s:372    .text.RCC_GetPCLK2ClockFreq:00000000 RCC_GetPCLK2ClockFreq
     /tmp/cc42qbQx.s:403    .text.RCC_GetPCLK2ClockFreq:00000010 $d
     /tmp/cc42qbQx.s:409    .text.RCC_PLL_GetFreqDomain_SYS:00000000 $t
     /tmp/cc42qbQx.s:415    .text.RCC_PLL_GetFreqDomain_SYS:00000000 RCC_PLL_GetFreqDomain_SYS
     /tmp/cc42qbQx.s:500    .text.RCC_PLL_GetFreqDomain_SYS:00000038 $d
     /tmp/cc42qbQx.s:507    .text.RCC_GetSystemClockFreq:00000000 $t
     /tmp/cc42qbQx.s:513    .text.RCC_GetSystemClockFreq:00000000 RCC_GetSystemClockFreq
     /tmp/cc42qbQx.s:567    .text.RCC_GetSystemClockFreq:00000020 $d
     /tmp/cc42qbQx.s:574    .text.LL_RCC_GetSystemClocksFreq:00000000 $t
     /tmp/cc42qbQx.s:580    .text.LL_RCC_GetSystemClocksFreq:00000000 LL_RCC_GetSystemClocksFreq
     /tmp/cc42qbQx.s:626    .text.LL_RCC_GetUSARTClockFreq:00000000 $t
     /tmp/cc42qbQx.s:632    .text.LL_RCC_GetUSARTClockFreq:00000000 LL_RCC_GetUSARTClockFreq
     /tmp/cc42qbQx.s:1032   .text.LL_RCC_GetUSARTClockFreq:00000160 $d
     /tmp/cc42qbQx.s:1042   .text.LL_RCC_GetUARTClockFreq:00000000 $t
     /tmp/cc42qbQx.s:1048   .text.LL_RCC_GetUARTClockFreq:00000000 LL_RCC_GetUARTClockFreq
     /tmp/cc42qbQx.s:1448   .text.LL_RCC_GetUARTClockFreq:00000168 $d
     /tmp/cc42qbQx.s:1458   .text.LL_RCC_GetI2CClockFreq:00000000 $t
     /tmp/cc42qbQx.s:1464   .text.LL_RCC_GetI2CClockFreq:00000000 LL_RCC_GetI2CClockFreq
     /tmp/cc42qbQx.s:1764   .text.LL_RCC_GetI2CClockFreq:00000108 $d
     /tmp/cc42qbQx.s:1774   .text.LL_RCC_GetLPTIMClockFreq:00000000 $t
     /tmp/cc42qbQx.s:1780   .text.LL_RCC_GetLPTIMClockFreq:00000000 LL_RCC_GetLPTIMClockFreq
     /tmp/cc42qbQx.s:1912   .text.LL_RCC_GetLPTIMClockFreq:00000064 $d
     /tmp/cc42qbQx.s:1918   .text.LL_RCC_GetDFSDMClockFreq:00000000 $t
     /tmp/cc42qbQx.s:1924   .text.LL_RCC_GetDFSDMClockFreq:00000000 LL_RCC_GetDFSDMClockFreq
     /tmp/cc42qbQx.s:1984   .text.LL_RCC_GetDFSDMClockFreq:00000024 $d
     /tmp/cc42qbQx.s:1989   .text.RCC_PLL_GetFreqDomain_48M:00000000 $t
     /tmp/cc42qbQx.s:1995   .text.RCC_PLL_GetFreqDomain_48M:00000000 RCC_PLL_GetFreqDomain_48M
     /tmp/cc42qbQx.s:2078   .text.RCC_PLL_GetFreqDomain_48M:00000034 $d
     /tmp/cc42qbQx.s:2085   .text.RCC_PLLSAI_GetFreqDomain_SAI:00000000 $t
     /tmp/cc42qbQx.s:2091   .text.RCC_PLLSAI_GetFreqDomain_SAI:00000000 RCC_PLLSAI_GetFreqDomain_SAI
     /tmp/cc42qbQx.s:2185   .text.RCC_PLLSAI_GetFreqDomain_SAI:00000044 $d
     /tmp/cc42qbQx.s:2192   .text.RCC_PLLSAI_GetFreqDomain_48M:00000000 $t
     /tmp/cc42qbQx.s:2198   .text.RCC_PLLSAI_GetFreqDomain_48M:00000000 RCC_PLLSAI_GetFreqDomain_48M
     /tmp/cc42qbQx.s:2283   .text.RCC_PLLSAI_GetFreqDomain_48M:0000003c $d
     /tmp/cc42qbQx.s:2290   .text.LL_RCC_GetSDMMCClockFreq:00000000 $t
     /tmp/cc42qbQx.s:2296   .text.LL_RCC_GetSDMMCClockFreq:00000000 LL_RCC_GetSDMMCClockFreq
     /tmp/cc42qbQx.s:2495   .text.LL_RCC_GetSDMMCClockFreq:00000090 $d
     /tmp/cc42qbQx.s:2500   .text.LL_RCC_GetRNGClockFreq:00000000 $t
     /tmp/cc42qbQx.s:2506   .text.LL_RCC_GetRNGClockFreq:00000000 LL_RCC_GetRNGClockFreq
     /tmp/cc42qbQx.s:2594   .text.LL_RCC_GetRNGClockFreq:00000030 $d
     /tmp/cc42qbQx.s:2599   .text.LL_RCC_GetUSBClockFreq:00000000 $t
     /tmp/cc42qbQx.s:2605   .text.LL_RCC_GetUSBClockFreq:00000000 LL_RCC_GetUSBClockFreq
ARM GAS  /tmp/cc42qbQx.s 			page 192


     /tmp/cc42qbQx.s:2693   .text.LL_RCC_GetUSBClockFreq:00000030 $d
     /tmp/cc42qbQx.s:2698   .text.RCC_PLLSAI_GetFreqDomain_LTDC:00000000 $t
     /tmp/cc42qbQx.s:2704   .text.RCC_PLLSAI_GetFreqDomain_LTDC:00000000 RCC_PLLSAI_GetFreqDomain_LTDC
     /tmp/cc42qbQx.s:2800   .text.RCC_PLLSAI_GetFreqDomain_LTDC:00000048 $d
     /tmp/cc42qbQx.s:3714   .rodata.aRCC_PLLSAIDIVRPrescTable:00000000 aRCC_PLLSAIDIVRPrescTable
     /tmp/cc42qbQx.s:2808   .text.LL_RCC_GetLTDCClockFreq:00000000 $t
     /tmp/cc42qbQx.s:2814   .text.LL_RCC_GetLTDCClockFreq:00000000 LL_RCC_GetLTDCClockFreq
     /tmp/cc42qbQx.s:2862   .text.LL_RCC_GetLTDCClockFreq:00000014 $d
     /tmp/cc42qbQx.s:2867   .text.RCC_PLLI2S_GetFreqDomain_SAI:00000000 $t
     /tmp/cc42qbQx.s:2873   .text.RCC_PLLI2S_GetFreqDomain_SAI:00000000 RCC_PLLI2S_GetFreqDomain_SAI
     /tmp/cc42qbQx.s:2968   .text.RCC_PLLI2S_GetFreqDomain_SAI:00000044 $d
     /tmp/cc42qbQx.s:2975   .text.LL_RCC_GetSAIClockFreq:00000000 $t
     /tmp/cc42qbQx.s:2981   .text.LL_RCC_GetSAIClockFreq:00000000 LL_RCC_GetSAIClockFreq
     /tmp/cc42qbQx.s:3286   .text.LL_RCC_GetSAIClockFreq:00000108 $d
     /tmp/cc42qbQx.s:3295   .text.LL_RCC_GetDFSDMAudioClockFreq:00000000 $t
     /tmp/cc42qbQx.s:3301   .text.LL_RCC_GetDFSDMAudioClockFreq:00000000 LL_RCC_GetDFSDMAudioClockFreq
     /tmp/cc42qbQx.s:3360   .text.LL_RCC_GetDFSDMAudioClockFreq:00000020 $d
     /tmp/cc42qbQx.s:3365   .text.RCC_PLLI2S_GetFreqDomain_SPDIFRX:00000000 $t
     /tmp/cc42qbQx.s:3371   .text.RCC_PLLI2S_GetFreqDomain_SPDIFRX:00000000 RCC_PLLI2S_GetFreqDomain_SPDIFRX
     /tmp/cc42qbQx.s:3456   .text.RCC_PLLI2S_GetFreqDomain_SPDIFRX:0000003c $d
     /tmp/cc42qbQx.s:3463   .text.LL_RCC_GetSPDIFRXClockFreq:00000000 $t
     /tmp/cc42qbQx.s:3469   .text.LL_RCC_GetSPDIFRXClockFreq:00000000 LL_RCC_GetSPDIFRXClockFreq
     /tmp/cc42qbQx.s:3517   .text.LL_RCC_GetSPDIFRXClockFreq:00000014 $d
     /tmp/cc42qbQx.s:3522   .text.RCC_PLLI2S_GetFreqDomain_I2S:00000000 $t
     /tmp/cc42qbQx.s:3528   .text.RCC_PLLI2S_GetFreqDomain_I2S:00000000 RCC_PLLI2S_GetFreqDomain_I2S
     /tmp/cc42qbQx.s:3610   .text.RCC_PLLI2S_GetFreqDomain_I2S:00000038 $d
     /tmp/cc42qbQx.s:3617   .text.LL_RCC_GetI2SClockFreq:00000000 $t
     /tmp/cc42qbQx.s:3623   .text.LL_RCC_GetI2SClockFreq:00000000 LL_RCC_GetI2SClockFreq
     /tmp/cc42qbQx.s:3705   .text.LL_RCC_GetI2SClockFreq:0000002c $d
     /tmp/cc42qbQx.s:3711   .rodata.aRCC_PLLSAIDIVRPrescTable:00000000 $d

UNDEFINED SYMBOLS
AHBPrescTable
APBPrescTable
