ARM GAS  /tmp/ccqw5Uyy.s 			page 1


   1              		.cpu cortex-m7
   2              		.arch armv7e-m
   3              		.fpu fpv5-d16
   4              		.eabi_attribute 28, 1
   5              		.eabi_attribute 20, 1
   6              		.eabi_attribute 21, 1
   7              		.eabi_attribute 23, 3
   8              		.eabi_attribute 24, 1
   9              		.eabi_attribute 25, 1
  10              		.eabi_attribute 26, 1
  11              		.eabi_attribute 30, 1
  12              		.eabi_attribute 34, 1
  13              		.eabi_attribute 18, 4
  14              		.file	"stm32f7xx_ll_utils.c"
  15              		.text
  16              	.Ltext0:
  17              		.cfi_sections	.debug_frame
  18              		.file 1 "Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c"
  19              		.section	.text.UTILS_GetPLLOutputFrequency,"ax",%progbits
  20              		.align	1
  21              		.syntax unified
  22              		.thumb
  23              		.thumb_func
  25              	UTILS_GetPLLOutputFrequency:
  26              	.LVL0:
  27              	.LFB411:
   1:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @file    stm32f7xx_ll_utils.c
   4:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief   UTILS LL module driver.
   6:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * This software is licensed under terms that can be found in the LICENSE file
  13:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * in the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *
  16:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ******************************************************************************
  17:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
  18:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Includes ------------------------------------------------------------------*/
  19:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #include "stm32f7xx_ll_utils.h"
  20:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #include "stm32f7xx_ll_rcc.h"
  21:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #include "stm32f7xx_ll_system.h"
  22:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #include "stm32f7xx_ll_pwr.h"
  23:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #ifdef  USE_FULL_ASSERT
  24:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #include "stm32_assert.h"
  25:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #else
  26:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define assert_param(expr) ((void)0U)
  27:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #endif /* USE_FULL_ASSERT */
  28:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  29:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup STM32F7xx_LL_Driver
  30:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
  31:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 2


  32:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  33:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL
  34:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
  35:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
  36:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  37:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Private types -------------------------------------------------------------*/
  38:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Private variables ---------------------------------------------------------*/
  39:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Private constants ---------------------------------------------------------*/
  40:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL_Private_Constants
  41:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
  42:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
  43:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_MAX_FREQUENCY_SCALE1  216000000U /*!< Maximum frequency for system clock at power sca
  44:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_MAX_FREQUENCY_SCALE2  180000000U       /*!< Maximum frequency for system clock at pow
  45:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_MAX_FREQUENCY_SCALE3  144000000U       /*!< Maximum frequency for system clock at pow
  46:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  47:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Defines used for PLL range */
  48:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_PLLVCO_INPUT_MIN         950000U       /*!< Frequency min for PLLVCO input, in Hz   *
  49:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_PLLVCO_INPUT_MAX        2100000U       /*!< Frequency max for PLLVCO input, in Hz   *
  50:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_PLLVCO_OUTPUT_MIN     100000000U       /*!< Frequency min for PLLVCO output, in Hz  *
  51:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_PLLVCO_OUTPUT_MAX     432000000U       /*!< Frequency max for PLLVCO output, in Hz  *
  52:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  53:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Defines used for HSE range */
  54:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_HSE_FREQUENCY_MIN      4000000U        /*!< Frequency min for HSE frequency, in Hz   
  55:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_HSE_FREQUENCY_MAX     26000000U        /*!< Frequency max for HSE frequency, in Hz   
  56:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  57:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Defines used for FLASH latency according to HCLK Frequency */
  58:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY1_FREQ   30000000U      /*!< HCLK frequency to set FLASH latency 1 in p
  59:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY2_FREQ   60000000U      /*!< HCLK frequency to set FLASH latency 2 in p
  60:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY3_FREQ   90000000U      /*!< HCLK frequency to set FLASH latency 3 in p
  61:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY4_FREQ  120000000U      /*!< HCLK frequency to set FLASH latency 4 in p
  62:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY5_FREQ  150000000U      /*!< HCLK frequency to set FLASH latency 5 in p
  63:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY6_FREQ  180000000U      /*!< HCLK frequency to set FLASH latency 6 in p
  64:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE1_LATENCY7_FREQ  210000000U      /*!< HCLK frequency to set FLASH latency 7 in p
  65:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE2_LATENCY1_FREQ   30000000U      /*!< HCLK frequency to set FLASH latency 1 in p
  66:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE2_LATENCY2_FREQ   60000000U      /*!< HCLK frequency to set FLASH latency 2 in p
  67:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE2_LATENCY3_FREQ   90000000U      /*!< HCLK frequency to set FLASH latency 3 in p
  68:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE2_LATENCY4_FREQ  120000000U      /*!< HCLK frequency to set FLASH latency 4 in p
  69:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE2_LATENCY5_FREQ  150000000U      /*!< HCLK frequency to set FLASH latency 5 in p
  70:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE3_LATENCY1_FREQ   30000000U      /*!< HCLK frequency to set FLASH latency 1 in p
  71:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE3_LATENCY2_FREQ   60000000U      /*!< HCLK frequency to set FLASH latency 2 in p
  72:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE3_LATENCY3_FREQ   90000000U      /*!< HCLK frequency to set FLASH latency 3 in p
  73:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define UTILS_SCALE3_LATENCY4_FREQ  120000000U      /*!< HCLK frequency to set FLASH latency 4 in p
  74:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
  75:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
  76:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
  77:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  78:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Private macros ------------------------------------------------------------*/
  79:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL_Private_Macros
  80:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
  81:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
  82:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_SYSCLK_DIV(__VALUE__) (((__VALUE__) == LL_RCC_SYSCLK_DIV_1)   \
  83:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_2)   \
  84:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_4)   \
  85:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_8)   \
  86:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_16)  \
  87:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_64)  \
  88:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_128) \
ARM GAS  /tmp/ccqw5Uyy.s 			page 3


  89:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_256) \
  90:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_SYSCLK_DIV_512))
  91:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  92:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_APB1_DIV(__VALUE__) (((__VALUE__) == LL_RCC_APB1_DIV_1) \
  93:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB1_DIV_2) \
  94:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB1_DIV_4) \
  95:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB1_DIV_8) \
  96:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB1_DIV_16))
  97:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
  98:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_APB2_DIV(__VALUE__) (((__VALUE__) == LL_RCC_APB2_DIV_1) \
  99:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB2_DIV_2) \
 100:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB2_DIV_4) \
 101:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB2_DIV_8) \
 102:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                       || ((__VALUE__) == LL_RCC_APB2_DIV_16))
 103:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 104:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLLM_VALUE(__VALUE__) (((__VALUE__) == LL_RCC_PLLM_DIV_2)  \
 105:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_3)  \
 106:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_4)  \
 107:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_5)  \
 108:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_6)  \
 109:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_7)  \
 110:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_8)  \
 111:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_9)  \
 112:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_10) \
 113:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_11) \
 114:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_12) \
 115:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_13) \
 116:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_14) \
 117:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_15) \
 118:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_16) \
 119:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_17) \
 120:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_18) \
 121:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_19) \
 122:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_20) \
 123:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_21) \
 124:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_22) \
 125:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_23) \
 126:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_24) \
 127:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_25) \
 128:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_26) \
 129:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_27) \
 130:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_28) \
 131:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_29) \
 132:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_30) \
 133:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_31) \
 134:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_32) \
 135:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_33) \
 136:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_34) \
 137:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_35) \
 138:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_36) \
 139:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_37) \
 140:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_38) \
 141:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_39) \
 142:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_40) \
 143:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_41) \
 144:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_42) \
 145:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_43) \
ARM GAS  /tmp/ccqw5Uyy.s 			page 4


 146:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_44) \
 147:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_45) \
 148:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_46) \
 149:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_47) \
 150:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_48) \
 151:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_49) \
 152:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_50) \
 153:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_51) \
 154:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_52) \
 155:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_53) \
 156:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_54) \
 157:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_55) \
 158:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_56) \
 159:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_57) \
 160:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_58) \
 161:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_59) \
 162:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_60) \
 163:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_61) \
 164:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_62) \
 165:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLM_DIV_63))
 166:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 167:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLLN_VALUE(__VALUE__) ((50 <= (__VALUE__)) && ((__VALUE__) <= 432))
 168:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 169:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLLP_VALUE(__VALUE__) (((__VALUE__) == LL_RCC_PLLP_DIV_2) \
 170:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLP_DIV_4) \
 171:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLP_DIV_6) \
 172:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__VALUE__) == LL_RCC_PLLP_DIV_8))
 173:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 174:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLLVCO_INPUT(__VALUE__)  ((UTILS_PLLVCO_INPUT_MIN <= (__VALUE__)) && ((__VALUE_
 175:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 176:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLLVCO_OUTPUT(__VALUE__) ((UTILS_PLLVCO_OUTPUT_MIN <= (__VALUE__)) && ((__VALUE
 177:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 178:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_PLL_FREQUENCY(__VALUE__) ((LL_PWR_GetRegulVoltageScaling() == LL_PWR_REGU_VOLTA
 179:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                               (LL_PWR_GetRegulVoltageScaling() == LL_PWR_REGU_VOLTA
 180:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                               ((__VALUE__) <= UTILS_MAX_FREQUENCY_SCALE3))
 181:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 182:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_HSE_BYPASS(__STATE__) (((__STATE__) == LL_UTILS_HSEBYPASS_ON) \
 183:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                         || ((__STATE__) == LL_UTILS_HSEBYPASS_OFF))
 184:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 185:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** #define IS_LL_UTILS_HSE_FREQUENCY(__FREQUENCY__) (((__FREQUENCY__) >= UTILS_HSE_FREQUENCY_MIN) && (
 186:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 187:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
 188:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 189:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Private function prototypes -----------------------------------------------*/
 190:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @defgroup UTILS_LL_Private_Functions UTILS Private functions
 191:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
 192:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 193:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static uint32_t    UTILS_GetPLLOutputFrequency(uint32_t PLL_InputFrequency,
 194:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                                LL_UTILS_PLLInitTypeDef *UTILS_PLLInitStruct);
 195:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static ErrorStatus UTILS_EnablePLLAndSwitchSystem(uint32_t SYSCLK_Frequency, LL_UTILS_ClkInitTypeDe
 196:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static ErrorStatus UTILS_PLL_IsBusy(void);
 197:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 198:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
 199:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 200:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 201:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /* Exported functions --------------------------------------------------------*/
 202:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL_Exported_Functions
ARM GAS  /tmp/ccqw5Uyy.s 			page 5


 203:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
 204:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 205:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 206:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL_EF_DELAY
 207:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
 208:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 209:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 210:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 211:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  This function configures the Cortex-M SysTick source to have 1ms time base.
 212:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   When a RTOS is used, it is recommended to avoid changing the Systick
 213:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         configuration by calling this function, for a delay use rather osDelay RTOS service.
 214:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  HCLKFrequency HCLK frequency in Hz
 215:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   HCLK frequency can be calculated thanks to RCC helper macro or function @ref LL_RCC_Get
 216:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval None
 217:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 218:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** void LL_Init1msTick(uint32_t HCLKFrequency)
 219:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 220:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Use frequency provided in argument */
 221:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   LL_InitTick(HCLKFrequency, 1000U);
 222:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 223:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 224:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 225:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  This function provides accurate delay (in milliseconds) based
 226:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         on SysTick counter flag
 227:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   When a RTOS is used, it is recommended to avoid using blocking delay
 228:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         and use rather osDelay service.
 229:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   To respect 1ms timebase, user should call @ref LL_Init1msTick function which
 230:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         will configure Systick to 1ms
 231:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  Delay specifies the delay time length, in milliseconds.
 232:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval None
 233:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 234:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** void LL_mDelay(uint32_t Delay)
 235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   __IO uint32_t  tmp = SysTick->CTRL;  /* Clear the COUNTFLAG first */
 237:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Add this code to indicate that local variable is not used */
 238:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ((void)tmp);
 239:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 240:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Add a period to guaranty minimum wait */
 241:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(Delay < LL_MAX_DELAY)
 242:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 243:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     Delay++;
 244:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 245:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   while (Delay)
 247:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     if((SysTick->CTRL & SysTick_CTRL_COUNTFLAG_Msk) != 0U)
 249:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       Delay--;
 251:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 252:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 253:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 254:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 255:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 256:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
 257:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 258:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 259:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_EF_SYSTEM
ARM GAS  /tmp/ccqw5Uyy.s 			page 6


 260:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *  @brief    System Configuration functions
 261:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *
 262:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   @verbatim
 263:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****  ===============================================================================
 264:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****            ##### System Configuration functions #####
 265:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****  ===============================================================================
 266:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     [..]
 267:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****          System, AHB and APB buses clocks configuration
 268:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 269:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****          (+) The maximum frequency of the SYSCLK, HCLK, PCLK1 and PCLK2 is 216000000 Hz.
 270:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   @endverbatim
 271:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   @internal
 272:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              Depending on the device voltage range, the maximum frequency should be
 273:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              adapted accordingly:
 274:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) +--------------------------------------------------------------------------------
 275:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |  Wait states   |                           HCLK clock frequency (MHz)          
 276:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |                |---------------------------------------------------------------
 277:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |  (Latency)     |   voltage range   |   voltage range   |   voltage range   |   
 278:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |                |    2.7V - 3.6V    |    2.4V - 2.7V    |    2.1V - 2.7V    |   
 279:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 280:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |0WS(1CPU cycle) |   0 < HCLK <= 30  |   0 < HCLK <= 24  |   0 < HCLK <= 22  |   
 281:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 282:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |1WS(2CPU cycle) |  30 < HCLK <= 60  |  24 < HCLK <= 48  |  22 < HCLK <= 44  |  2
 283:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 284:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |2WS(3CPU cycle) |  60 < HCLK <= 90  |  48 < HCLK <= 72  |  44 < HCLK <= 66  |  4
 285:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 286:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |3WS(4CPU cycle) |  90 < HCLK <= 120 |  72 < HCLK <= 96  |  66 < HCLK <= 88  |  6
 287:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 288:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |4WS(5CPU cycle) | 120 < HCLK <= 150 |  96 < HCLK <= 120 |  88 < HCLK <= 110 |  8
 289:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 290:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |5WS(6CPU cycle) | 150 < HCLK <= 180 | 120 < HCLK <= 144 | 110 < HCLK <= 132 | 10
 291:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 292:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |6WS(7CPU cycle) | 180 < HCLK <= 210 | 144 < HCLK <= 168 | 132 < HCLK <= 154 | 12
 293:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 294:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |7WS(8CPU cycle) | 210 < HCLK <= 216 | 168 < HCLK <= 192 | 154 < HCLK <= 176 | 14
 295:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 296:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |8WS(9CPU cycle) |        --         | 192 < HCLK <= 216 | 176 < HCLK <= 198 | 16
 297:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |----------------|-------------------|-------------------|-------------------|---
 298:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) |9WS(10CPU cycle)|        --         |         --        | 198 < HCLK <= 216 |   
 299:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****              (++) +--------------------------------------------------------------------------------
 300:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 301:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   @endinternal
 302:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
 303:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 304:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 305:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 306:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  This function sets directly SystemCoreClock CMSIS variable.
 307:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   Variable can be calculated also through SystemCoreClockUpdate function.
 308:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  HCLKFrequency HCLK frequency in Hz (can be calculated thanks to RCC helper macro)
 309:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval None
 310:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 311:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** void LL_SetSystemCoreClock(uint32_t HCLKFrequency)
 312:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 313:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* HCLK clock frequency */
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   SystemCoreClock = HCLKFrequency;
 315:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 316:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 7


 317:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 318:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  Update number of Flash wait states in line with new frequency and current
 319:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****             voltage range.
 320:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   This Function support ONLY devices with supply voltage (voltage range) between 2.7V and
 321:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  HCLK_Frequency  HCLK frequency
 322:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval An ErrorStatus enumeration value:
 323:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - SUCCESS: Latency has been modified
 324:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - ERROR: Latency cannot be modified
 325:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 326:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** ErrorStatus LL_SetFlashLatency(uint32_t HCLK_Frequency)
 327:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t timeout;
 329:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t getlatency;
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t latency = LL_FLASH_LATENCY_0;  /* default value 0WS */
 331:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 332:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 333:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Frequency cannot be equal to 0 */
 334:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(HCLK_Frequency == 0U)
 335:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 336:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 337:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 338:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   else
 339:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 340:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     if(LL_PWR_GetRegulVoltageScaling() == LL_PWR_REGU_VOLTAGE_SCALE1)
 341:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 342:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if(LL_PWR_IsEnabledOverDriveMode() != 0U)
 343:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           if(HCLK_Frequency > UTILS_SCALE1_LATENCY7_FREQ)
 345:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           {
 346:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****             /* 210 < HCLK <= 216 => 7WS (8 CPU cycles) */
 347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****             latency = LL_FLASH_LATENCY_7;
 348:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           }
 349:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           else /* (HCLK_Frequency > UTILS_SCALE1_LATENCY6_FREQ) */
 350:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           {
 351:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****             /* 180 < HCLK <= 210 => 6WS (7 CPU cycles) */
 352:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****             latency = LL_FLASH_LATENCY_6;
 353:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           }
 354:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if((HCLK_Frequency > UTILS_SCALE1_LATENCY5_FREQ) && (latency == LL_FLASH_LATENCY_0))
 356:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 357:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 150 < HCLK <= 180 => 5WS (6 CPU cycles) */
 358:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_5;
 359:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if((HCLK_Frequency > UTILS_SCALE1_LATENCY4_FREQ) && (latency == LL_FLASH_LATENCY_0))
 361:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 362:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 120 < HCLK <= 150 => 4WS (5 CPU cycles) */
 363:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_4;
 364:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if((HCLK_Frequency > UTILS_SCALE1_LATENCY3_FREQ) && (latency == LL_FLASH_LATENCY_0))
 366:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 367:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 90 < HCLK <= 120 => 3WS (4 CPU cycles) */
 368:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_3;
 369:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if((HCLK_Frequency > UTILS_SCALE1_LATENCY2_FREQ) && (latency == LL_FLASH_LATENCY_0))
 371:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 372:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 60 < HCLK <= 90 => 2WS (3 CPU cycles) */
 373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_2;
ARM GAS  /tmp/ccqw5Uyy.s 			page 8


 374:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 375:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else
 376:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         if((HCLK_Frequency > UTILS_SCALE1_LATENCY1_FREQ) && (latency == LL_FLASH_LATENCY_0))
 378:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 379:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           /* 30 < HCLK <= 60 => 1WS (2 CPU cycles) */
 380:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           latency = LL_FLASH_LATENCY_1;
 381:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 382:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* else HCLK_Frequency < 30MHz default LL_FLASH_LATENCY_0 0WS */
 383:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 384:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     else if(LL_PWR_GetRegulVoltageScaling() == LL_PWR_REGU_VOLTAGE_SCALE2)
 386:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 387:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if(HCLK_Frequency > UTILS_SCALE2_LATENCY5_FREQ)
 388:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 389:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 150 < HCLK <= 168 OR 150 < HCLK <= 180 (when OverDrive mode is enable) => 5WS (6 CPU cyc
 390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_5;
 391:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 392:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if(HCLK_Frequency > UTILS_SCALE2_LATENCY4_FREQ)
 393:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 394:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 120 < HCLK <= 150 => 4WS (5 CPU cycles) */
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_4;
 396:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if(HCLK_Frequency > UTILS_SCALE2_LATENCY3_FREQ)
 398:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 399:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 90 < HCLK <= 120 => 3WS (4 CPU cycles) */
 400:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_3;
 401:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if(HCLK_Frequency > UTILS_SCALE2_LATENCY2_FREQ)
 403:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 404:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 60 < HCLK <= 90 => 2WS (3 CPU cycles) */
 405:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_2;
 406:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 407:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else
 408:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         if(HCLK_Frequency > UTILS_SCALE2_LATENCY1_FREQ)
 410:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 411:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           /* 30 < HCLK <= 60 => 1WS (2 CPU cycles) */
 412:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           latency = LL_FLASH_LATENCY_1;
 413:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 414:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* else HCLK_Frequency < 24MHz default LL_FLASH_LATENCY_0 0WS */
 415:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 416:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 417:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     else /* Scale 3 */
 418:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 419:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if(HCLK_Frequency > UTILS_SCALE3_LATENCY4_FREQ)
 420:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 421:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 120 < HCLK <= 144 => 4WS (5 CPU cycles) */
 422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_4;
 423:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 424:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if(HCLK_Frequency > UTILS_SCALE3_LATENCY3_FREQ)
 425:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 426:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 90 < HCLK <= 120 => 3WS (4 CPU cycles) */
 427:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_3;
 428:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 429:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else if(HCLK_Frequency > UTILS_SCALE3_LATENCY2_FREQ)
 430:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
ARM GAS  /tmp/ccqw5Uyy.s 			page 9


 431:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* 60 < HCLK <= 90 => 2WS (3 CPU cycles) */
 432:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         latency = LL_FLASH_LATENCY_2;
 433:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 434:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else
 435:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 436:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         if(HCLK_Frequency > UTILS_SCALE3_LATENCY1_FREQ)
 437:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 438:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           /* 30 < HCLK <= 60 => 1WS (2 CPU cycles) */
 439:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           latency = LL_FLASH_LATENCY_1;
 440:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 441:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* else HCLK_Frequency < 22MHz default LL_FLASH_LATENCY_0 0WS */
 442:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 443:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 444:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     if (status != ERROR)
 446:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 447:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       LL_FLASH_SetLatency(latency);
 448:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 449:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Check that the new number of wait states is taken into account to access the Flash
 450:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****            memory by reading the FLASH_ACR register */
 451:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       timeout = 2;
 452:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       do
 453:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 454:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Wait for Flash latency to be updated */
 455:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       getlatency = LL_FLASH_GetLatency();
 456:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       timeout--;
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       } while ((getlatency != latency) && (timeout > 0));
 458:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 459:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if(getlatency != latency)
 460:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 461:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         status = ERROR;
 462:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 463:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else
 464:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         status = SUCCESS;
 466:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 467:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 468:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return status;
 470:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 471:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 472:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 473:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  This function configures system clock at maximum frequency with HSI as clock source of 
 474:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   The application need to ensure that PLL is disabled.
 475:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   Function is based on the following formula:
 476:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLL output frequency = (((HSI frequency / PLLM) * PLLN) / PLLP)
 477:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLM: ensure that the VCO input frequency ranges from 0.95 to 2.1 MHz (PLLVCO_input =
 478:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLN: ensure that the VCO output frequency is between 100 and 432 MHz (PLLVCO_output 
 479:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLP: ensure that max frequency at 216000000 Hz is reach (PLLVCO_output / PLLP)
 480:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_PLLInitStruct pointer to a @ref LL_UTILS_PLLInitTypeDef structure that contains
 481:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the PLL.
 482:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_ClkInitStruct pointer to a @ref LL_UTILS_ClkInitTypeDef structure that contains
 483:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the BUS prescalers.
 484:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval An ErrorStatus enumeration value:
 485:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - SUCCESS: Max frequency configuration done
 486:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - ERROR: Max frequency configuration not done
 487:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 10


 488:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** ErrorStatus LL_PLL_ConfigSystemClock_HSI(LL_UTILS_PLLInitTypeDef *UTILS_PLLInitStruct,
 489:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                          LL_UTILS_ClkInitTypeDef *UTILS_ClkInitStruct)
 490:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 491:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t pllfreq = 0U;
 493:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 494:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check if one of the PLL is enabled */
 495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(UTILS_PLL_IsBusy() == SUCCESS)
 496:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 497:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Calculate the new PLL output frequency */
 498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     pllfreq = UTILS_GetPLLOutputFrequency(HSI_VALUE, UTILS_PLLInitStruct);
 499:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 500:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Enable HSI if not enabled */
 501:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     if(LL_RCC_HSI_IsReady() != 1U)
 502:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       LL_RCC_HSI_Enable();
 504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       while (LL_RCC_HSI_IsReady() != 1U)
 505:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 506:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* Wait for HSI ready */
 507:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 508:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 509:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 510:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Configure PLL */
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_PLL_ConfigDomain_SYS(LL_RCC_PLLSOURCE_HSI, UTILS_PLLInitStruct->PLLM, UTILS_PLLInitStruc
 512:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                 UTILS_PLLInitStruct->PLLP);
 513:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 514:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Enable PLL and switch system clock to PLL */
 515:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = UTILS_EnablePLLAndSwitchSystem(pllfreq, UTILS_ClkInitStruct);
 516:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 517:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   else
 518:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 519:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Current PLL configuration cannot be modified */
 520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 521:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 522:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return status;
 524:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 525:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 526:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 527:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  This function configures system clock with HSE as clock source of the PLL
 528:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   The application need to ensure that PLL is disabled.
 529:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @note   Function is based on the following formula:
 530:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLL output frequency = (((HSE frequency / PLLM) * PLLN) / PLLP)
 531:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLM: ensure that the VCO input frequency ranges from 0.95 to 2.10 MHz (PLLVCO_input 
 532:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLN: ensure that the VCO output frequency is between 100 and 432 MHz (PLLVCO_output 
 533:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         - PLLP: ensure that max frequency at 216000000 Hz is reached (PLLVCO_output / PLLP)
 534:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  HSEFrequency Value between Min_Data = 4000000 and Max_Data = 26000000
 535:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  HSEBypass This parameter can be one of the following values:
 536:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         @arg @ref LL_UTILS_HSEBYPASS_ON
 537:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *         @arg @ref LL_UTILS_HSEBYPASS_OFF
 538:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_PLLInitStruct pointer to a @ref LL_UTILS_PLLInitTypeDef structure that contains
 539:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the PLL.
 540:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_ClkInitStruct pointer to a @ref LL_UTILS_ClkInitTypeDef structure that contains
 541:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the BUS prescalers.
 542:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval An ErrorStatus enumeration value:
 543:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - SUCCESS: Max frequency configuration done
 544:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - ERROR: Max frequency configuration not done
ARM GAS  /tmp/ccqw5Uyy.s 			page 11


 545:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 546:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** ErrorStatus LL_PLL_ConfigSystemClock_HSE(uint32_t HSEFrequency, uint32_t HSEBypass,
 547:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                          LL_UTILS_PLLInitTypeDef *UTILS_PLLInitStruct, LL_UTILS_Clk
 548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 549:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 550:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t pllfreq = 0U;
 551:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 552:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check the parameters */
 553:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_HSE_FREQUENCY(HSEFrequency));
 554:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_HSE_BYPASS(HSEBypass));
 555:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 556:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check if one of the PLL is enabled */
 557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(UTILS_PLL_IsBusy() == SUCCESS)
 558:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 559:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Calculate the new PLL output frequency */
 560:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     pllfreq = UTILS_GetPLLOutputFrequency(HSEFrequency, UTILS_PLLInitStruct);
 561:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 562:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Enable HSE if not enabled */
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     if(LL_RCC_HSE_IsReady() != 1U)
 564:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 565:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Check if need to enable HSE bypass feature or not */
 566:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       if(HSEBypass == LL_UTILS_HSEBYPASS_ON)
 567:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 568:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         LL_RCC_HSE_EnableBypass();
 569:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 570:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       else
 571:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 572:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         LL_RCC_HSE_DisableBypass();
 573:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 574:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 575:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Enable HSE */
 576:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       LL_RCC_HSE_Enable();
 577:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       while (LL_RCC_HSE_IsReady() != 1U)
 578:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 579:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         /* Wait for HSE ready */
 580:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 581:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 582:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 583:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Configure PLL */
 584:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_PLL_ConfigDomain_SYS(LL_RCC_PLLSOURCE_HSE, UTILS_PLLInitStruct->PLLM, UTILS_PLLInitStruc
 585:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                 UTILS_PLLInitStruct->PLLP);
 586:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 587:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Enable PLL and switch system clock to PLL */
 588:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = UTILS_EnablePLLAndSwitchSystem(pllfreq, UTILS_ClkInitStruct);
 589:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 590:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   else
 591:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 592:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Current PLL configuration cannot be modified */
 593:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 594:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 595:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 596:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return status;
 597:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 598:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 599:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 600:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
 601:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 12


 602:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 603:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 604:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @}
 605:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 606:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 607:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /** @addtogroup UTILS_LL_Private_Functions
 608:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @{
 609:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 610:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 611:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  Function to check that PLL can be modified
 612:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  PLL_InputFrequency  PLL input frequency (in Hz)
 613:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_PLLInitStruct pointer to a @ref LL_UTILS_PLLInitTypeDef structure that contains
 614:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the PLL.
 615:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval PLL output frequency (in Hz)
 616:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 617:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static uint32_t UTILS_GetPLLOutputFrequency(uint32_t PLL_InputFrequency, LL_UTILS_PLLInitTypeDef *U
 618:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
  28              		.loc 1 618 1 view -0
  29              		.cfi_startproc
  30              		@ args = 0, pretend = 0, frame = 0
  31              		@ frame_needed = 0, uses_anonymous_args = 0
  32              		@ link register save eliminated.
 619:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t pllfreq = 0U;
  33              		.loc 1 619 3 view .LVU1
 620:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 621:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check the parameters */
 622:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLLM_VALUE(UTILS_PLLInitStruct->PLLM));
  34              		.loc 1 622 3 view .LVU2
 623:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLLN_VALUE(UTILS_PLLInitStruct->PLLN));
  35              		.loc 1 623 3 view .LVU3
 624:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLLP_VALUE(UTILS_PLLInitStruct->PLLP));
  36              		.loc 1 624 3 view .LVU4
 625:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   
 626:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check different PLL parameters according to RM                          */
 627:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /*  - PLLM: ensure that the VCO input frequency ranges from 0.95 to 2.1 MHz.   */
 628:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   pllfreq = PLL_InputFrequency / (UTILS_PLLInitStruct->PLLM & (RCC_PLLCFGR_PLLM >> RCC_PLLCFGR_PLLM
  37              		.loc 1 628 3 view .LVU5
  38              		.loc 1 628 54 is_stmt 0 view .LVU6
  39 0000 0B68     		ldr	r3, [r1]
  40              		.loc 1 628 61 view .LVU7
  41 0002 03F03F03 		and	r3, r3, #63
  42              		.loc 1 628 11 view .LVU8
  43 0006 B0FBF3F0 		udiv	r0, r0, r3
  44              	.LVL1:
 629:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLLVCO_INPUT(pllfreq));
  45              		.loc 1 629 3 is_stmt 1 view .LVU9
 630:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 631:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /*  - PLLN: ensure that the VCO output frequency is between 100 and 432 MHz.*/
 632:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   pllfreq = pllfreq * (UTILS_PLLInitStruct->PLLN & (RCC_PLLCFGR_PLLN >> RCC_PLLCFGR_PLLN_Pos));
  46              		.loc 1 632 3 view .LVU10
  47              		.loc 1 632 43 is_stmt 0 view .LVU11
  48 000a 4B68     		ldr	r3, [r1, #4]
  49              		.loc 1 632 50 view .LVU12
  50 000c C3F30803 		ubfx	r3, r3, #0, #9
  51              		.loc 1 632 11 view .LVU13
  52 0010 03FB00F0 		mul	r0, r3, r0
  53              	.LVL2:
ARM GAS  /tmp/ccqw5Uyy.s 			page 13


 633:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLLVCO_OUTPUT(pllfreq));
  54              		.loc 1 633 3 is_stmt 1 view .LVU14
 634:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   
 635:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /*  - PLLP: ensure that max frequency at 216000000 Hz is reached     */
 636:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   pllfreq = pllfreq / (((UTILS_PLLInitStruct->PLLP >> RCC_PLLCFGR_PLLP_Pos) + 1) * 2);
  55              		.loc 1 636 3 view .LVU15
  56              		.loc 1 636 52 is_stmt 0 view .LVU16
  57 0014 4B89     		ldrh	r3, [r1, #10]
  58              		.loc 1 636 77 view .LVU17
  59 0016 0133     		adds	r3, r3, #1
  60              		.loc 1 636 82 view .LVU18
  61 0018 5B00     		lsls	r3, r3, #1
  62              	.LVL3:
 637:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_PLL_FREQUENCY(pllfreq));
  63              		.loc 1 637 3 is_stmt 1 view .LVU19
 638:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 639:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return pllfreq;
  64              		.loc 1 639 3 view .LVU20
 640:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
  65              		.loc 1 640 1 is_stmt 0 view .LVU21
  66 001a B0FBF3F0 		udiv	r0, r0, r3
  67              	.LVL4:
  68              		.loc 1 640 1 view .LVU22
  69 001e 7047     		bx	lr
  70              		.cfi_endproc
  71              	.LFE411:
  73              		.section	.text.UTILS_PLL_IsBusy,"ax",%progbits
  74              		.align	1
  75              		.syntax unified
  76              		.thumb
  77              		.thumb_func
  79              	UTILS_PLL_IsBusy:
  80              	.LFB412:
 641:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 642:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 643:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  Function to check that PLL can be modified
 644:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval An ErrorStatus enumeration value:
 645:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - SUCCESS: PLL modification can be done
 646:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - ERROR: PLL is busy
 647:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 648:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static ErrorStatus UTILS_PLL_IsBusy(void)
 649:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
  81              		.loc 1 649 1 is_stmt 1 view -0
  82              		.cfi_startproc
  83              		@ args = 0, pretend = 0, frame = 0
  84              		@ frame_needed = 0, uses_anonymous_args = 0
  85              		@ link register save eliminated.
 650:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
  86              		.loc 1 650 3 view .LVU24
  87              	.LVL5:
 651:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 652:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check if PLL is busy*/
 653:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(LL_RCC_PLL_IsReady() != 0U)
  88              		.loc 1 653 3 view .LVU25
  89              	.LBB54:
  90              	.LBI54:
  91              		.file 2 "Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h"
ARM GAS  /tmp/ccqw5Uyy.s 			page 14


   1:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @file    stm32f7xx_ll_rcc.h
   4:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief   Header file of RCC LL module.
   6:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * This software is licensed under terms that can be found in the LICENSE file in
  13:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   ******************************************************************************
  16:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  17:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  18:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Define to prevent recursive inclusion -------------------------------------*/
  19:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #ifndef __STM32F7xx_LL_RCC_H
  20:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __STM32F7xx_LL_RCC_H
  21:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  22:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #ifdef __cplusplus
  23:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** extern "C" {
  24:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif
  25:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  26:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Includes ------------------------------------------------------------------*/
  27:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #include "stm32f7xx.h"
  28:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  29:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @addtogroup STM32F7xx_LL_Driver
  30:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  31:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  32:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  33:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC)
  34:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  35:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL RCC
  36:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  37:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  38:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  39:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private types -------------------------------------------------------------*/
  40:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private variables ---------------------------------------------------------*/
  41:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Private_Variables RCC Private Variables
  42:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  43:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  44:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  45:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_DCKCFGR1_PLLSAIDIVR)
  46:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** static const uint8_t aRCC_PLLSAIDIVRPrescTable[4] = {2, 4, 8, 16};
  47:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_DCKCFGR1_PLLSAIDIVR */
  48:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  49:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  50:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  51:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  52:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private constants ---------------------------------------------------------*/
  53:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Private macros ------------------------------------------------------------*/
  54:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
  55:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Private_Macros RCC Private Macros
  56:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  57:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 15


  58:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  59:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  60:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  61:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /*USE_FULL_LL_DRIVER*/
  62:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported types ------------------------------------------------------------*/
  63:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
  64:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Types RCC Exported Types
  65:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  66:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  67:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  68:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup LL_ES_CLOCK_FREQ Clocks Frequency Structure
  69:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  70:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  71:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  72:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  73:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  RCC Clocks Frequency Structure
  74:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  75:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** typedef struct
  76:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
  77:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t SYSCLK_Frequency;        /*!< SYSCLK clock frequency */
  78:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t HCLK_Frequency;          /*!< HCLK clock frequency */
  79:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t PCLK1_Frequency;         /*!< PCLK1 clock frequency */
  80:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   uint32_t PCLK2_Frequency;         /*!< PCLK2 clock frequency */
  81:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** } LL_RCC_ClocksTypeDef;
  82:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  83:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  84:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  85:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  86:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  87:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
  88:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
  89:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  90:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* USE_FULL_LL_DRIVER */
  91:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  92:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported constants --------------------------------------------------------*/
  93:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Constants RCC Exported Constants
  94:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
  95:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
  96:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
  97:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_OSC_VALUES Oscillator Values adaptation
  98:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Defines used to adapt values of different oscillators
  99:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note     These values could be modified in the user environment according to 
 100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *           HW set-up.
 101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (HSE_VALUE)
 104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define HSE_VALUE    25000000U  /*!< Value of the HSE oscillator in Hz */
 105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* HSE_VALUE */
 106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (HSI_VALUE)
 108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define HSI_VALUE    16000000U  /*!< Value of the HSI oscillator in Hz */
 109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* HSI_VALUE */
 110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (LSE_VALUE)
 112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LSE_VALUE    32768U     /*!< Value of the LSE oscillator in Hz */
 113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LSE_VALUE */
 114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 16


 115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (LSI_VALUE)
 116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LSI_VALUE    32000U     /*!< Value of the LSI oscillator in Hz */
 117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LSI_VALUE */
 118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined  (EXTERNAL_CLOCK_VALUE)
 120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_CLOCK_VALUE    12288000U /*!< Value of the I2S_CKIN external oscillator in Hz */
 121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_CLOCK_VALUE */
 122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined (EXTERNAL_SAI1_CLOCK_VALUE)
 124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_SAI1_CLOCK_VALUE    48000U /*!< Value of the SAI1_EXTCLK external oscillator in Hz
 125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_SAI1_CLOCK_VALUE */
 126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if !defined (EXTERNAL_SAI2_CLOCK_VALUE)
 128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define EXTERNAL_SAI2_CLOCK_VALUE    48000U /*!< Value of the SAI2_EXTCLK external oscillator in Hz
 129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* EXTERNAL_SAI2_CLOCK_VALUE */
 130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CLEAR_FLAG Clear Flags Defines
 135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Flags defines which can be used with LL_RCC_WriteReg function
 136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYC                RCC_CIR_LSIRDYC     /*!< LSI Ready Interrupt Clear */
 139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYC                RCC_CIR_LSERDYC     /*!< LSE Ready Interrupt Clear */
 140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYC                RCC_CIR_HSIRDYC     /*!< HSI Ready Interrupt Clear */
 141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYC                RCC_CIR_HSERDYC     /*!< HSE Ready Interrupt Clear */
 142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYC                RCC_CIR_PLLRDYC     /*!< PLL Ready Interrupt Clear */
 143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYC             RCC_CIR_PLLI2SRDYC  /*!< PLLI2S Ready Interrupt Clear */
 144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYC             RCC_CIR_PLLSAIRDYC  /*!< PLLSAI Ready Interrupt Clear */
 145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_CSSC                   RCC_CIR_CSSC        /*!< Clock Security System Interrupt 
 146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_GET_FLAG Get Flags Defines
 151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    Flags defines which can be used with LL_RCC_ReadReg function
 152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYF                RCC_CIR_LSIRDYF     /*!< LSI Ready Interrupt flag */
 155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYF                RCC_CIR_LSERDYF     /*!< LSE Ready Interrupt flag */
 156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYF                RCC_CIR_HSIRDYF     /*!< HSI Ready Interrupt flag */
 157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYF                RCC_CIR_HSERDYF     /*!< HSE Ready Interrupt flag */
 158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYF                RCC_CIR_PLLRDYF     /*!< PLL Ready Interrupt flag */
 159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYF             RCC_CIR_PLLI2SRDYF  /*!< PLLI2S Ready Interrupt flag */
 160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYF             RCC_CIR_PLLSAIRDYF  /*!< PLLSAI Ready Interrupt flag */
 161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_CSSF                   RCC_CIR_CSSF        /*!< Clock Security System Interrupt 
 162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_LPWRRSTF                RCC_CSR_LPWRRSTF   /*!< Low-Power reset flag */
 163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_PINRSTF                 RCC_CSR_PINRSTF    /*!< PIN reset flag */
 164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_PORRSTF                 RCC_CSR_PORRSTF    /*!< POR/PDR reset flag */
 165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_SFTRSTF                 RCC_CSR_SFTRSTF    /*!< Software Reset flag */
 166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_IWDGRSTF                RCC_CSR_IWDGRSTF   /*!< Independent Watchdog reset flag 
 167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_WWDGRSTF                RCC_CSR_WWDGRSTF   /*!< Window watchdog reset flag */
 168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CSR_BORRSTF                 RCC_CSR_BORRSTF    /*!< BOR reset flag */
 169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 17


 172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_IT IT Defines
 174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief    IT defines which can be used with LL_RCC_ReadReg and  LL_RCC_WriteReg functions
 175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSIRDYIE               RCC_CIR_LSIRDYIE      /*!< LSI Ready Interrupt Enable */
 178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_LSERDYIE               RCC_CIR_LSERDYIE      /*!< LSE Ready Interrupt Enable */
 179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSIRDYIE               RCC_CIR_HSIRDYIE      /*!< HSI Ready Interrupt Enable */
 180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_HSERDYIE               RCC_CIR_HSERDYIE      /*!< HSE Ready Interrupt Enable */
 181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLRDYIE               RCC_CIR_PLLRDYIE      /*!< PLL Ready Interrupt Enable */
 182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLI2SRDYIE            RCC_CIR_PLLI2SRDYIE   /*!< PLLI2S Ready Interrupt Enable 
 183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CIR_PLLSAIRDYIE            RCC_CIR_PLLSAIRDYIE   /*!< PLLSAI Ready Interrupt Enable 
 184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LSEDRIVE  LSE oscillator drive capability
 189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_LOW                0x00000000U             /*!< Xtal mode lower driving cap
 192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_MEDIUMHIGH         RCC_BDCR_LSEDRV_0       /*!< Xtal mode medium high drivi
 193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_MEDIUMLOW          RCC_BDCR_LSEDRV_1       /*!< Xtal mode medium low drivin
 194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LSEDRIVE_HIGH               RCC_BDCR_LSEDRV         /*!< Xtal mode higher driving ca
 195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYS_CLKSOURCE  System clock switch
 200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_HSI           RCC_CFGR_SW_HSI    /*!< HSI selection as system clock */
 203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_HSE           RCC_CFGR_SW_HSE    /*!< HSE selection as system clock */
 204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_PLL           RCC_CFGR_SW_PLL    /*!< PLL selection as system clock */
 205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYS_CLKSOURCE_STATUS  System clock switch status
 210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_HSI    RCC_CFGR_SWS_HSI   /*!< HSI used as system clock */
 213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_HSE    RCC_CFGR_SWS_HSE   /*!< HSE used as system clock */
 214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYS_CLKSOURCE_STATUS_PLL    RCC_CFGR_SWS_PLL   /*!< PLL used as system clock */
 215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SYSCLK_DIV  AHB prescaler
 220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_1                RCC_CFGR_HPRE_DIV1   /*!< SYSCLK not divided */
 223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_2                RCC_CFGR_HPRE_DIV2   /*!< SYSCLK divided by 2 */
 224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_4                RCC_CFGR_HPRE_DIV4   /*!< SYSCLK divided by 4 */
 225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_8                RCC_CFGR_HPRE_DIV8   /*!< SYSCLK divided by 8 */
 226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_16               RCC_CFGR_HPRE_DIV16  /*!< SYSCLK divided by 16 */
 227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_64               RCC_CFGR_HPRE_DIV64  /*!< SYSCLK divided by 64 */
 228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_128              RCC_CFGR_HPRE_DIV128 /*!< SYSCLK divided by 128 */
ARM GAS  /tmp/ccqw5Uyy.s 			page 18


 229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_256              RCC_CFGR_HPRE_DIV256 /*!< SYSCLK divided by 256 */
 230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SYSCLK_DIV_512              RCC_CFGR_HPRE_DIV512 /*!< SYSCLK divided by 512 */
 231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_APB1_DIV  APB low-speed prescaler (APB1)
 236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_1                  RCC_CFGR_PPRE1_DIV1  /*!< HCLK not divided */
 239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_2                  RCC_CFGR_PPRE1_DIV2  /*!< HCLK divided by 2 */
 240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_4                  RCC_CFGR_PPRE1_DIV4  /*!< HCLK divided by 4 */
 241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_8                  RCC_CFGR_PPRE1_DIV8  /*!< HCLK divided by 8 */
 242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB1_DIV_16                 RCC_CFGR_PPRE1_DIV16 /*!< HCLK divided by 16 */
 243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_APB2_DIV  APB high-speed prescaler (APB2)
 247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_1                  RCC_CFGR_PPRE2_DIV1  /*!< HCLK not divided */
 250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_2                  RCC_CFGR_PPRE2_DIV2  /*!< HCLK divided by 2 */
 251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_4                  RCC_CFGR_PPRE2_DIV4  /*!< HCLK divided by 4 */
 252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_8                  RCC_CFGR_PPRE2_DIV8  /*!< HCLK divided by 8 */
 253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_APB2_DIV_16                 RCC_CFGR_PPRE2_DIV16 /*!< HCLK divided by 16 */
 254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_MCOxSOURCE  MCO source selection
 259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_HSI              (uint32_t)(RCC_CFGR_MCO1|0x00000000U)                   
 262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_LSE              (uint32_t)(RCC_CFGR_MCO1|(RCC_CFGR_MCO1_0 >> 16U))      
 263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_HSE              (uint32_t)(RCC_CFGR_MCO1|(RCC_CFGR_MCO1_1 >> 16U))      
 264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1SOURCE_PLLCLK           (uint32_t)(RCC_CFGR_MCO1|((RCC_CFGR_MCO1_1|RCC_CFGR_MCO1
 265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_SYSCLK           (uint32_t)(RCC_CFGR_MCO2|0x00000000U)                   
 266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_PLLI2S           (uint32_t)(RCC_CFGR_MCO2|(RCC_CFGR_MCO2_0 >> 16U))      
 267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_HSE              (uint32_t)(RCC_CFGR_MCO2|(RCC_CFGR_MCO2_1 >> 16U))      
 268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2SOURCE_PLLCLK           (uint32_t)(RCC_CFGR_MCO2|((RCC_CFGR_MCO2_1|RCC_CFGR_MCO2
 269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_MCOx_DIV  MCO prescaler
 274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_1                  (uint32_t)(RCC_CFGR_MCO1PRE|0x00000000U)                
 277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_2                  (uint32_t)(RCC_CFGR_MCO1PRE|(RCC_CFGR_MCO1PRE_2 >> 16U))
 278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_3                  (uint32_t)(RCC_CFGR_MCO1PRE|((RCC_CFGR_MCO1PRE_2|RCC_CFG
 279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_4                  (uint32_t)(RCC_CFGR_MCO1PRE|((RCC_CFGR_MCO1PRE_2|RCC_CFG
 280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO1_DIV_5                  (uint32_t)(RCC_CFGR_MCO1PRE|(RCC_CFGR_MCO1PRE >> 16U))  
 281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_1                  (uint32_t)(RCC_CFGR_MCO2PRE|0x00000000U)                
 282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_2                  (uint32_t)(RCC_CFGR_MCO2PRE|(RCC_CFGR_MCO2PRE_2 >> 16U))
 283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_3                  (uint32_t)(RCC_CFGR_MCO2PRE|((RCC_CFGR_MCO2PRE_2|RCC_CFG
 284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_4                  (uint32_t)(RCC_CFGR_MCO2PRE|((RCC_CFGR_MCO2PRE_2|RCC_CFG
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_MCO2_DIV_5                  (uint32_t)(RCC_CFGR_MCO2PRE|(RCC_CFGR_MCO2PRE >> 16U))  
ARM GAS  /tmp/ccqw5Uyy.s 			page 19


 286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RTC_HSEDIV  HSE prescaler for RTC clock
 291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_NOCLOCK                  0x00000000U             /*!< HSE not divided */
 294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_2                RCC_CFGR_RTCPRE_1       /*!< HSE clock divided by 2 */
 295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_3                (RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_4                RCC_CFGR_RTCPRE_2       /*!< HSE clock divided by 4 */
 297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_5                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_6                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_7                (RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_8                RCC_CFGR_RTCPRE_3       /*!< HSE clock divided by 8 */
 301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_9                (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_10               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_11               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_12               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2)       /*!< HSE cl
 305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_13               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)
 306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_14               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)
 307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_15               (RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|
 308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_16               RCC_CFGR_RTCPRE_4       /*!< HSE clock divided by 16 */
 309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_17               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_0)       /*!< HSE cl
 310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_18               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_1)       /*!< HSE cl
 311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_19               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_1|RCC_CFGR_RTCPRE_0)
 312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_20               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2)       /*!< HSE cl
 313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_21               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_0)
 314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_22               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1)
 315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_23               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_2|RCC_CFGR_RTCPRE_1|
 316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_24               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3)       /*!< HSE cl
 317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_25               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_0)
 318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_26               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1)
 319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_27               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_1|
 320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_28               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2)
 321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_29               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_30               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_HSE_DIV_31               (RCC_CFGR_RTCPRE_4|RCC_CFGR_RTCPRE_3|RCC_CFGR_RTCPRE_2|
 324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(USE_FULL_LL_DRIVER)
 329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PERIPH_FREQUENCY Peripheral clock frequency
 330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PERIPH_FREQUENCY_NO         0x00000000U                 /*!< No clock enabled for th
 333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PERIPH_FREQUENCY_NA         0xFFFFFFFFU                 /*!< Frequency cannot be pro
 334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* USE_FULL_LL_DRIVER */
 338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USARTx_CLKSOURCE  Peripheral USART clock source selection
 340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_PCLK2      (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | 0x00000000U
ARM GAS  /tmp/ccqw5Uyy.s 			page 20


 343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART1SEL << 16U) | RCC_DCKCFGR
 346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | 0x00000000U
 347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART2SEL << 16U) | RCC_DCKCFGR
 350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | 0x00000000U
 351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART3SEL << 16U) | RCC_DCKCFGR
 354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_PCLK2      (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | 0x00000000U
 355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_USART6SEL << 16U) | RCC_DCKCFGR
 358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_UARTx_CLKSOURCE  Peripheral UART clock source selection
 363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | 0x00000000U) 
 366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART4SEL << 16U) | RCC_DCKCFGR2_
 369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | 0x00000000U) 
 370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART5SEL << 16U) | RCC_DCKCFGR2_
 373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | 0x00000000U) 
 374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART7SEL << 16U) | RCC_DCKCFGR2_
 377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_PCLK1      (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | 0x00000000U) 
 378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_SYSCLK     (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_HSI        (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE_LSE        (uint32_t)((RCC_DCKCFGR2_UART8SEL << 16U) | RCC_DCKCFGR2_
 381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2Cx_CLKSOURCE  Peripheral I2C clock source selection
 386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C1SEL|0x00000000U) /*!< PCLK1 
 389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C1SEL|(RCC_DCKCFGR2_I2C1SEL_0 
 390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C1SEL|(RCC_DCKCFGR2_I2C1SEL_1 
 391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C2SEL|0x00000000U) /*!< PCLK1 
 392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C2SEL|(RCC_DCKCFGR2_I2C2SEL_0 
 393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C2SEL|(RCC_DCKCFGR2_I2C2SEL_1 
 394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C3SEL|0x00000000U) /*!< PCLK1 
 395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C3SEL|(RCC_DCKCFGR2_I2C3SEL_0 
 396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C3SEL|(RCC_DCKCFGR2_I2C3SEL_1 
 397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(I2C4)
 398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_PCLK1        (uint32_t)(RCC_DCKCFGR2_I2C4SEL|0x00000000U) /*!< PCLK1 
 399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_SYSCLK       (uint32_t)(RCC_DCKCFGR2_I2C4SEL|(RCC_DCKCFGR2_I2C4SEL_0 
ARM GAS  /tmp/ccqw5Uyy.s 			page 21


 400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE_HSI          (uint32_t)(RCC_DCKCFGR2_I2C4SEL|(RCC_DCKCFGR2_I2C4SEL_1 
 401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* I2C4 */
 402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LPTIM1_CLKSOURCE  Peripheral LPTIM clock source selection
 407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_PCLK1       0x00000000U                 /*!< PCLK1 clock used as LP
 410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_LSI         RCC_DCKCFGR2_LPTIM1SEL_0    /*!< LSI oscillator clock u
 411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_HSI         RCC_DCKCFGR2_LPTIM1SEL_1    /*!< HSI oscillator clock u
 412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE_LSE         (uint32_t)(RCC_DCKCFGR2_LPTIM1SEL_1 | RCC_DCKCFGR2_LPTI
 413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SAIx_CLKSOURCE  Peripheral SAI clock source selection
 418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLSAI       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | 0x00000000U)          
 421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLI2S       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL_
 422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PIN          (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL_
 423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_SAI1SEL_PLLSRC_SUPPORT)
 424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE_PLLSRC       (uint32_t)(RCC_DCKCFGR1_SAI1SEL | (RCC_DCKCFGR1_SAI1SEL 
 425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_SAI1SEL_PLLSRC_SUPPORT */
 426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLSAI       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | 0x00000000U)          
 427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLI2S       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL_
 428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PIN          (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL_
 429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_SAI2SEL_PLLSRC_SUPPORT)
 430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE_PLLSRC       (uint32_t)(RCC_DCKCFGR1_SAI2SEL | (RCC_DCKCFGR1_SAI2SEL 
 431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_SAI2SEL_PLLSRC_SUPPORT */
 432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SDMMCx_CLKSOURCE  Peripheral SDMMC clock source selection
 437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK       (uint32_t)(RCC_DCKCFGR2_SDMMC1SEL | 0x00000000U)    
 440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE_SYSCLK         (uint32_t)(RCC_DCKCFGR2_SDMMC1SEL | (RCC_DCKCFGR2_SD
 441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SDMMC2)
 442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK       (uint32_t)(RCC_DCKCFGR2_SDMMC2SEL | 0x00000000U)    
 443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE_SYSCLK         (uint32_t)(RCC_DCKCFGR2_SDMMC2SEL | (RCC_DCKCFGR2_SD
 444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SDMMC2 */
 445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RNG_CLKSOURCE  Peripheral RNG clock source selection
 450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE_PLL          0x00000000U            /*!< PLL clock used as RNG clock s
 453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE_PLLSAI       RCC_DCKCFGR2_CK48MSEL  /*!< PLLSAI clock used as RNG cloc
 454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 22


 457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USB_CLKSOURCE  Peripheral USB clock source selection
 459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE_PLL          0x00000000U            /*!< PLL clock used as USB clock s
 462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE_PLLSAI       RCC_DCKCFGR2_CK48MSEL  /*!< PLLSAI1 clock used as USB clo
 463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
 468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DSI_CLKSOURCE  Peripheral DSI clock source selection
 469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE_PHY          0x00000000U           /*!< DSI-PHY clock used as DSI byte
 472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE_PLL          RCC_DCKCFGR2_DSISEL   /*!< PLL clock used as DSI byte lan
 473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
 477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
 479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CEC_CLKSOURCE  Peripheral CEC clock source selection
 480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE_LSE               0x00000000U                /*!< LSE oscillator clock
 483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE_HSI_DIV488        RCC_DCKCFGR2_CECSEL        /*!< HSI oscillator clock
 484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
 488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2S1_CLKSOURCE  Peripheral I2S clock source selection
 490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE_PLLI2S           0x00000000U                /*!< I2S oscillator clock
 493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE_PIN              RCC_CFGR_I2SSRC            /*!< External pin clock u
 494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CK48M_CLKSOURCE  Peripheral 48Mhz domain clock source selection
 499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE_PLL             0x00000000U                /*!< PLL oscillator clock
 502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE_PLLSAI          RCC_DCKCFGR2_CK48MSEL      /*!< PLLSAI oscillator cl
 503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
 508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM1_AUDIO_CLKSOURCE  Peripheral DFSDM Audio clock source selection
 509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1     0x00000000U                /*!< SAI1 clock used as D
 512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2     RCC_DCKCFGR1_ADFSDM1SEL    /*!< SAI2 clock used as D
 513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/ccqw5Uyy.s 			page 23


 514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM1_CLKSOURCE  Peripheral DFSDM clock source selection
 518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE_PCLK2          0x00000000U                /*!< PCLK2 clock used as 
 521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE_SYSCLK         RCC_DCKCFGR1_DFSDM1SEL     /*!< System clock used as
 522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
 526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USARTx  Peripheral USART get clock source
 528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART1_CLKSOURCE            RCC_DCKCFGR2_USART1SEL /*!< USART1 Clock source selectio
 531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART2_CLKSOURCE            RCC_DCKCFGR2_USART2SEL /*!< USART2 Clock source selectio
 532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART3_CLKSOURCE            RCC_DCKCFGR2_USART3SEL /*!< USART3 Clock source selectio
 533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USART6_CLKSOURCE            RCC_DCKCFGR2_USART6SEL /*!< USART6 Clock source selectio
 534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_UARTx  Peripheral UART get clock source
 539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART4_CLKSOURCE             RCC_DCKCFGR2_UART4SEL /*!< UART4 Clock source selection 
 542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART5_CLKSOURCE             RCC_DCKCFGR2_UART5SEL /*!< UART5 Clock source selection 
 543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART7_CLKSOURCE             RCC_DCKCFGR2_UART7SEL /*!< UART7 Clock source selection 
 544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_UART8_CLKSOURCE             RCC_DCKCFGR2_UART8SEL /*!< UART8 Clock source selection 
 545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2Cx  Peripheral I2C get clock source
 550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C1_CLKSOURCE              RCC_DCKCFGR2_I2C1SEL  /*!< I2C1 Clock source selection *
 553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C2_CLKSOURCE              RCC_DCKCFGR2_I2C2SEL  /*!< I2C2 Clock source selection *
 554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C3_CLKSOURCE              RCC_DCKCFGR2_I2C3SEL  /*!< I2C3 Clock source selection *
 555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(I2C4)
 556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2C4_CLKSOURCE              RCC_DCKCFGR2_I2C4SEL  /*!< I2C4 Clock source selection *
 557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* I2C4 */
 558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LPTIM1  Peripheral LPTIM get clock source
 563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LPTIM1_CLKSOURCE            RCC_DCKCFGR2_LPTIM1SEL /*!< LPTIM1 Clock source selectio
 566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SAIx  Peripheral SAI get clock source
ARM GAS  /tmp/ccqw5Uyy.s 			page 24


 571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI1_CLKSOURCE              RCC_DCKCFGR1_SAI1SEL /*!< SAI1 Clock source selection */
 574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SAI2_CLKSOURCE              RCC_DCKCFGR1_SAI2SEL /*!< SAI2 Clock source selection */
 575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SDMMCx  Peripheral SDMMC get clock source
 580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC1_CLKSOURCE            RCC_DCKCFGR2_SDMMC1SEL /*!< SDMMC1 Clock source selectio
 583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SDMMC2)
 584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SDMMC2_CLKSOURCE            RCC_DCKCFGR2_SDMMC2SEL /*!< SDMMC2 Clock source selectio
 585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SDMMC2 */
 586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CK48M  Peripheral CK48M get clock source
 591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CK48M_CLKSOURCE             RCC_DCKCFGR2_CK48MSEL /*!< CK48M Domain clock source sel
 594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RNG  Peripheral RNG get clock source
 599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RNG_CLKSOURCE               RCC_DCKCFGR2_CK48MSEL /*!< RNG Clock source selection */
 602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_USB  Peripheral USB get clock source
 607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_USB_CLKSOURCE               RCC_DCKCFGR2_CK48MSEL /*!< USB Clock source selection */
 610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
 615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_CEC  Peripheral CEC get clock source
 616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_CEC_CLKSOURCE               RCC_DCKCFGR2_CECSEL /*!< CEC Clock source selection */
 619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
 623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_I2S1  Peripheral I2S get clock source
 625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_I2S1_CLKSOURCE              RCC_CFGR_I2SSRC /*!< I2S Clock source selection */
ARM GAS  /tmp/ccqw5Uyy.s 			page 25


 628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
 632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM_AUDIO  Peripheral DFSDM Audio get clock source
 633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_AUDIO_CLKSOURCE      RCC_DCKCFGR1_ADFSDM1SEL /*!< DFSDM Audio Clock source se
 636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DFSDM  Peripheral DFSDM get clock source
 641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DFSDM1_CLKSOURCE            RCC_DCKCFGR1_DFSDM1SEL /*!< DFSDM Clock source selection
 644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
 648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
 650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_DSI  Peripheral DSI get clock source
 651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_DSI_CLKSOURCE               RCC_DCKCFGR2_DSISEL /*!< DSI Clock source selection */
 654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
 658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(LTDC)
 660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_LTDC  Peripheral LTDC get clock source
 661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_LTDC_CLKSOURCE              RCC_DCKCFGR1_PLLSAIDIVR /*!< LTDC Clock source selection
 664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LTDC */
 668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
 670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_SPDIFRX  Peripheral SPDIFRX get clock source
 671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPDIFRX1_CLKSOURCE           RCC_PLLI2SCFGR_PLLI2SP /*!< SPDIFRX Clock source select
 674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
 678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_RTC_CLKSOURCE  RTC clock source selection
 680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_NONE          0x00000000U             /*!< No clock used as RTC clock 
 683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_LSE           RCC_BDCR_RTCSEL_0       /*!< LSE oscillator clock used a
 684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_LSI           RCC_BDCR_RTCSEL_1       /*!< LSI oscillator clock used a
ARM GAS  /tmp/ccqw5Uyy.s 			page 26


 685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_RTC_CLKSOURCE_HSE           RCC_BDCR_RTCSEL         /*!< HSE oscillator clock divide
 686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_TIM_CLKPRESCALER  Timers clocks prescalers selection
 691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_TIM_PRESCALER_TWICE          0x00000000U                  /*!< Timers clock to twice
 694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_TIM_PRESCALER_FOUR_TIMES     RCC_DCKCFGR1_TIMPRE          /*!< Timers clock to four 
 695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSOURCE  PLL, PLLI2S and PLLSAI entry clock source
 700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSOURCE_HSI               RCC_PLLCFGR_PLLSRC_HSI  /*!< HSI16 clock selected as PLL
 703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSOURCE_HSE               RCC_PLLCFGR_PLLSRC_HSE  /*!< HSE clock selected as PLL e
 704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLM_DIV  PLL, PLLI2S and PLLSAI division factor
 709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_2                  (RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI2S and PLLSAI divisio
 712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_3                  (RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_4                  (RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI2S and PLLSAI divisio
 714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_5                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_6                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_7                  (RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_8                  (RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI2S and PLLSAI divisio
 718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_9                  (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_10                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_11                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_12                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_13                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_14                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_15                 (RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_16                 (RCC_PLLCFGR_PLLM_4) /*!< PLL, PLLI2S and PLLSAI divisio
 726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_17                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_18                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_19                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_20                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_21                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_22                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_23                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_24                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI
 734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_25                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_26                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_27                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_28                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_29                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_30                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_31                 (RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_32                 (RCC_PLLCFGR_PLLM_5) /*!< PLL, PLLI2S and PLLSAI divisio
ARM GAS  /tmp/ccqw5Uyy.s 			page 27


 742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_33                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_0) /*!< PLL, PLLI
 743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_34                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_1) /*!< PLL, PLLI
 744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_35                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_1 | RCC_PLLCFGR_P
 745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_36                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2) /*!< PLL, PLLI
 746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_37                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_38                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_39                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_2 | RCC_PLLCFGR_P
 749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_40                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3) /*!< PLL, PLLI
 750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_41                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_42                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_43                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_44                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_45                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_46                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_47                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_3 | RCC_PLLCFGR_P
 757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_48                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4) /*!< PLL, PLLI
 758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_49                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_50                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_51                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_52                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_53                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_54                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_55                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_56                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_57                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_58                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_59                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_60                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_61                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_62                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLM_DIV_63                 (RCC_PLLCFGR_PLLM_5 | RCC_PLLCFGR_PLLM_4 | RCC_PLLCFGR_P
 773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLCFGR_PLLR)
 778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLR_DIV  PLL division factor (PLLR)
 779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_2                  (RCC_PLLCFGR_PLLR_1)                     /*!< Main PLL d
 782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_3                  (RCC_PLLCFGR_PLLR_1|RCC_PLLCFGR_PLLR_0)  /*!< Main PLL d
 783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_4                  (RCC_PLLCFGR_PLLR_2)                     /*!< Main PLL d
 784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_5                  (RCC_PLLCFGR_PLLR_2|RCC_PLLCFGR_PLLR_0)  /*!< Main PLL d
 785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_6                  (RCC_PLLCFGR_PLLR_2|RCC_PLLCFGR_PLLR_1)  /*!< Main PLL d
 786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLR_DIV_7                  (RCC_PLLCFGR_PLLR)                       /*!< Main PLL d
 787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLCFGR_PLLR */
 791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLP_DIV  PLL division factor (PLLP)
 793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_2                  0x00000000U            /*!< Main PLL division factor for
 796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_4                  RCC_PLLCFGR_PLLP_0     /*!< Main PLL division factor for
 797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_6                  RCC_PLLCFGR_PLLP_1     /*!< Main PLL division factor for
 798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLP_DIV_8                  (RCC_PLLCFGR_PLLP_1 | RCC_PLLCFGR_PLLP_0)   /*!< Main PL
ARM GAS  /tmp/ccqw5Uyy.s 			page 28


 799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLQ_DIV  PLL division factor (PLLQ)
 804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_2                  RCC_PLLCFGR_PLLQ_1                      /*!< Main PLL di
 807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_3                  (RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_4                  RCC_PLLCFGR_PLLQ_2                      /*!< Main PLL di
 809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_5                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_6                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_1) /*!< Main PLL di
 811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_7                  (RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_
 812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_8                  RCC_PLLCFGR_PLLQ_3                      /*!< Main PLL di
 813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_9                  (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_0) /*!< Main PLL di
 814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_10                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_1) /*!< Main PLL di
 815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_11                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_1|RCC_PLLCFGR_PLLQ_
 816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_12                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2) /*!< Main PLL di
 817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_13                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_14                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLQ_DIV_15                 (RCC_PLLCFGR_PLLQ_3|RCC_PLLCFGR_PLLQ_2|RCC_PLLCFGR_PLLQ_
 820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLL_SPRE_SEL  PLL Spread Spectrum Selection
 825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPREAD_SELECT_CENTER        0x00000000U                   /*!< PLL center spread spe
 828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_SPREAD_SELECT_DOWN          RCC_SSCGR_SPREADSEL           /*!< PLL down spread spect
 829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SQ  PLLI2SQ division factor (PLLI2SQ)
 834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_2              RCC_PLLI2SCFGR_PLLI2SQ_1        /*!< PLLI2S division fact
 837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_3              (RCC_PLLI2SCFGR_PLLI2SQ_1 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_4              RCC_PLLI2SCFGR_PLLI2SQ_2        /*!< PLLI2S division fact
 839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_5              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_6              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_1)    
 841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_7              (RCC_PLLI2SCFGR_PLLI2SQ_2 | RCC_PLLI2SCFGR_PLLI2SQ_1 | RC
 842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_8              RCC_PLLI2SCFGR_PLLI2SQ_3        /*!< PLLI2S division fact
 843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_9              (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_0)    
 844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_10             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_1)    
 845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_11             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_1 | RC
 846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_12             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2)    
 847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_13             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_14             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SQ_DIV_15             (RCC_PLLI2SCFGR_PLLI2SQ_3 | RCC_PLLI2SCFGR_PLLI2SQ_2 | RC
 850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SDIVQ  PLLI2SDIVQ division factor (PLLI2SDIVQ)
 855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
ARM GAS  /tmp/ccqw5Uyy.s 			page 29


 856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_1           0x00000000U                        /*!< PLLI2S division f
 858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_2           RCC_DCKCFGR1_PLLI2SDIVQ_0          /*!< PLLI2S division f
 859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_3           RCC_DCKCFGR1_PLLI2SDIVQ_1          /*!< PLLI2S division f
 860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_4           (RCC_DCKCFGR1_PLLI2SDIVQ_1 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_5           RCC_DCKCFGR1_PLLI2SDIVQ_2          /*!< PLLI2S division f
 862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_6           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_7           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_8           (RCC_DCKCFGR1_PLLI2SDIVQ_2 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_9           RCC_DCKCFGR1_PLLI2SDIVQ_3          /*!< PLLI2S division f
 866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_10          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_11          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_12          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_13          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2)  
 870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_14          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_15          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_16          (RCC_DCKCFGR1_PLLI2SDIVQ_3 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_17          RCC_DCKCFGR1_PLLI2SDIVQ_4          /*!< PLLI2S division f
 874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_18          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_0)  
 875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_19          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_1)  
 876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_20          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_1 | 
 877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_21          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2)  
 878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_22          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_23          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_24          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_2 | 
 881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_25          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3)  
 882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_26          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_27          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_28          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_29          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_30          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_31          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SDIVQ_DIV_32          (RCC_DCKCFGR1_PLLI2SDIVQ_4 | RCC_DCKCFGR1_PLLI2SDIVQ_3 | 
 889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SR  PLLI2SR division factor (PLLI2SR)
 894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_2              RCC_PLLI2SCFGR_PLLI2SR_1                                 
 897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_3              (RCC_PLLI2SCFGR_PLLI2SR_1 | RCC_PLLI2SCFGR_PLLI2SR_0)    
 898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_4              RCC_PLLI2SCFGR_PLLI2SR_2                                 
 899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_5              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_0)    
 900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_6              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_1)    
 901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SR_DIV_7              (RCC_PLLI2SCFGR_PLLI2SR_2 | RCC_PLLI2SCFGR_PLLI2SR_1 | RC
 902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLI2SCFGR_PLLI2SP)
 907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLI2SP  PLLI2SP division factor (PLLI2SP)
 908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_2              0x00000000U            /*!< PLLI2S division factor for PL
 911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_4              RCC_PLLI2SCFGR_PLLI2SP_0        /*!< PLLI2S division fact
 912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_6              RCC_PLLI2SCFGR_PLLI2SP_1        /*!< PLLI2S division fact
ARM GAS  /tmp/ccqw5Uyy.s 			page 30


 913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLI2SP_DIV_8              (RCC_PLLI2SCFGR_PLLI2SP_1 | RCC_PLLI2SCFGR_PLLI2SP_0)    
 914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLI2SCFGR_PLLI2SP */
 918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIQ  PLLSAIQ division factor (PLLSAIQ)
 920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_2              RCC_PLLSAICFGR_PLLSAIQ_1        /*!< PLLSAI division fact
 923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_3              (RCC_PLLSAICFGR_PLLSAIQ_1 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_4              RCC_PLLSAICFGR_PLLSAIQ_2        /*!< PLLSAI division fact
 925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_5              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_6              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_1)    
 927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_7              (RCC_PLLSAICFGR_PLLSAIQ_2 | RCC_PLLSAICFGR_PLLSAIQ_1 | RC
 928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_8              RCC_PLLSAICFGR_PLLSAIQ_3        /*!< PLLSAI division fact
 929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_9              (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_0)    
 930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_10             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_1)    
 931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_11             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_1 | RC
 932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_12             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2)    
 933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_13             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
 934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_14             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
 935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIQ_DIV_15             (RCC_PLLSAICFGR_PLLSAIQ_3 | RCC_PLLSAICFGR_PLLSAIQ_2 | RC
 936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIDIVQ  PLLSAIDIVQ division factor (PLLSAIDIVQ)
 941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_1           0x00000000U               /*!< PLLSAI division factor for
 944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_2           RCC_DCKCFGR1_PLLSAIDIVQ_0          /*!< PLLSAI division f
 945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_3           RCC_DCKCFGR1_PLLSAIDIVQ_1          /*!< PLLSAI division f
 946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_4           (RCC_DCKCFGR1_PLLSAIDIVQ_1 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_5           RCC_DCKCFGR1_PLLSAIDIVQ_2          /*!< PLLSAI division f
 948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_6           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_7           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_8           (RCC_DCKCFGR1_PLLSAIDIVQ_2 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_9           RCC_DCKCFGR1_PLLSAIDIVQ_3          /*!< PLLSAI division f
 952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_10          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_11          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_12          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_13          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2)  
 956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_14          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_15          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_16          (RCC_DCKCFGR1_PLLSAIDIVQ_3 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_17          RCC_DCKCFGR1_PLLSAIDIVQ_4         /*!< PLLSAI division fa
 960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_18          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_0)  
 961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_19          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_1)  
 962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_20          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_1 | 
 963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_21          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2)  
 964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_22          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_23          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_24          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_2 | 
 967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_25          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3)  
 968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_26          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_27          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
ARM GAS  /tmp/ccqw5Uyy.s 			page 31


 970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_28          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_29          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_30          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_31          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVQ_DIV_32          (RCC_DCKCFGR1_PLLSAIDIVQ_4 | RCC_DCKCFGR1_PLLSAIDIVQ_3 | 
 975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLSAICFGR_PLLSAIR)
 980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIR  PLLSAIR division factor (PLLSAIR)
 981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_2              RCC_PLLSAICFGR_PLLSAIR_1                                 
 984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_3              (RCC_PLLSAICFGR_PLLSAIR_1 | RCC_PLLSAICFGR_PLLSAIR_0)    
 985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_4              RCC_PLLSAICFGR_PLLSAIR_2                                 
 986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_5              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_0)    
 987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_6              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_1)    
 988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIR_DIV_7              (RCC_PLLSAICFGR_PLLSAIR_2 | RCC_PLLSAICFGR_PLLSAIR_1 | RC
 989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
 990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
 991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLSAICFGR_PLLSAIR */
 993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_DCKCFGR1_PLLSAIDIVR)
 995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIDIVR  PLLSAIDIVR division factor (PLLSAIDIVR)
 996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
 997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
 998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_2           0x00000000U             /*!< PLLSAI division factor for P
 999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_4           RCC_DCKCFGR1_PLLSAIDIVR_0        /*!< PLLSAI division fac
1000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_8           RCC_DCKCFGR1_PLLSAIDIVR_1        /*!< PLLSAI division fac
1001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIDIVR_DIV_16          (RCC_DCKCFGR1_PLLSAIDIVR_1 | RCC_DCKCFGR1_PLLSAIDIVR_0)  
1002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_DCKCFGR1_PLLSAIDIVR */
1006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EC_PLLSAIP  PLLSAIP division factor (PLLSAIP)
1008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_2              0x00000000U               /*!< PLLSAI division factor for
1011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_4              RCC_PLLSAICFGR_PLLSAIP_0        /*!< PLLSAI division fact
1012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_6              RCC_PLLSAICFGR_PLLSAIP_1        /*!< PLLSAI division fact
1013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_PLLSAIP_DIV_8              (RCC_PLLSAICFGR_PLLSAIP_1 | RCC_PLLSAICFGR_PLLSAIP_0)    
1014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported macro ------------------------------------------------------------*/
1023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Macros RCC Exported Macros
1024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 32


1027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EM_WRITE_READ Common Write and read registers Macros
1028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Write a value in RCC register
1033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __REG__ Register to be written
1034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __VALUE__ Value to be written in the register
1035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_WriteReg(__REG__, __VALUE__) WRITE_REG(RCC->__REG__, (__VALUE__))
1038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Read a value in RCC register
1041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __REG__ Register to be read
1042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Register value
1043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define LL_RCC_ReadReg(__REG__) READ_REG(RCC->__REG__)
1045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EM_CALC_FREQ Calculate frequencies
1050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency on system domain
1055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetP ());
1057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
ARM GAS  /tmp/ccqw5Uyy.s 			page 33


1084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLP__ This parameter can be one of the following values:
1123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
1124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
1125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
1126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
1127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLP__) ((__INPUTFREQ__) / (
1130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLP__) >> RCC_PLLCFGR_PLLP_Pos ) + 1U) * 2U))
1131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency used on 48M domain
1134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_48M_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetQ ());
1136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
ARM GAS  /tmp/ccqw5Uyy.s 			page 34


1141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
ARM GAS  /tmp/ccqw5Uyy.s 			page 35


1198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLQ__ This parameter can be one of the following values:
1202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
1203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
1204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
1205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
1206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
1207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
1208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
1209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
1210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
1211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
1212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
1213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
1214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
1215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
1216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_48M_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLQ__) ((__INPUTFREQ__)
1219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLQ__) >> RCC_PLLCFGR_PLLQ_Pos ))
1220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
1222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLCLK frequency used on DSI
1224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLCLK_DSI_FREQ (HSE_VALUE, @ref LL_RCC_PLL_GetDivider (),
1225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLL_GetN (), @ref LL_RCC_PLL_GetR ());
1226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
ARM GAS  /tmp/ccqw5Uyy.s 			page 36


1255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLN__ Between 50 and 432
1291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLR__ This parameter can be one of the following values:
1292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
1293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
1294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
1295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
1296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
1297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
1298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLL clock frequency (in Hz)
1299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLCLK_DSI_FREQ(__INPUTFREQ__, __PLLM__, __PLLN__, __PLLR__) ((__INPUTFREQ__)
1301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLR__) >> RCC_PLLCFGR_PLLR_Pos ))
1302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
1303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used for SAI1 and SAI2 domains
1306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_SAI_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetQ (), @ref LL_RCC_PLLSAI_GetDIVQ 
1308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
ARM GAS  /tmp/ccqw5Uyy.s 			page 37


1312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
ARM GAS  /tmp/ccqw5Uyy.s 			page 38


1369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIQ__ This parameter can be one of the following values:
1374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_2
1375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_3
1376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_4
1377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_5
1378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_6
1379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_7
1380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_8
1381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_9
1382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_10
1383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_11
1384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_12
1385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_13
1386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_14
1387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIQ_DIV_15
1388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIDIVQ__ This parameter can be one of the following values:
1389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_1
1390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_2
1391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_3
1392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_4
1393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_5
1394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_6
1395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_7
1396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_8
1397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_9
1398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_10
1399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_11
1400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_12
1401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_13
1402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_14
1403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_15
1404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_16
1405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_17
1406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_18
1407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_19
1408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_20
1409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_21
1410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_22
1411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_23
1412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_24
1413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_25
1414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_26
1415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_27
1416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_28
1417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_29
1418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_30
1419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_31
1420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVQ_DIV_32
1421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_SAI_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIQ__, __PLLSAIDI
1424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLSAIQ__) >> RCC_PLLSAICFGR_PLLSAIQ_Pos) * (((__PLLSAIDIVQ__) >> RCC_DCKCF
1425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 39


1426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used on 48Mhz domain
1428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_48M_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetP ());
1430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
ARM GAS  /tmp/ccqw5Uyy.s 			page 40


1483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIP__ This parameter can be one of the following values:
1496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_2
1497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_4
1498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_6
1499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIP_DIV_8
1500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_48M_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIP__) (((__INPUT
1503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLSAIP__) >> RCC_PLLSAICFGR_PLLSAIP_Pos) + 1U ) * 2U))
1504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(LTDC)
1506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLSAI frequency used for LTDC domain
1508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLSAI_LTDC_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLSAI_GetN (), @ref LL_RCC_PLLSAI_GetR (), @ref LL_RCC_PLLSAI_GetDIVR 
1510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
ARM GAS  /tmp/ccqw5Uyy.s 			page 41


1540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIN__ Between 50 and 432
1575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIR__ This parameter can be one of the following values:
1576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_2
1577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_3
1578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_4
1579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_5
1580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_6
1581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIR_DIV_7
1582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLSAIDIVR__ This parameter can be one of the following values:
1583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_2
1584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_4
1585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_8
1586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSAIDIVR_DIV_16
1587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLSAI clock frequency (in Hz)
1588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLSAI_LTDC_FREQ(__INPUTFREQ__, __PLLM__, __PLLSAIN__, __PLLSAIR__, __PLLSAID
1590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLSAIR__) >> RCC_PLLSAICFGR_PLLSAIR_Pos) * (aRCC_PLLSAIDIVRPrescTable[(__P
1591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* LTDC */
1592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used for SAI1 and SAI2 domains
1595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_SAI_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetQ (), @ref LL_RCC_PLLI2S_GetDIVQ 
ARM GAS  /tmp/ccqw5Uyy.s 			page 42


1597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
ARM GAS  /tmp/ccqw5Uyy.s 			page 43


1654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SQ__ This parameter can be one of the following values:
1663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
1664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
1665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
1666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
1667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
1668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
1669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
1670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
1671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
1672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
1673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
1674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
1675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
1676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
1677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SDIVQ__ This parameter can be one of the following values:
1678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
1679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
1680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
1681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
1682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
1683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
1684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
1685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
1686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
1687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
1688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
1689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
1690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
1691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
1692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
1693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
1694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
1695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
1696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
1697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
1698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
1699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
1700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
1701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
1702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
1703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
1704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
1705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
1706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
1707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
1708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
1709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
1710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
ARM GAS  /tmp/ccqw5Uyy.s 			page 44


1711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_SAI_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SQ__, __PLLI2SDI
1713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    (((__PLLI2SQ__) >> RCC_PLLI2SCFGR_PLLI2SQ_Pos) * (((__PLLI2SDIVQ__) >> RCC_DCKCF
1714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
1716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used on SPDIFRX domain
1718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_SPDIFRX_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetP ());
1720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
1745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
ARM GAS  /tmp/ccqw5Uyy.s 			page 45


1768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SP__ This parameter can be one of the following values:
1786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
1787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
1788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
1789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
1790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
1791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_SPDIFRX_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SP__) (((__I
1793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((((__PLLI2SP__) >> RCC_PLLI2SCFGR_PLLI2SP_Pos) + 1U) * 2U))
1794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
1795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PLLI2S frequency used for I2S domain
1798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note ex: @ref __LL_RCC_CALC_PLLI2S_I2S_FREQ (HSE_VALUE,@ref LL_RCC_PLL_GetDivider (),
1799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *             @ref LL_RCC_PLLI2S_GetN (), @ref LL_RCC_PLLI2S_GetR ());
1800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __INPUTFREQ__ PLL Input frequency (based on HSE/HSI)
1801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLM__ This parameter can be one of the following values:
1802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
1803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
1804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
1805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
1806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
1807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
1808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
1809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
1810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
1811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
1812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
1813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
1814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
1815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
1816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
1817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
1818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
1819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
1820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
1821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
1822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
1823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
1824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
ARM GAS  /tmp/ccqw5Uyy.s 			page 46


1825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
1826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
1827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
1828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
1829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
1830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
1831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
1832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
1833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
1834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
1835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
1836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
1837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
1838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
1839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
1840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
1841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
1842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
1843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
1844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
1845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
1846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
1847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
1848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
1849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
1850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
1851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
1852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
1853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
1854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
1855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
1856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
1857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
1858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
1859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
1860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
1861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
1862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
1863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
1864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SN__ Between 50 and 432
1865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __PLLI2SR__ This parameter can be one of the following values:
1866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
1867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
1868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
1869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
1870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
1871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
1872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PLLI2S clock frequency (in Hz)
1873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PLLI2S_I2S_FREQ(__INPUTFREQ__, __PLLM__, __PLLI2SN__, __PLLI2SR__) (((__INPUT
1875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****                    ((__PLLI2SR__) >> RCC_PLLI2SCFGR_PLLI2SR_Pos))
1876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the HCLK frequency
1879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __SYSCLKFREQ__ SYSCLK frequency (based on HSE/HSI/PLLCLK)
1880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __AHBPRESCALER__ This parameter can be one of the following values:
1881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
ARM GAS  /tmp/ccqw5Uyy.s 			page 47


1882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
1883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
1884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
1885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
1886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
1887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
1888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
1889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
1890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval HCLK clock frequency (in Hz)
1891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_HCLK_FREQ(__SYSCLKFREQ__, __AHBPRESCALER__) ((__SYSCLKFREQ__) >> AHBPrescTabl
1893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PCLK1 frequency (ABP1)
1896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __HCLKFREQ__ HCLK frequency
1897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __APB1PRESCALER__ This parameter can be one of the following values:
1898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
1899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
1900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
1901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
1902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
1903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PCLK1 clock frequency (in Hz)
1904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PCLK1_FREQ(__HCLKFREQ__, __APB1PRESCALER__) ((__HCLKFREQ__) >> APBPrescTable[
1906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Helper macro to calculate the PCLK2 frequency (ABP2)
1909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __HCLKFREQ__ HCLK frequency
1910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  __APB2PRESCALER__ This parameter can be one of the following values:
1911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
1912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
1913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
1914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
1915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
1916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval PCLK2 clock frequency (in Hz)
1917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #define __LL_RCC_CALC_PCLK2_FREQ(__HCLKFREQ__, __APB2PRESCALER__) ((__HCLKFREQ__) >> APBPrescTable[
1919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /* Exported functions --------------------------------------------------------*/
1929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_Exported_Functions RCC Exported Functions
1930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_HSE HSE
1934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
1935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable the Clock Security System.
ARM GAS  /tmp/ccqw5Uyy.s 			page 48


1939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           CSSON         LL_RCC_HSE_EnableCSS
1940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_EnableCSS(void)
1943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_CSSON);
1945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSE external oscillator (HSE Bypass)
1949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEBYP        LL_RCC_HSE_EnableBypass
1950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_EnableBypass(void)
1953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSEBYP);
1955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSE external oscillator (HSE Bypass)
1959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEBYP        LL_RCC_HSE_DisableBypass
1960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_DisableBypass(void)
1963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSEBYP);
1965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSE crystal oscillator (HSE ON)
1969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEON         LL_RCC_HSE_Enable
1970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_Enable(void)
1973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSEON);
1975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSE crystal oscillator (HSE ON)
1979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSEON         LL_RCC_HSE_Disable
1980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
1981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSE_Disable(void)
1983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSEON);
1985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
1986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if HSE oscillator Ready
1989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSERDY        LL_RCC_HSE_IsReady
1990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
1991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSE_IsReady(void)
1993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_HSERDY) == (RCC_CR_HSERDY));
1995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 49


1996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
1997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
1998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
1999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_HSI HSI
2002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable HSI oscillator
2007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSION         LL_RCC_HSI_Enable
2008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_Enable(void)
2011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_HSION);
2013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable HSI oscillator
2017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSION         LL_RCC_HSI_Disable
2018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_Disable(void)
2021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_HSION);
2023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if HSI clock is ready
2027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           HSIRDY        LL_RCC_HSI_IsReady
2028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_IsReady(void)
2031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_HSIRDY) == (RCC_CR_HSIRDY));
2033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSI Calibration value
2037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note When HSITRIM is written, HSICAL is updated with the sum of
2038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       HSITRIM and the factory trim value
2039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSICAL        LL_RCC_HSI_GetCalibration
2040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data = 0x00 and Max_Data = 0xFF
2041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_GetCalibration(void)
2043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CR, RCC_CR_HSICAL) >> RCC_CR_HSICAL_Pos);
2045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set HSI Calibration trimming
2049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note user-programmable trimming value that is added to the HSICAL
2050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Default value is 16, which, when added to the HSICAL value,
2051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       should trim the HSI to 16 MHz +/- 1 %
2052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSITRIM       LL_RCC_HSI_SetCalibTrimming
ARM GAS  /tmp/ccqw5Uyy.s 			page 50


2053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Value Between Min_Data = 0 and Max_Data = 31
2054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_HSI_SetCalibTrimming(uint32_t Value)
2057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CR, RCC_CR_HSITRIM, Value << RCC_CR_HSITRIM_Pos);
2059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSI Calibration trimming
2063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR        HSITRIM       LL_RCC_HSI_GetCalibTrimming
2064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data = 0 and Max_Data = 31
2065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_HSI_GetCalibTrimming(void)
2067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CR, RCC_CR_HSITRIM) >> RCC_CR_HSITRIM_Pos);
2069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_LSE LSE
2076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable  Low Speed External (LSE) crystal.
2081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEON         LL_RCC_LSE_Enable
2082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_Enable(void)
2085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_LSEON);
2087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable  Low Speed External (LSE) crystal.
2091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEON         LL_RCC_LSE_Disable
2092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_Disable(void)
2095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_LSEON);
2097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable external clock source (LSE bypass).
2101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEBYP        LL_RCC_LSE_EnableBypass
2102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_EnableBypass(void)
2105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_LSEBYP);
2107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/ccqw5Uyy.s 			page 51


2110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable external clock source (LSE bypass).
2111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEBYP        LL_RCC_LSE_DisableBypass
2112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_DisableBypass(void)
2115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_LSEBYP);
2117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set LSE oscillator drive capability
2121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note The oscillator is in Xtal mode when it is not in bypass mode.
2122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEDRV        LL_RCC_LSE_SetDriveCapability
2123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LSEDrive This parameter can be one of the following values:
2124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_LOW
2125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMHIGH
2126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMLOW
2127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_HIGH
2128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSE_SetDriveCapability(uint32_t LSEDrive)
2131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->BDCR, RCC_BDCR_LSEDRV, LSEDrive);
2133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get LSE oscillator drive capability
2137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSEDRV        LL_RCC_LSE_GetDriveCapability
2138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_LOW
2140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMHIGH
2141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_MEDIUMLOW
2142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LSEDRIVE_HIGH
2143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSE_GetDriveCapability(void)
2145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->BDCR, RCC_BDCR_LSEDRV));
2147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if LSE oscillator Ready
2151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         LSERDY        LL_RCC_LSE_IsReady
2152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSE_IsReady(void)
2155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->BDCR, RCC_BDCR_LSERDY) == (RCC_BDCR_LSERDY));
2157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_LSI LSI
2164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 52


2167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable LSI Oscillator
2169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSION         LL_RCC_LSI_Enable
2170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSI_Enable(void)
2173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CSR, RCC_CSR_LSION);
2175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable LSI Oscillator
2179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSION         LL_RCC_LSI_Disable
2180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_LSI_Disable(void)
2183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CSR, RCC_CSR_LSION);
2185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if LSI is Ready
2189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CSR          LSIRDY        LL_RCC_LSI_IsReady
2190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_LSI_IsReady(void)
2193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CSR, RCC_CSR_LSIRDY) == (RCC_CSR_LSIRDY));
2195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_System System
2202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure the system clock source
2207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         SW            LL_RCC_SetSysClkSource
2208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_HSI
2210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_HSE
2211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_PLL
2212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSysClkSource(uint32_t Source)
2215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_SW, Source);
2217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get the system clock source
2221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         SWS           LL_RCC_GetSysClkSource
2222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_HSI
ARM GAS  /tmp/ccqw5Uyy.s 			page 53


2224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_HSE
2225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYS_CLKSOURCE_STATUS_PLL
2226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSysClkSource(void)
2228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_SWS));
2230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set AHB prescaler
2234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         HPRE          LL_RCC_SetAHBPrescaler
2235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
2237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
2238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
2239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
2240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
2241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
2242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
2243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
2244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
2245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAHBPrescaler(uint32_t Prescaler)
2248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_HPRE, Prescaler);
2250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set APB1 prescaler
2254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE1         LL_RCC_SetAPB1Prescaler
2255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
2257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
2258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
2259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
2260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
2261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAPB1Prescaler(uint32_t Prescaler)
2264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_PPRE1, Prescaler);
2266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set APB2 prescaler
2270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE2         LL_RCC_SetAPB2Prescaler
2271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
2272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
2273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
2274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
2275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
2276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
2277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetAPB2Prescaler(uint32_t Prescaler)
2280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
ARM GAS  /tmp/ccqw5Uyy.s 			page 54


2281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_PPRE2, Prescaler);
2282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get AHB prescaler
2286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         HPRE          LL_RCC_GetAHBPrescaler
2287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_1
2289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_2
2290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_4
2291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_8
2292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_16
2293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_64
2294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_128
2295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_256
2296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SYSCLK_DIV_512
2297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAHBPrescaler(void)
2299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_HPRE));
2301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get APB1 prescaler
2305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE1         LL_RCC_GetAPB1Prescaler
2306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_1
2308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_2
2309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_4
2310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_8
2311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB1_DIV_16
2312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAPB1Prescaler(void)
2314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_PPRE1));
2316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get APB2 prescaler
2320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         PPRE2         LL_RCC_GetAPB2Prescaler
2321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_1
2323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_2
2324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_4
2325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_8
2326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_APB2_DIV_16
2327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetAPB2Prescaler(void)
2329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_PPRE2));
2331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_MCO MCO
ARM GAS  /tmp/ccqw5Uyy.s 			page 55


2338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure MCOx
2343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         MCO1          LL_RCC_ConfigMCO\n
2344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO1PRE       LL_RCC_ConfigMCO\n
2345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO2          LL_RCC_ConfigMCO\n
2346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         CFGR         MCO2PRE       LL_RCC_ConfigMCO
2347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  MCOxSource This parameter can be one of the following values:
2348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_HSI
2349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_LSE
2350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_HSE
2351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1SOURCE_PLLCLK
2352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_SYSCLK
2353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_PLLI2S
2354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_HSE
2355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2SOURCE_PLLCLK
2356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  MCOxPrescaler This parameter can be one of the following values:
2357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_1
2358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_2
2359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_3
2360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_4
2361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO1_DIV_5
2362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_1
2363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_2
2364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_3
2365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_4
2366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_MCO2_DIV_5
2367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ConfigMCO(uint32_t MCOxSource, uint32_t MCOxPrescaler)
2370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, (MCOxSource & 0xFFFF0000U) | (MCOxPrescaler & 0xFFFF0000U),  (MCOxSource <<
2372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_Peripheral_Clock_Source Peripheral Clock Source
2379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure USARTx clock source
2384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        USART1SEL     LL_RCC_SetUSARTClockSource\n
2385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART2SEL     LL_RCC_SetUSARTClockSource\n
2386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART3SEL     LL_RCC_SetUSARTClockSource\n
2387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART6SEL     LL_RCC_SetUSARTClockSource
2388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USARTxSource This parameter can be one of the following values:
2389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_PCLK2
2390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_SYSCLK
2391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_HSI
2392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_LSE
2393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_PCLK1
2394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_SYSCLK
ARM GAS  /tmp/ccqw5Uyy.s 			page 56


2395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_HSI
2396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_LSE
2397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_PCLK1
2398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_SYSCLK
2399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_HSI
2400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_LSE
2401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_PCLK2
2402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_SYSCLK
2403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_HSI
2404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_LSE
2405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUSARTClockSource(uint32_t USARTxSource)
2408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (USARTxSource >> 16U), (USARTxSource & 0x0000FFFFU));
2410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure UARTx clock source
2414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        UART4SEL      LL_RCC_SetUARTClockSource\n
2415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART5SEL      LL_RCC_SetUARTClockSource\n
2416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART7SEL      LL_RCC_SetUARTClockSource\n
2417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART8SEL      LL_RCC_SetUARTClockSource
2418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  UARTxSource This parameter can be one of the following values:
2419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_PCLK1
2420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_SYSCLK
2421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_HSI
2422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_LSE
2423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_PCLK1
2424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_SYSCLK
2425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_HSI
2426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_LSE
2427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_PCLK1
2428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_SYSCLK
2429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_HSI
2430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_LSE
2431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_PCLK1
2432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_SYSCLK
2433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_HSI
2434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_LSE
2435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUARTClockSource(uint32_t UARTxSource)
2438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (UARTxSource >> 16U), (UARTxSource & 0x0000FFFFU));
2440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure I2Cx clock source
2444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        I2C1SEL       LL_RCC_SetI2CClockSource\n
2445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C2SEL       LL_RCC_SetI2CClockSource\n
2446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C3SEL       LL_RCC_SetI2CClockSource\n
2447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C4SEL       LL_RCC_SetI2CClockSource
2448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2CxSource This parameter can be one of the following values:
2449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_PCLK1
2450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_SYSCLK
2451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_HSI
ARM GAS  /tmp/ccqw5Uyy.s 			page 57


2452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_PCLK1
2453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_SYSCLK
2454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_HSI
2455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_PCLK1
2456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_SYSCLK
2457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_HSI
2458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_PCLK1 (*)
2459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_SYSCLK (*)
2460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_HSI (*)
2461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetI2CClockSource(uint32_t I2CxSource)
2466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (I2CxSource & 0xFFFF0000U),  (I2CxSource << 16U));
2468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure LPTIMx clock source
2472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        LPTIM1SEL     LL_RCC_SetLPTIMClockSource
2473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LPTIMxSource This parameter can be one of the following values:
2474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_PCLK1
2475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSI
2476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_HSI
2477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSE
2478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetLPTIMClockSource(uint32_t LPTIMxSource)
2481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_LPTIM1SEL, LPTIMxSource);
2483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure SAIx clock source
2487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1        SAI1SEL       LL_RCC_SetSAIClockSource\n
2488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1        SAI2SEL       LL_RCC_SetSAIClockSource
2489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SAIxSource This parameter can be one of the following values:
2490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSAI
2491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLI2S
2492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PIN
2493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSRC (*)
2494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSAI
2495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLI2S
2496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PIN
2497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSRC (*)
2498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSAIClockSource(uint32_t SAIxSource)
2503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, (SAIxSource & 0xFFFF0000U), (SAIxSource << 16U));
2505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure SDMMC clock source
ARM GAS  /tmp/ccqw5Uyy.s 			page 58


2509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        SDMMC1SEL      LL_RCC_SetSDMMCClockSource\n
2510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        SDMMC2SEL      LL_RCC_SetSDMMCClockSource
2511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SDMMCxSource This parameter can be one of the following values:
2512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK
2513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_SYSCLK
2514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK (*)
2515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_SYSCLK (*)
2516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetSDMMCClockSource(uint32_t SDMMCxSource)
2521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, (SDMMCxSource & 0xFFFF0000U), (SDMMCxSource << 16U));
2523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure 48Mhz domain clock source
2527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetCK48MClockSource
2528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CK48MxSource This parameter can be one of the following values:
2529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLL
2530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLLSAI
2531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetCK48MClockSource(uint32_t CK48MxSource)
2534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, CK48MxSource);
2536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure RNG clock source
2540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetRNGClockSource
2541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  RNGxSource This parameter can be one of the following values:
2542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLL
2543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLLSAI
2544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRNGClockSource(uint32_t RNGxSource)
2547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, RNGxSource);
2549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure USB clock source
2553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_SetUSBClockSource
2554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USBxSource This parameter can be one of the following values:
2555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLL
2556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLLSAI
2557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetUSBClockSource(uint32_t USBxSource)
2560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CK48MSEL, USBxSource);
2562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
2565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
ARM GAS  /tmp/ccqw5Uyy.s 			page 59


2566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure CEC clock source
2567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         CECSEL        LL_RCC_SetCECClockSource
2568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_LSE
2570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_HSI_DIV488
2571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetCECClockSource(uint32_t Source)
2574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_CECSEL, Source);
2576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
2578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure I2S clock source
2581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         I2SSRC        LL_RCC_SetI2SClockSource
2582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PLLI2S
2584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PIN
2585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetI2SClockSource(uint32_t Source)
2588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_I2SSRC, Source);
2590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
2593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DSI clock source
2595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         DSISEL        LL_RCC_SetDSIClockSource
2596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PHY
2598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PLL
2599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDSIClockSource(uint32_t Source)
2602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR2, RCC_DCKCFGR2_DSISEL, Source);
2604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
2606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
2608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DFSDM Audio clock source
2610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         ADFSDM1SEL        LL_RCC_SetDFSDMAudioClockSource
2611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1
2613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2
2614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDFSDMAudioClockSource(uint32_t Source)
2617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_ADFSDM1SEL, Source);
2619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure DFSDM Kernel clock source
ARM GAS  /tmp/ccqw5Uyy.s 			page 60


2623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         DFSDM1SEL        LL_RCC_SetDFSDMClockSource
2624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_PCLK2
2626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_SYSCLK
2627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetDFSDMClockSource(uint32_t Source)
2630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_DFSDM1SEL, Source);
2632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
2634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get USARTx clock source
2637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        USART1SEL     LL_RCC_GetUSARTClockSource\n
2638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART2SEL     LL_RCC_GetUSARTClockSource\n
2639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART3SEL     LL_RCC_GetUSARTClockSource\n
2640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        USART6SEL     LL_RCC_GetUSARTClockSource
2641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USARTx This parameter can be one of the following values:
2642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE
2643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE
2644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE
2645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE
2646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_PCLK2
2648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_SYSCLK
2649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_HSI
2650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART1_CLKSOURCE_LSE
2651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_PCLK1
2652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_SYSCLK
2653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_HSI
2654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART2_CLKSOURCE_LSE
2655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_PCLK1
2656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_SYSCLK
2657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_HSI
2658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART3_CLKSOURCE_LSE
2659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_PCLK2
2660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_SYSCLK
2661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_HSI
2662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USART6_CLKSOURCE_LSE
2663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUSARTClockSource(uint32_t USARTx)
2665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, USARTx) | (USARTx << 16U));
2667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get UARTx clock source
2671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        UART4SEL      LL_RCC_GetUARTClockSource\n
2672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART5SEL      LL_RCC_GetUARTClockSource\n
2673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART7SEL      LL_RCC_GetUARTClockSource\n
2674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        UART8SEL      LL_RCC_GetUARTClockSource
2675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  UARTx This parameter can be one of the following values:
2676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE
2677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE
2678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE
2679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE
ARM GAS  /tmp/ccqw5Uyy.s 			page 61


2680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_PCLK1
2682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_SYSCLK
2683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_HSI
2684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART4_CLKSOURCE_LSE
2685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_PCLK1
2686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_SYSCLK
2687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_HSI
2688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART5_CLKSOURCE_LSE
2689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_PCLK1
2690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_SYSCLK
2691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_HSI
2692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART7_CLKSOURCE_LSE
2693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_PCLK1
2694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_SYSCLK
2695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_HSI
2696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_UART8_CLKSOURCE_LSE
2697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUARTClockSource(uint32_t UARTx)
2699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, UARTx) | (UARTx << 16U));
2701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2Cx clock source
2705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        I2C1SEL       LL_RCC_GetI2CClockSource\n
2706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C2SEL       LL_RCC_GetI2CClockSource\n
2707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C3SEL       LL_RCC_GetI2CClockSource\n
2708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        I2C4SEL       LL_RCC_GetI2CClockSource
2709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2Cx This parameter can be one of the following values:
2710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE
2711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE
2712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE
2713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE (*)
2714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_PCLK1
2716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_SYSCLK
2717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C1_CLKSOURCE_HSI
2718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_PCLK1
2719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_SYSCLK
2720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C2_CLKSOURCE_HSI
2721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_PCLK1
2722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_SYSCLK
2723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C3_CLKSOURCE_HSI
2724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_PCLK1 (*)
2725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_SYSCLK (*)
2726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2C4_CLKSOURCE_HSI (*)
2727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****  */
2730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetI2CClockSource(uint32_t I2Cx)
2731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)((READ_BIT(RCC->DCKCFGR2, I2Cx) >> 16U) | I2Cx);
2733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get LPTIMx clock source
ARM GAS  /tmp/ccqw5Uyy.s 			page 62


2737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        LPTIM1SEL     LL_RCC_GetLPTIMClockSource
2738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  LPTIMx This parameter can be one of the following values:
2739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE
2740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_PCLK1
2742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSI
2743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_HSI
2744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_LPTIM1_CLKSOURCE_LSE
2745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetLPTIMClockSource(uint32_t LPTIMx)
2747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, RCC_DCKCFGR2_LPTIM1SEL));
2749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SAIx clock source
2753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1        SAI1SEL       LL_RCC_GetSAIClockSource\n
2754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1        SAI2SEL       LL_RCC_GetSAIClockSource
2755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SAIx This parameter can be one of the following values:
2756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE
2757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE
2758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSAI
2760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLI2S
2761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PIN
2762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI1_CLKSOURCE_PLLSRC (*)
2763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSAI
2764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLI2S
2765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PIN
2766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SAI2_CLKSOURCE_PLLSRC (*)
2767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSAIClockSource(uint32_t SAIx)
2771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, SAIx) >> 16U | SAIx);
2773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get SDMMCx clock source
2777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        SDMMC1SEL      LL_RCC_GetSDMMCClockSource\n
2778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR2        SDMMC2SEL      LL_RCC_GetSDMMCClockSource
2779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  SDMMCx This parameter can be one of the following values:
2780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE
2781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE (*)
2782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_PLL48CLK
2784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC1_CLKSOURCE_SYSCLK
2785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_PLL48CLK (*)
2786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SDMMC2_CLKSOURCE_SYSCLK (*)
2787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *
2788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         (*) value not defined in all devices.
2789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetSDMMCClockSource(uint32_t SDMMCx)
2791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, SDMMCx) >> 16U | SDMMCx);
2793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 63


2794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get 48Mhz domain clock source
2797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetCK48MClockSource
2798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CK48Mx This parameter can be one of the following values:
2799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE
2800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLL
2802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CK48M_CLKSOURCE_PLLSAI
2803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetCK48MClockSource(uint32_t CK48Mx)
2805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, CK48Mx));
2807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get RNGx clock source
2811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetRNGClockSource
2812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  RNGx This parameter can be one of the following values:
2813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE
2814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLL
2816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RNG_CLKSOURCE_PLLSAI
2817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRNGClockSource(uint32_t RNGx)
2819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, RNGx));
2821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get USBx clock source
2825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2        CK48MSEL      LL_RCC_GetUSBClockSource
2826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  USBx This parameter can be one of the following values:
2827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE
2828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLL
2830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_USB_CLKSOURCE_PLLSAI
2831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetUSBClockSource(uint32_t USBx)
2833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, USBx));
2835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(CEC)
2838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get CEC Clock Source
2840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         CECSEL        LL_RCC_GetCECClockSource
2841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  CECx This parameter can be one of the following values:
2842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE
2843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_LSE
2845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_CEC_CLKSOURCE_HSI_DIV488
2846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetCECClockSource(uint32_t CECx)
2848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, CECx));
2850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 64


2851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* CEC */
2852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2S Clock Source
2855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         I2SSRC        LL_RCC_GetI2SClockSource
2856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  I2Sx This parameter can be one of the following values:
2857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE
2858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PLLI2S
2860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_I2S1_CLKSOURCE_PIN
2861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetI2SClockSource(uint32_t I2Sx)
2863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, I2Sx));
2865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DFSDM1_Channel0)
2868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DFSDM Audio Clock Source
2870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         ADFSDM1SEL        LL_RCC_GetDFSDMAudioClockSource
2871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DFSDMx This parameter can be one of the following values:
2872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE
2873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI1
2875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_AUDIO_CLKSOURCE_SAI2
2876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDFSDMAudioClockSource(uint32_t DFSDMx)
2878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, DFSDMx));
2880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DFSDM Audio Clock Source
2884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         DFSDM1SEL        LL_RCC_GetDFSDMClockSource
2885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DFSDMx This parameter can be one of the following values:
2886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE
2887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_PCLK2
2889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DFSDM1_CLKSOURCE_SYSCLK
2890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDFSDMClockSource(uint32_t DFSDMx)
2892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, DFSDMx));
2894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DFSDM1_Channel0 */
2896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
2898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get DSI Clock Source
2900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR2         DSISEL        LL_RCC_GetDSIClockSource
2901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  DSIx This parameter can be one of the following values:
2902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE
2903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PHY
2905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_DSI_CLKSOURCE_PLL
2906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetDSIClockSource(uint32_t DSIx)
ARM GAS  /tmp/ccqw5Uyy.s 			page 65


2908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR2, DSIx));
2910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
2912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
2915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_RTC RTC
2918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
2919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set RTC Clock Source
2923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Once the RTC clock source has been selected, it cannot be changed anymore unless
2924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       the Backup domain is reset, or unless a failure is detected on LSE (LSECSSD is
2925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       set). The BDRST bit can be used to reset them.
2926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCSEL        LL_RCC_SetRTCClockSource
2927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
2928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_NONE
2929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSE
2930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSI
2931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_HSE
2932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRTCClockSource(uint32_t Source)
2935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->BDCR, RCC_BDCR_RTCSEL, Source);
2937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get RTC Clock Source
2941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCSEL        LL_RCC_GetRTCClockSource
2942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
2943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_NONE
2944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSE
2945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_LSI
2946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_CLKSOURCE_HSE
2947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRTCClockSource(void)
2949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->BDCR, RCC_BDCR_RTCSEL));
2951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable RTC
2955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_EnableRTC
2956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_EnableRTC(void)
2959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_RTCEN);
2961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable RTC
ARM GAS  /tmp/ccqw5Uyy.s 			page 66


2965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_DisableRTC
2966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_DisableRTC(void)
2969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_RTCEN);
2971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if RTC has been enabled or not
2975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         RTCEN         LL_RCC_IsEnabledRTC
2976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
2977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_IsEnabledRTC(void)
2979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->BDCR, RCC_BDCR_RTCEN) == (RCC_BDCR_RTCEN));
2981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Force the Backup domain reset
2985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         BDRST         LL_RCC_ForceBackupDomainReset
2986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ForceBackupDomainReset(void)
2989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
2990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->BDCR, RCC_BDCR_BDRST);
2991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
2992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
2993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
2994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Release the Backup domain reset
2995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll BDCR         BDRST         LL_RCC_ReleaseBackupDomainReset
2996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
2997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
2998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_ReleaseBackupDomainReset(void)
2999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->BDCR, RCC_BDCR_BDRST);
3001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set HSE Prescalers for RTC Clock
3005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         RTCPRE        LL_RCC_SetRTC_HSEPrescaler
3006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
3007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_NOCLOCK
3008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_2
3009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_3
3010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_4
3011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_5
3012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_6
3013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_7
3014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_8
3015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_9
3016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_10
3017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_11
3018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_12
3019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_13
3020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_14
3021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_15
ARM GAS  /tmp/ccqw5Uyy.s 			page 67


3022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_16
3023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_17
3024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_18
3025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_19
3026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_20
3027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_21
3028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_22
3029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_23
3030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_24
3031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_25
3032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_26
3033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_27
3034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_28
3035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_29
3036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_30
3037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_31
3038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetRTC_HSEPrescaler(uint32_t Prescaler)
3041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->CFGR, RCC_CFGR_RTCPRE, Prescaler);
3043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get HSE Prescalers for RTC Clock
3047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CFGR         RTCPRE        LL_RCC_GetRTC_HSEPrescaler
3048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_NOCLOCK
3050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_2
3051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_3
3052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_4
3053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_5
3054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_6
3055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_7
3056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_8
3057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_9
3058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_10
3059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_11
3060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_12
3061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_13
3062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_14
3063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_15
3064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_16
3065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_17
3066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_18
3067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_19
3068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_20
3069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_21
3070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_22
3071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_23
3072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_24
3073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_25
3074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_26
3075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_27
3076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_28
3077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_29
3078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_30
ARM GAS  /tmp/ccqw5Uyy.s 			page 68


3079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_RTC_HSE_DIV_31
3080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetRTC_HSEPrescaler(void)
3082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->CFGR, RCC_CFGR_RTCPRE));
3084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
3088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_TIM_CLOCK_PRESCALER TIM
3091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
3092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Set Timers Clock Prescalers
3096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         TIMPRE        LL_RCC_SetTIMPrescaler
3097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Prescaler This parameter can be one of the following values:
3098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_TWICE
3099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_FOUR_TIMES
3100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_SetTIMPrescaler(uint32_t Prescaler)
3103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_TIMPRE, Prescaler);
3105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Timers Clock Prescalers
3109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1         TIMPRE        LL_RCC_GetTIMPrescaler
3110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_TWICE
3112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_TIM_PRESCALER_FOUR_TIMES
3113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_GetTIMPrescaler(void)
3115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_TIMPRE));
3117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
3121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLL PLL
3124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
3125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLL
3129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLON         LL_RCC_PLL_Enable
3130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_Enable(void)
3133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLON);
3135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 69


3136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLL
3139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Cannot be disabled if the PLL clock is used as the system clock
3140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLON         LL_RCC_PLL_Disable
3141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_Disable(void)
3144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLON);
3146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLL Ready
3150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLRDY        LL_RCC_PLL_IsReady
3151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
3152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_IsReady(void)
  92              		.loc 2 3153 26 view .LVU26
  93              	.LBB55:
3154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLRDY) == (RCC_CR_PLLRDY));
  94              		.loc 2 3155 3 view .LVU27
  95              		.loc 2 3155 11 is_stmt 0 view .LVU28
  96 0000 0A4B     		ldr	r3, .L9
  97 0002 1B68     		ldr	r3, [r3]
  98              	.LBE55:
  99              	.LBE54:
 100              		.loc 1 653 5 discriminator 1 view .LVU29
 101 0004 13F0007F 		tst	r3, #33554432
 102 0008 0DD1     		bne	.L6
 650:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 103              		.loc 1 650 15 view .LVU30
 104 000a 0020     		movs	r0, #0
 105              	.L3:
 106              	.LVL6:
 654:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 655:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* PLL configuration cannot be modified */
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 657:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 658:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 659:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check if PLLSAI is busy*/
 660:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(LL_RCC_PLLSAI_IsReady() != 0U)
 107              		.loc 1 660 3 is_stmt 1 view .LVU31
 108              	.LBB56:
 109              	.LBI56:
3156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for SYSCLK Domain
3160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLP can be written only when PLL is disabled
3163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_SYS\n
3164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_SYS\n
3165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_SYS\n
3166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLP          LL_RCC_PLL_ConfigDomain_SYS
ARM GAS  /tmp/ccqw5Uyy.s 			page 70


3167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
ARM GAS  /tmp/ccqw5Uyy.s 			page 71


3224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLP This parameter can be one of the following values:
3235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
3236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
3237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
3238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
3239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_SYS(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
3245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for 48Mhz domain clock
3249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLQ can be written only when PLL is disabled
3252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for USB, RNG, SDMMC1
3253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_48M\n
3254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_48M\n
3255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_48M\n
3256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLQ          LL_RCC_PLL_ConfigDomain_48M
3257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
ARM GAS  /tmp/ccqw5Uyy.s 			page 72


3281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLQ This parameter can be one of the following values:
3325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
3326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
3327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
3328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
3329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
3330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
3331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
3332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
3333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
3334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
3335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
3336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
3337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
ARM GAS  /tmp/ccqw5Uyy.s 			page 73


3338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
3339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_48M(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLQ);
3345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(DSI)
3348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL used for DSI clock
3350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLR can be written only when PLL is disabled
3353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for DSI
3354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_ConfigDomain_DSI\n
3355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLL_ConfigDomain_DSI\n
3356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLN          LL_RCC_PLL_ConfigDomain_DSI\n
3357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLR          LL_RCC_PLL_ConfigDomain_DSI
3358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
ARM GAS  /tmp/ccqw5Uyy.s 			page 74


3395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLR This parameter can be one of the following values:
3426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
3427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
3428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
3429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
3430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
3431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
3432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigDomain_DSI(uint32_t Source, uint32_t PLLM, uint32_t PLLN, uin
3435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM | RCC_PLLCFGR_PLLN | RCC_PLLCFGR_P
3437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLR);
3438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* DSI */
3440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLL clock source
3443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_SetMainSource
3444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param PLLSource This parameter can be one of the following values:
3445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SetMainSource(uint32_t PLLSource)
3450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC, PLLSource);
ARM GAS  /tmp/ccqw5Uyy.s 			page 75


3452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get the oscillator used as PLL clock source.
3456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLL_GetMainSource
3457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetMainSource(void)
3462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC));
3464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL multiplication factor for VCO
3468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLN          LL_RCC_PLL_GetN
3469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between 50 and 432
3470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetN(void)
3472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLN) >>  RCC_PLLCFGR_PLLN_Pos);
3474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLP 
3478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLP       LL_RCC_PLL_GetP
3479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_2
3481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_4
3482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_6
3483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLP_DIV_8
3484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetP(void)
3486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLP));
3488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLQ
3492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLL48MCLK selected for USB, RNG, SDMMC (48 MHz clock)
3493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLQ          LL_RCC_PLL_GetQ
3494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_2
3496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_3
3497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_4
3498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_5
3499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_6
3500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_7
3501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_8
3502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_9
3503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_10
3504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_11
3505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_12
3506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_13
3507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_14
3508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLQ_DIV_15
ARM GAS  /tmp/ccqw5Uyy.s 			page 76


3509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetQ(void)
3511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLQ));
3513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLCFGR_PLLR)
3516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Main PLL division factor for PLLR
3518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLCLK (system clock)
3519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLR          LL_RCC_PLL_GetR
3520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_2
3522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_3
3523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_4
3524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_5
3525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_6
3526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLR_DIV_7
3527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetR(void)
3529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLR));
3531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLCFGR_PLLR */
3533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Division factor for the main PLL and other PLL
3536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLM          LL_RCC_PLL_GetDivider
3537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
ARM GAS  /tmp/ccqw5Uyy.s 			page 77


3566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetDivider(void)
3602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLCFGR, RCC_PLLCFGR_PLLM));
3604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure Spread Spectrum used for PLL
3608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note These bits must be written before enabling PLL
3609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR        MODPER        LL_RCC_PLL_ConfigSpreadSpectrum\n
3610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         SSCGR        INCSTEP       LL_RCC_PLL_ConfigSpreadSpectrum\n
3611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         SSCGR        SPREADSEL     LL_RCC_PLL_ConfigSpreadSpectrum
3612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Mod Between Min_Data=0 and Max_Data=8191
3613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Inc Between Min_Data=0 and Max_Data=32767
3614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Sel This parameter can be one of the following values:
3615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_CENTER
3616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_DOWN
3617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_ConfigSpreadSpectrum(uint32_t Mod, uint32_t Inc, uint32_t Sel)
3620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->SSCGR, RCC_SSCGR_MODPER | RCC_SSCGR_INCSTEP | RCC_SSCGR_SPREADSEL, Mod | (Inc << 
3622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 78


3623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Modulation Period for PLL
3626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         MODPER        LL_RCC_PLL_GetPeriodModulation
3627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data=0 and Max_Data=8191
3628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetPeriodModulation(void)
3630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_MODPER));
3632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Incrementation Step for PLL
3636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Must be written before enabling PLL
3637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         INCSTEP        LL_RCC_PLL_GetStepIncrementation
3638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between Min_Data=0 and Max_Data=32767
3639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetStepIncrementation(void)
3641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_INCSTEP) >> RCC_SSCGR_INCSTEP_Pos);
3643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get Spread Spectrum Selection for PLL
3647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note Must be written before enabling PLL
3648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SPREADSEL        LL_RCC_PLL_GetSpreadSelection
3649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
3650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_CENTER
3651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_SPREAD_SELECT_DOWN
3652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLL_GetSpreadSelection(void)
3654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->SSCGR, RCC_SSCGR_SPREADSEL));
3656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable Spread Spectrum for PLL.
3660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SSCGEN         LL_RCC_PLL_SpreadSpectrum_Enable
3661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SpreadSpectrum_Enable(void)
3664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->SSCGR, RCC_SSCGR_SSCGEN);
3666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable Spread Spectrum for PLL.
3670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll SSCGR         SSCGEN         LL_RCC_PLL_SpreadSpectrum_Disable
3671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLL_SpreadSpectrum_Disable(void)
3674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->SSCGR, RCC_SSCGR_SSCGEN);
3676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
ARM GAS  /tmp/ccqw5Uyy.s 			page 79


3680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLLI2S PLLI2S
3683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
3684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLLI2S
3688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SON     LL_RCC_PLLI2S_Enable
3689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_Enable(void)
3692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLI2SON);
3694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLLI2S
3698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SON     LL_RCC_PLLI2S_Disable
3699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_Disable(void)
3702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLI2SON);
3704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLLI2S Ready
3708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLI2SRDY    LL_RCC_PLLI2S_IsReady
3709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
3710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_IsReady(void)
3712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLI2SRDY) == (RCC_CR_PLLI2SRDY));
3714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLI2S used for SAI1 and SAI2 domain clock
3718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLQ can be written only when PLLI2S is disabled
3721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This can be selected for SAI1 and SAI2
3722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_SAI\n
3723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_SAI\n
3724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_SAI\n
3725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SQ       LL_RCC_PLLI2S_ConfigDomain_SAI\n
3726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         DCKCFGR1      PLLI2SDIVQ    LL_RCC_PLLI2S_ConfigDomain_SAI
3727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
ARM GAS  /tmp/ccqw5Uyy.s 			page 80


3737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
ARM GAS  /tmp/ccqw5Uyy.s 			page 81


3794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLQ This parameter can be one of the following values:
3795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
3796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
3797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
3798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
3799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
3800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
3801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
3802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
3803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
3804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
3805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
3806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
3807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
3808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
3809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLDIVQ This parameter can be one of the following values:
3810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
3811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
3812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
3813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
3814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
3815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
3816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
3817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
3818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
3819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
3820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
3821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
3822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
3823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
3824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
3825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
3826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
3827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
3828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
3829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
3830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
3831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
3832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
3833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
3834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
3835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
3836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
3837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
3838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
3839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
3840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
3841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
3842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_SAI(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
3845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
3847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SQ, PLLN << RCC_PLLI2SCF
3848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLI2SDIVQ, PLLDIVQ);
3849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 82


3851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(SPDIFRX)
3852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief Configure PLLI2S used for SPDIFRX domain clock
3854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLP can be written only when PLLI2S is disabled
3857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for SPDIFRX
3858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_SPDIFRX\n
3861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SP       LL_RCC_PLLI2S_ConfigDomain_SPDIFRX
3862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
3874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
ARM GAS  /tmp/ccqw5Uyy.s 			page 83


3908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
3909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
3910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
3911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
3912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
3913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
3914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
3915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
3916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
3917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
3918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
3919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
3920:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
3921:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
3922:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
3923:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
3924:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
3925:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
3926:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
3927:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
3928:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
3929:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLP This parameter can be one of the following values:
3930:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
3931:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
3932:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
3933:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
3934:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
3935:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
3936:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_SPDIFRX(uint32_t Source, uint32_t PLLM, uint32_t PL
3937:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
3938:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
3939:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SP, PLLN << RCC_PLLI2SCF
3940:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
3941:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* SPDIFRX */
3942:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
3943:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
3944:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Configure PLLI2S used for I2S1 domain clock
3945:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLL Source and PLLM Divider can be written only when PLL,
3946:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *       PLLI2S and PLLSAI are disabled
3947:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note PLLN/PLLR can be written only when PLLI2S is disabled
3948:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note This  can be selected for I2S
3949:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLCFGR      PLLSRC        LL_RCC_PLLI2S_ConfigDomain_I2S\n
3950:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLCFGR      PLLM          LL_RCC_PLLI2S_ConfigDomain_I2S\n
3951:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SN       LL_RCC_PLLI2S_ConfigDomain_I2S\n
3952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         PLLI2SCFGR   PLLI2SR       LL_RCC_PLLI2S_ConfigDomain_I2S
3953:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  Source This parameter can be one of the following values:
3954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSI
3955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLSOURCE_HSE
3956:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLM This parameter can be one of the following values:
3957:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_2
3958:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_3
3959:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_4
3960:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_5
3961:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_6
3962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_7
3963:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_8
3964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_9
ARM GAS  /tmp/ccqw5Uyy.s 			page 84


3965:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_10
3966:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_11
3967:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_12
3968:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_13
3969:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_14
3970:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_15
3971:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_16
3972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_17
3973:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_18
3974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_19
3975:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_20
3976:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_21
3977:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_22
3978:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_23
3979:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_24
3980:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_25
3981:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_26
3982:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_27
3983:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_28
3984:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_29
3985:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_30
3986:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_31
3987:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_32
3988:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_33
3989:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_34
3990:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_35
3991:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_36
3992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_37
3993:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_38
3994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_39
3995:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_40
3996:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_41
3997:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_42
3998:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_43
3999:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_44
4000:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_45
4001:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_46
4002:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_47
4003:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_48
4004:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_49
4005:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_50
4006:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_51
4007:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_52
4008:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_53
4009:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_54
4010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_55
4011:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_56
4012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_57
4013:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_58
4014:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_59
4015:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_60
4016:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_61
4017:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_62
4018:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLM_DIV_63
4019:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLN Between 50 and 432
4020:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @param  PLLR This parameter can be one of the following values:
4021:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
ARM GAS  /tmp/ccqw5Uyy.s 			page 85


4022:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
4023:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
4024:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
4025:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
4026:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
4027:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4028:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4029:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLI2S_ConfigDomain_I2S(uint32_t Source, uint32_t PLLM, uint32_t PLLN, 
4030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4031:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLCFGR, RCC_PLLCFGR_PLLSRC | RCC_PLLCFGR_PLLM, Source | PLLM);
4032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   MODIFY_REG(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN | RCC_PLLI2SCFGR_PLLI2SR, PLLN << RCC_PLLI2SCF
4033:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4034:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4035:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4036:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL multiplication factor for VCO
4037:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SN      LL_RCC_PLLI2S_GetN
4038:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Between 50 and 432
4039:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4040:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetN(void)
4041:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4042:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SN) >> RCC_PLLI2SCFGR_PLLI2SN_Pos
4043:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4044:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4045:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4046:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SQ
4047:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SQ      LL_RCC_PLLI2S_GetQ
4048:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4049:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_2
4050:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_3
4051:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_4
4052:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_5
4053:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_6
4054:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_7
4055:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_8
4056:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_9
4057:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_10
4058:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_11
4059:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_12
4060:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_13
4061:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_14
4062:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SQ_DIV_15
4063:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4064:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetQ(void)
4065:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4066:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SQ));
4067:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4068:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4069:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4070:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SR
4071:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLI2SCLK (I2S clock)
4072:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SR      LL_RCC_PLLI2S_GetR
4073:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4074:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_2
4075:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_3
4076:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_4
4077:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_5
4078:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_6
ARM GAS  /tmp/ccqw5Uyy.s 			page 86


4079:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SR_DIV_7
4080:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4081:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetR(void)
4082:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4083:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SR));
4084:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4085:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4086:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #if defined(RCC_PLLI2SCFGR_PLLI2SP)
4087:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4088:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SP
4089:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used for PLLSPDIFRXCLK (SPDIFRX clock)
4090:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll PLLI2SCFGR  PLLI2SP      LL_RCC_PLLI2S_GetP
4091:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4092:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_2
4093:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_4
4094:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_6
4095:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SP_DIV_8
4096:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4097:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetP(void)
4098:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4099:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->PLLI2SCFGR, RCC_PLLI2SCFGR_PLLI2SP));
4100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** #endif /* RCC_PLLI2SCFGR_PLLI2SP */
4102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Get I2SPLL division factor for PLLI2SDIVQ
4105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @note used PLLSAI1CLK, PLLSAI2CLK selected (SAI1 and SAI2 clock)
4106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll DCKCFGR1   PLLI2SDIVQ      LL_RCC_PLLI2S_GetDIVQ
4107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval Returned value can be one of the following values:
4108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_1
4109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_2
4110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_3
4111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_4
4112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_5
4113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_6
4114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_7
4115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_8
4116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_9
4117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_10
4118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_11
4119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_12
4120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_13
4121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_14
4122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_15
4123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_16
4124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_17
4125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_18
4126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_19
4127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_20
4128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_21
4129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_22
4130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_23
4131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_24
4132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_25
4133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_26
4134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_27
4135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_28
ARM GAS  /tmp/ccqw5Uyy.s 			page 87


4136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_29
4137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_30
4138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_31
4139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   *         @arg @ref LL_RCC_PLLI2SDIVQ_DIV_32
4140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLI2S_GetDIVQ(void)
4142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (uint32_t)(READ_BIT(RCC->DCKCFGR1, RCC_DCKCFGR1_PLLI2SDIVQ));
4144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @}
4148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /** @defgroup RCC_LL_EF_PLLSAI PLLSAI
4151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @{
4152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Enable PLLSAI
4156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAION     LL_RCC_PLLSAI_Enable
4157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_Enable(void)
4160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   SET_BIT(RCC->CR, RCC_CR_PLLSAION);
4162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Disable PLLSAI
4166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAION     LL_RCC_PLLSAI_Disable
4167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval None
4168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE void LL_RCC_PLLSAI_Disable(void)
4170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   CLEAR_BIT(RCC->CR, RCC_CR_PLLSAION);
4172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
4173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
4174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** /**
4175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @brief  Check if PLLSAI Ready
4176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @rmtoll CR           PLLSAIRDY    LL_RCC_PLLSAI_IsReady
4177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   * @retval State of bit (1 or 0).
4178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   */
4179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** __STATIC_INLINE uint32_t LL_RCC_PLLSAI_IsReady(void)
 110              		.loc 2 4179 26 view .LVU32
 111              	.LBB57:
4180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
4181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****   return (READ_BIT(RCC->CR, RCC_CR_PLLSAIRDY) == (RCC_CR_PLLSAIRDY));
 112              		.loc 2 4181 3 view .LVU33
 113              		.loc 2 4181 11 is_stmt 0 view .LVU34
 114 000c 074B     		ldr	r3, .L9
 115 000e 1B68     		ldr	r3, [r3]
 116              	.LBE57:
 117              	.LBE56:
 118              		.loc 1 660 5 discriminator 1 view .LVU35
 119 0010 13F0005F 		tst	r3, #536870912
 120 0014 00D0     		beq	.L4
ARM GAS  /tmp/ccqw5Uyy.s 			page 88


 661:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 662:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* PLLSAI1 configuration cannot be modified */
 663:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 121              		.loc 1 663 12 view .LVU36
 122 0016 0120     		movs	r0, #1
 123              	.LVL7:
 124              	.L4:
 664:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 665:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Check if PLLI2S is busy*/
 666:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(LL_RCC_PLLI2S_IsReady() != 0U)
 125              		.loc 1 666 3 is_stmt 1 view .LVU37
 126              	.LBB58:
 127              	.LBI58:
3711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 128              		.loc 2 3711 26 view .LVU38
 129              	.LBB59:
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 130              		.loc 2 3713 3 view .LVU39
3713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 131              		.loc 2 3713 11 is_stmt 0 view .LVU40
 132 0018 044B     		ldr	r3, .L9
 133 001a 1B68     		ldr	r3, [r3]
 134              	.LBE59:
 135              	.LBE58:
 136              		.loc 1 666 5 discriminator 1 view .LVU41
 137 001c 13F0006F 		tst	r3, #134217728
 138 0020 00D0     		beq	.L5
 667:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 668:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* PLLI2S configuration cannot be modified */
 669:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = ERROR;
 139              		.loc 1 669 12 view .LVU42
 140 0022 0120     		movs	r0, #1
 141              	.LVL8:
 142              	.L5:
 670:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 671:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return status;
 143              		.loc 1 671 3 is_stmt 1 view .LVU43
 672:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 144              		.loc 1 672 1 is_stmt 0 view .LVU44
 145 0024 7047     		bx	lr
 146              	.LVL9:
 147              	.L6:
 656:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 148              		.loc 1 656 12 view .LVU45
 149 0026 0120     		movs	r0, #1
 150 0028 F0E7     		b	.L3
 151              	.L10:
 152 002a 00BF     		.align	2
 153              	.L9:
 154 002c 00380240 		.word	1073887232
 155              		.cfi_endproc
 156              	.LFE412:
 158              		.section	.text.LL_Init1msTick,"ax",%progbits
 159              		.align	1
 160              		.global	LL_Init1msTick
 161              		.syntax unified
 162              		.thumb
ARM GAS  /tmp/ccqw5Uyy.s 			page 89


 163              		.thumb_func
 165              	LL_Init1msTick:
 166              	.LVL10:
 167              	.LFB405:
 219:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Use frequency provided in argument */
 168              		.loc 1 219 1 is_stmt 1 view -0
 169              		.cfi_startproc
 170              		@ args = 0, pretend = 0, frame = 0
 171              		@ frame_needed = 0, uses_anonymous_args = 0
 172              		@ link register save eliminated.
 221:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 173              		.loc 1 221 3 view .LVU47
 174              	.LBB60:
 175              	.LBI60:
 176              		.file 3 "Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h"
   1:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @file    stm32f7xx_ll_utils.h
   4:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief   Header file of UTILS LL module.
   6:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   @verbatim
   7:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   ==============================================================================
   8:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                      ##### How to use this driver #####
   9:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   ==============================================================================
  10:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****     [..]
  11:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****     The LL UTILS driver contains a set of generic APIs that can be
  12:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****     used by user:
  13:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****       (+) Device electronic signature
  14:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****       (+) Timing functions
  15:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****       (+) PLL configuration functions
  16:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  17:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   @endverbatim
  18:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   ******************************************************************************
  19:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @attention
  20:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *
  21:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * Copyright (c) 2017 STMicroelectronics.
  22:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * All rights reserved.
  23:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *
  24:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * This software is licensed under terms that can be found in the LICENSE file
  25:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * in the root directory of this software component.
  26:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  27:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *
  28:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   ******************************************************************************
  29:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  30:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  31:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Define to prevent recursive inclusion -------------------------------------*/
  32:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #ifndef __STM32F7xx_LL_UTILS_H
  33:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define __STM32F7xx_LL_UTILS_H
  34:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  35:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #ifdef __cplusplus
  36:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** extern "C" {
  37:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #endif
  38:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  39:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Includes ------------------------------------------------------------------*/
  40:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #include "stm32f7xx.h"
  41:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  42:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @addtogroup STM32F7xx_LL_Driver
ARM GAS  /tmp/ccqw5Uyy.s 			page 90


  43:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
  44:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  45:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  46:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL UTILS
  47:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
  48:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  49:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  50:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Private types -------------------------------------------------------------*/
  51:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Private variables ---------------------------------------------------------*/
  52:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  53:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Private constants ---------------------------------------------------------*/
  54:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_Private_Constants UTILS Private Constants
  55:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
  56:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  57:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  58:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Max delay can be used in LL_mDelay */
  59:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_MAX_DELAY                  0xFFFFFFFFU
  60:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  61:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  62:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  * @brief Unique device ID register base address
  63:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  */
  64:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define UID_BASE_ADDRESS              UID_BASE
  65:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  66:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  67:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  * @brief Flash size data register base address
  68:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  */
  69:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define FLASHSIZE_BASE_ADDRESS        FLASHSIZE_BASE
  70:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  71:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  72:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  * @brief Package data register base address
  73:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****  */
  74:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define PACKAGE_BASE_ADDRESS          PACKAGE_BASE
  75:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  76:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  77:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
  78:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  79:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  80:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Private macros ------------------------------------------------------------*/
  81:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_Private_Macros UTILS Private Macros
  82:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
  83:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  84:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  85:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
  86:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  87:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Exported types ------------------------------------------------------------*/
  88:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_ES_INIT UTILS Exported structures
  89:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
  90:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  91:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
  92:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  UTILS PLL structure definition
  93:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
  94:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** typedef struct
  95:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
  96:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t PLLM;   /*!< Division factor for PLL VCO input clock.
  97:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This parameter can be a value of @ref RCC_LL_EC_PLLM_DIV
  98:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
  99:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This feature can be modified afterwards using unitary function
ARM GAS  /tmp/ccqw5Uyy.s 			page 91


 100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         @ref LL_RCC_PLL_ConfigDomain_SYS(). */
 101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t PLLN;   /*!< Multiplication factor for PLL VCO output clock.
 103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This parameter must be a number between Min_Data = 50 and Max_Data = 432
 104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This feature can be modified afterwards using unitary function
 106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         @ref LL_RCC_PLL_ConfigDomain_SYS(). */
 107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t PLLP;   /*!< Division for the main system clock.
 109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This parameter can be a value of @ref RCC_LL_EC_PLLP_DIV
 110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         This feature can be modified afterwards using unitary function
 112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                         @ref LL_RCC_PLL_ConfigDomain_SYS(). */
 113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** } LL_UTILS_PLLInitTypeDef;
 114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  UTILS System, AHB and APB buses clock configuration structure definition
 117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** typedef struct
 119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t AHBCLKDivider;         /*!< The AHB clock (HCLK) divider. This clock is derived from the
 121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This parameter can be a value of @ref RCC_LL_EC_SYSCLK_DIV
 122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This feature can be modified afterwards using unitary functi
 124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        @ref LL_RCC_SetAHBPrescaler(). */
 125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t APB1CLKDivider;        /*!< The APB1 clock (PCLK1) divider. This clock is derived from t
 127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This parameter can be a value of @ref RCC_LL_EC_APB1_DIV
 128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This feature can be modified afterwards using unitary functi
 130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        @ref LL_RCC_SetAPB1Prescaler(). */
 131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   uint32_t APB2CLKDivider;        /*!< The APB2 clock (PCLK2) divider. This clock is derived from t
 133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This parameter can be a value of @ref RCC_LL_EC_APB2_DIV
 134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        This feature can be modified afterwards using unitary functi
 136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****                                        @ref LL_RCC_SetAPB2Prescaler(). */
 137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** } LL_UTILS_ClkInitTypeDef;
 139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
 142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Exported constants --------------------------------------------------------*/
 145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_Exported_Constants UTILS Exported Constants
 146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_EC_HSE_BYPASS HSE Bypass activation
 150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_HSEBYPASS_OFF        0x00000000U       /*!< HSE Bypass is not enabled             
 153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_HSEBYPASS_ON         0x00000001U       /*!< HSE Bypass is enabled                 
 154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
 156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 92


 157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_EC_PACKAGETYPE PACKAGE TYPE
 159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_LQFP100                    0x00000100U /*!< LQFP100 package type      
 162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_LQFP144_WLCSP143           0x00000200U /*!< LQFP144 or WLCSP143 packag
 163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_WLCSP180_LQFP176_UFBGA176  0x00000300U /*!< WLCSP180, LQFP176 or UFBGA
 164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_LQFP176_LQFP208_TFBGA216   0x00000400U /*!< LQFP176, LQFP208 or TFBGA2
 165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_TFBGA216_LQFP176_LQFP208   0x00000500U /*!< LQFP176, LQFP208 or TFBGA2
 166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_LQFP176_TFBGA216_LQFP208   0x00000600U /*!< LQFP176, LQFP208 or TFBGA2
 167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** #define LL_UTILS_PACKAGETYPE_LQFP208_LQFP176_TFBGA216   0x00000700U /*!< LQFP176, LQFP208 or TFBGA2
 168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
 170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
 174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Exported macro ------------------------------------------------------------*/
 177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /* Exported functions --------------------------------------------------------*/
 179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_Exported_Functions UTILS Exported Functions
 180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_EF_DEVICE_ELECTRONIC_SIGNATURE DEVICE ELECTRONIC SIGNATURE
 184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  Get Word0 of the unique device identifier (UID based on 96 bits)
 189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval UID[31:0]
 190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE uint32_t LL_GetUID_Word0(void)
 192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   return (uint32_t)(READ_REG(*((uint32_t *)UID_BASE_ADDRESS)));
 194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** }
 195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  Get Word1 of the unique device identifier (UID based on 96 bits)
 198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval UID[63:32]
 199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE uint32_t LL_GetUID_Word1(void)
 201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   return (uint32_t)(READ_REG(*((uint32_t *)(UID_BASE_ADDRESS + 4U))));
 203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** }
 204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  Get Word2 of the unique device identifier (UID based on 96 bits)
 207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval UID[95:64]
 208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE uint32_t LL_GetUID_Word2(void)
 210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   return (uint32_t)(READ_REG(*((uint32_t *)(UID_BASE_ADDRESS + 8U))));
 212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** }
 213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
ARM GAS  /tmp/ccqw5Uyy.s 			page 93


 214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  Get Flash memory size
 216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @note   This bitfield indicates the size of the device Flash memory expressed in
 217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         Kbytes. As an example, 0x040 corresponds to 64 Kbytes.
 218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval FLASH_SIZE[15:0]: Flash memory size
 219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE uint32_t LL_GetFlashSize(void)
 221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   return (uint32_t)(READ_REG(*((uint32_t *)FLASHSIZE_BASE_ADDRESS)) & 0xFFFFU);
 223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** }
 224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  Get Package type
 227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval Returned value can be one of the following values:
 228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         @arg @ref LL_UTILS_PACKAGETYPE_LQFP100
 229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         @arg @ref LL_UTILS_PACKAGETYPE_LQFP144_WLCSP143 (*)
 230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         @arg @ref LL_UTILS_PACKAGETYPE_WLCSP180_LQFP176_UFBGA176 (*)
 231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         @arg @ref LL_UTILS_PACKAGETYPE_LQFP176_LQFP208_TFBGA216 (*)
 232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *
 233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         (*) value not defined in all devices.
 234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE uint32_t LL_GetPackageType(void)
 236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   return (uint32_t)(READ_REG(*((uint32_t *)PACKAGE_BASE_ADDRESS)) & 0x0700U);
 238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** }
 239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @}
 242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /** @defgroup UTILS_LL_EF_DELAY DELAY
 245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @{
 246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** 
 248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** /**
 249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @brief  This function configures the Cortex-M SysTick source of the time base.
 250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @param  HCLKFrequency HCLK frequency in Hz (can be calculated thanks to RCC helper macro)
 251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @note   When a RTOS is used, it is recommended to avoid changing the SysTick 
 252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   *         configuration by calling this function, for a delay use rather osDelay RTOS service.
 253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @param  Ticks Frequency of Ticks (Hz)
 254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   * @retval None
 255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   */
 256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** __STATIC_INLINE void LL_InitTick(uint32_t HCLKFrequency, uint32_t Ticks)
 177              		.loc 3 256 22 view .LVU48
 178              	.LBB61:
 257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h **** {
 258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   /* Configure the SysTick to have interrupt in 1ms time base */
 259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   SysTick->LOAD  = (uint32_t)((HCLKFrequency / Ticks) - 1UL);  /* set reload register */
 179              		.loc 3 259 3 view .LVU49
 180              		.loc 3 259 46 is_stmt 0 view .LVU50
 181 0000 064B     		ldr	r3, .L12
 182 0002 A3FB0023 		umull	r2, r3, r3, r0
 183 0006 9B09     		lsrs	r3, r3, #6
 184              		.loc 3 259 20 view .LVU51
 185 0008 013B     		subs	r3, r3, #1
 186              		.loc 3 259 18 view .LVU52
 187 000a 4FF0E022 		mov	r2, #-536813568
ARM GAS  /tmp/ccqw5Uyy.s 			page 94


 188 000e 5361     		str	r3, [r2, #20]
 260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   SysTick->VAL   = 0UL;                                       /* Load the SysTick Counter Value */
 189              		.loc 3 260 3 is_stmt 1 view .LVU53
 190              		.loc 3 260 18 is_stmt 0 view .LVU54
 191 0010 0023     		movs	r3, #0
 192 0012 9361     		str	r3, [r2, #24]
 261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_utils.h ****   SysTick->CTRL  = SysTick_CTRL_CLKSOURCE_Msk |
 193              		.loc 3 261 3 is_stmt 1 view .LVU55
 194              		.loc 3 261 18 is_stmt 0 view .LVU56
 195 0014 0523     		movs	r3, #5
 196 0016 1361     		str	r3, [r2, #16]
 197              	.LVL11:
 198              		.loc 3 261 18 view .LVU57
 199              	.LBE61:
 200              	.LBE60:
 222:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 201              		.loc 1 222 1 view .LVU58
 202 0018 7047     		bx	lr
 203              	.L13:
 204 001a 00BF     		.align	2
 205              	.L12:
 206 001c D34D6210 		.word	274877907
 207              		.cfi_endproc
 208              	.LFE405:
 210              		.section	.text.LL_mDelay,"ax",%progbits
 211              		.align	1
 212              		.global	LL_mDelay
 213              		.syntax unified
 214              		.thumb
 215              		.thumb_func
 217              	LL_mDelay:
 218              	.LVL12:
 219              	.LFB406:
 235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   __IO uint32_t  tmp = SysTick->CTRL;  /* Clear the COUNTFLAG first */
 220              		.loc 1 235 1 is_stmt 1 view -0
 221              		.cfi_startproc
 222              		@ args = 0, pretend = 0, frame = 8
 223              		@ frame_needed = 0, uses_anonymous_args = 0
 224              		@ link register save eliminated.
 235:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   __IO uint32_t  tmp = SysTick->CTRL;  /* Clear the COUNTFLAG first */
 225              		.loc 1 235 1 is_stmt 0 view .LVU60
 226 0000 82B0     		sub	sp, sp, #8
 227              	.LCFI0:
 228              		.cfi_def_cfa_offset 8
 236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Add this code to indicate that local variable is not used */
 229              		.loc 1 236 3 is_stmt 1 view .LVU61
 236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Add this code to indicate that local variable is not used */
 230              		.loc 1 236 31 is_stmt 0 view .LVU62
 231 0002 4FF0E023 		mov	r3, #-536813568
 232 0006 1B69     		ldr	r3, [r3, #16]
 236:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Add this code to indicate that local variable is not used */
 233              		.loc 1 236 18 view .LVU63
 234 0008 0193     		str	r3, [sp, #4]
 238:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 235              		.loc 1 238 3 is_stmt 1 view .LVU64
 238:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 236              		.loc 1 238 4 is_stmt 0 view .LVU65
ARM GAS  /tmp/ccqw5Uyy.s 			page 95


 237 000a 019B     		ldr	r3, [sp, #4]
 241:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 238              		.loc 1 241 3 is_stmt 1 view .LVU66
 241:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 239              		.loc 1 241 5 is_stmt 0 view .LVU67
 240 000c B0F1FF3F 		cmp	r0, #-1
 241 0010 00D0     		beq	.L17
 243:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 242              		.loc 1 243 5 is_stmt 1 view .LVU68
 243:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 243              		.loc 1 243 10 is_stmt 0 view .LVU69
 244 0012 0130     		adds	r0, r0, #1
 245              	.LVL13:
 246              	.L17:
 246:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 247              		.loc 1 246 10 is_stmt 1 view .LVU70
 248 0014 38B1     		cbz	r0, .L20
 248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 249              		.loc 1 248 5 view .LVU71
 248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 250              		.loc 1 248 16 is_stmt 0 view .LVU72
 251 0016 4FF0E023 		mov	r3, #-536813568
 252 001a 1B69     		ldr	r3, [r3, #16]
 248:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 253              		.loc 1 248 7 view .LVU73
 254 001c 13F4803F 		tst	r3, #65536
 255 0020 F8D0     		beq	.L17
 250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 256              		.loc 1 250 7 is_stmt 1 view .LVU74
 250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 257              		.loc 1 250 12 is_stmt 0 view .LVU75
 258 0022 0138     		subs	r0, r0, #1
 259              	.LVL14:
 250:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 260              		.loc 1 250 12 view .LVU76
 261 0024 F6E7     		b	.L17
 262              	.L20:
 253:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 263              		.loc 1 253 1 view .LVU77
 264 0026 02B0     		add	sp, sp, #8
 265              	.LCFI1:
 266              		.cfi_def_cfa_offset 0
 267              		@ sp needed
 268 0028 7047     		bx	lr
 269              		.cfi_endproc
 270              	.LFE406:
 272              		.section	.text.LL_SetSystemCoreClock,"ax",%progbits
 273              		.align	1
 274              		.global	LL_SetSystemCoreClock
 275              		.syntax unified
 276              		.thumb
 277              		.thumb_func
 279              	LL_SetSystemCoreClock:
 280              	.LVL15:
 281              	.LFB407:
 312:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* HCLK clock frequency */
 282              		.loc 1 312 1 is_stmt 1 view -0
ARM GAS  /tmp/ccqw5Uyy.s 			page 96


 283              		.cfi_startproc
 284              		@ args = 0, pretend = 0, frame = 0
 285              		@ frame_needed = 0, uses_anonymous_args = 0
 286              		@ link register save eliminated.
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 287              		.loc 1 314 3 view .LVU79
 314:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 288              		.loc 1 314 19 is_stmt 0 view .LVU80
 289 0000 014B     		ldr	r3, .L22
 290 0002 1860     		str	r0, [r3]
 315:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 291              		.loc 1 315 1 view .LVU81
 292 0004 7047     		bx	lr
 293              	.L23:
 294 0006 00BF     		.align	2
 295              	.L22:
 296 0008 00000000 		.word	SystemCoreClock
 297              		.cfi_endproc
 298              	.LFE407:
 300              		.section	.text.LL_SetFlashLatency,"ax",%progbits
 301              		.align	1
 302              		.global	LL_SetFlashLatency
 303              		.syntax unified
 304              		.thumb
 305              		.thumb_func
 307              	LL_SetFlashLatency:
 308              	.LVL16:
 309              	.LFB408:
 327:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t timeout;
 310              		.loc 1 327 1 is_stmt 1 view -0
 311              		.cfi_startproc
 312              		@ args = 0, pretend = 0, frame = 0
 313              		@ frame_needed = 0, uses_anonymous_args = 0
 314              		@ link register save eliminated.
 328:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t getlatency;
 315              		.loc 1 328 3 view .LVU83
 329:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t latency = LL_FLASH_LATENCY_0;  /* default value 0WS */
 316              		.loc 1 329 3 view .LVU84
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 317              		.loc 1 330 3 view .LVU85
 331:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 318              		.loc 1 331 3 view .LVU86
 334:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 319              		.loc 1 334 3 view .LVU87
 334:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 320              		.loc 1 334 5 is_stmt 0 view .LVU88
 321 0000 0028     		cmp	r0, #0
 322 0002 00F09880 		beq	.L32
 327:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t timeout;
 323              		.loc 1 327 1 view .LVU89
 324 0006 10B4     		push	{r4}
 325              	.LCFI2:
 326              		.cfi_def_cfa_offset 4
 327              		.cfi_offset 4, -4
 328 0008 0246     		mov	r2, r0
 340:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 329              		.loc 1 340 5 is_stmt 1 view .LVU90
ARM GAS  /tmp/ccqw5Uyy.s 			page 97


 330              	.LBB62:
 331              	.LBI62:
 332              		.file 4 "Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h"
   1:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @file    stm32f7xx_ll_pwr.h
   4:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief   Header file of PWR LL module.
   6:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * This software is licensed under terms that can be found in the LICENSE file
  13:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * in the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *
  16:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   ******************************************************************************
  17:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  18:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  19:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Define to prevent recursive inclusion -------------------------------------*/
  20:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #ifndef __STM32F7xx_LL_PWR_H
  21:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define __STM32F7xx_LL_PWR_H
  22:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  23:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #ifdef __cplusplus
  24:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** extern "C" {
  25:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #endif
  26:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  27:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Includes ------------------------------------------------------------------*/
  28:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #include "stm32f7xx.h"
  29:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  30:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @addtogroup STM32F7xx_LL_Driver
  31:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  32:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  33:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  34:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #if defined(PWR)
  35:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  36:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL PWR
  37:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  38:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  39:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  40:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Private types -------------------------------------------------------------*/
  41:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Private variables ---------------------------------------------------------*/
  42:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Private constants ---------------------------------------------------------*/
  43:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Private macros ------------------------------------------------------------*/
  44:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Exported types ------------------------------------------------------------*/
  45:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Exported constants --------------------------------------------------------*/
  46:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_Exported_Constants PWR Exported Constants
  47:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  48:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  49:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  50:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_CLEAR_FLAG Clear Flags Defines
  51:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief    Flags defines which can be used with LL_PWR_WriteReg function
  52:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  53:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  54:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR1_CSBF                    PWR_CR1_CSBF            /*!< Clear standby flag */
ARM GAS  /tmp/ccqw5Uyy.s 			page 98


  55:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  56:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF6                   PWR_CR2_CWUF6           /*!< Clear WKUP pin 6 */
  57:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF5                   PWR_CR2_CWUF5           /*!< Clear WKUP pin 5 */
  58:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF4                   PWR_CR2_CWUF4           /*!< Clear WKUP pin 4 */
  59:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF3                   PWR_CR2_CWUF3           /*!< Clear WKUP pin 3 */
  60:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF2                   PWR_CR2_CWUF2           /*!< Clear WKUP pin 2 */
  61:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CR2_CWUF1                   PWR_CR2_CWUF1           /*!< Clear WKUP pin 1 */
  62:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
  63:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
  64:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  65:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  66:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_GET_FLAG Get Flags Defines
  67:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief    Flags defines which can be used with LL_PWR_ReadReg function
  68:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  69:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  70:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_WUIF                   PWR_CSR1_WUIF           /*!< Wakeup flag */
  71:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_SBF                    PWR_CSR1_SBF            /*!< Standby flag */
  72:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_PVDO                   PWR_CSR1_PVDO           /*!< Power voltage detector outp
  73:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_BRR                    PWR_CSR1_BRR            /*!< Backup Regulator ready flag
  74:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_VOSRDY                 PWR_CSR1_VOSRDY         /*!< Voltage scaling select flag
  75:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_ODRDY                  PWR_CSR1_ODRDY          /*!< Over-drive mode ready */
  76:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_ODSWRDY                PWR_CSR1_ODSWRDY        /*!< Over-drive mode switching r
  77:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR1_UDRDY                  PWR_CSR1_UDRDY          /*!< Under-drive ready flag */
  78:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
  79:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP1                  PWR_CSR2_EWUP1          /*!< Enable WKUP pin 1 */
  80:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP2                  PWR_CSR2_EWUP2          /*!< Enable WKUP pin 2 */
  81:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP3                  PWR_CSR2_EWUP3          /*!< Enable WKUP pin 3 */
  82:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP4                  PWR_CSR2_EWUP4          /*!< Enable WKUP pin 4 */
  83:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP5                  PWR_CSR2_EWUP5          /*!< Enable WKUP pin 5 */
  84:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_CSR2_EWUP6                  PWR_CSR2_EWUP6          /*!< Enable WKUP pin 6 */
  85:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
  86:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
  87:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  88:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   
  89:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_MODE_PWR Mode Power
  90:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
  91:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
  92:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_MODE_STOP_MAINREGU                     0x00000000U                                  
  93:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_MODE_STOP_MAINREGU_UNDERDRIVE          (PWR_CR1_MRUDS | PWR_CR1_FPDS)               
  94:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_MODE_STOP_LPREGU                       PWR_CR1_LPDS                                 
  95:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_MODE_STOP_LPREGU_UNDERDRIVE            (PWR_CR1_LPDS | PWR_CR1_LPUDS | PWR_CR1_FPDS)
  96:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_MODE_STANDBY                           PWR_CR1_PDDS                                 
  97:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
  98:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
  99:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_REGU_VOLTAGE Regulator Voltage
 102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_REGU_VOLTAGE_SCALE3         PWR_CR1_VOS_0
 105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_REGU_VOLTAGE_SCALE2         PWR_CR1_VOS_1
 106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_REGU_VOLTAGE_SCALE1         (PWR_CR1_VOS_0 | PWR_CR1_VOS_1)
 107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_REGU_MODE_DS_MODE  Regulator Mode In Deep Sleep Mode
ARM GAS  /tmp/ccqw5Uyy.s 			page 99


 112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_REGU_DSMODE_MAIN        0x00000000U                    /*!< Voltage Regulator in mai
 115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_REGU_DSMODE_LOW_POWER   PWR_CR1_LPDS                   /*!< Voltage Regulator in low
 116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_PVDLEVEL Power Voltage Detector Level
 121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_0                  PWR_CR1_PLS_LEV0      /*!< Voltage threshold detected by
 124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_1                  PWR_CR1_PLS_LEV1      /*!< Voltage threshold detected by
 125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_2                  PWR_CR1_PLS_LEV2      /*!< Voltage threshold detected by
 126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_3                  PWR_CR1_PLS_LEV3      /*!< Voltage threshold detected by
 127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_4                  PWR_CR1_PLS_LEV4      /*!< Voltage threshold detected by
 128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_5                  PWR_CR1_PLS_LEV5      /*!< Voltage threshold detected by
 129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_6                  PWR_CR1_PLS_LEV6      /*!< Voltage threshold detected by
 130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_PVDLEVEL_7                  PWR_CR1_PLS_LEV7      /*!< Voltage threshold detected by
 131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EC_WAKEUP_PIN  Wakeup Pins
 136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN1                 PWR_CSR2_EWUP1        /*!< WKUP pin 1 : PA0  */
 139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN2                 PWR_CSR2_EWUP2        /*!< WKUP pin 2 : PA2  */
 140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN3                 PWR_CSR2_EWUP3        /*!< WKUP pin 3 : PC1  */
 141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN4                 PWR_CSR2_EWUP4        /*!< WKUP pin 4 : PC13 */
 142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN5                 PWR_CSR2_EWUP5        /*!< WKUP pin 5 : PI8  */
 143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WAKEUP_PIN6                 PWR_CSR2_EWUP6        /*!< WKUP pin 6 : PI11 */
 144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   
 148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Exported macro ------------------------------------------------------------*/
 152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_Exported_Macros PWR Exported Macros
 153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EM_WRITE_READ Common write and read registers Macros
 157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Write a value in PWR register
 162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @param  __REG__ Register to be written
 163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @param  __VALUE__ Value to be written in the register
 164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_WriteReg(__REG__, __VALUE__) WRITE_REG(PWR->__REG__, (__VALUE__))
 167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
ARM GAS  /tmp/ccqw5Uyy.s 			page 100


 169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Read a value in PWR register
 170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @param  __REG__ Register to be read
 171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval Register value
 172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** #define LL_PWR_ReadReg(__REG__) READ_REG(PWR->__REG__)
 174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @}
 180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /* Exported functions --------------------------------------------------------*/
 182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_Exported_Functions PWR Exported Functions
 183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /** @defgroup PWR_LL_EF_Configuration Configuration
 187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @{
 188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Enable Under Drive Mode
 192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    UDEN       LL_PWR_EnableUnderDriveMode
 193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @note  This mode is enabled only with STOP low power mode.
 194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        In this mode, the 1.2V domain is preserved in reduced leakage mode. This 
 195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        mode is only available when the main Regulator or the low power Regulator 
 196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        is in low voltage mode.      
 197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @note  If the Under-drive mode was enabled, it is automatically disabled after 
 198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        exiting Stop mode. 
 199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        When the voltage Regulator operates in Under-drive mode, an additional  
 200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *        startup delay is induced when waking up from Stop mode.
 201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_EnableUnderDriveMode(void)
 204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   SET_BIT(PWR->CR1, PWR_CR1_UDEN);
 206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Disable Under Drive Mode
 210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    UDEN       LL_PWR_DisableUnderDriveMode
 211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_DisableUnderDriveMode(void)
 214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   CLEAR_BIT(PWR->CR1, PWR_CR1_UDEN);
 216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Check if Under Drive Mode is enabled
 220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    UDEN       LL_PWR_IsEnabledUnderDriveMode
 221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval State of bit (1 or 0).
 222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE uint32_t LL_PWR_IsEnabledUnderDriveMode(void)
 224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   return (READ_BIT(PWR->CR1, PWR_CR1_UDEN) == (PWR_CR1_UDEN));
ARM GAS  /tmp/ccqw5Uyy.s 			page 101


 226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Enable Over drive switching
 230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODSWEN       LL_PWR_EnableOverDriveSwitching
 231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_EnableOverDriveSwitching(void)
 234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   SET_BIT(PWR->CR1, PWR_CR1_ODSWEN);
 236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Disable Over drive switching
 240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODSWEN       LL_PWR_DisableOverDriveSwitching
 241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_DisableOverDriveSwitching(void)
 244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   CLEAR_BIT(PWR->CR1, PWR_CR1_ODSWEN);
 246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Check if Over drive switching is enabled
 250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODSWEN       LL_PWR_IsEnabledOverDriveSwitching
 251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval State of bit (1 or 0).
 252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE uint32_t LL_PWR_IsEnabledOverDriveSwitching(void)
 254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   return (READ_BIT(PWR->CR1, PWR_CR1_ODSWEN) == (PWR_CR1_ODSWEN));
 256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Enable Over drive Mode
 260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODEN       LL_PWR_EnableOverDriveMode
 261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_EnableOverDriveMode(void)
 264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   SET_BIT(PWR->CR1, PWR_CR1_ODEN);
 266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Disable Over drive Mode
 270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODEN       LL_PWR_DisableOverDriveMode
 271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_DisableOverDriveMode(void)
 274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   CLEAR_BIT(PWR->CR1, PWR_CR1_ODEN);
 276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Check if Over drive switching is enabled
 280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    ODEN       LL_PWR_IsEnabledOverDriveMode
 281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval State of bit (1 or 0).
 282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
ARM GAS  /tmp/ccqw5Uyy.s 			page 102


 283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE uint32_t LL_PWR_IsEnabledOverDriveMode(void)
 284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   return (READ_BIT(PWR->CR1, PWR_CR1_ODEN) == (PWR_CR1_ODEN));
 286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Set the main internal Regulator output voltage
 290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    VOS       LL_PWR_SetRegulVoltageScaling
 291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @param  VoltageScaling This parameter can be one of the following values:
 292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE1
 293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE2
 294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE3
 295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval None
 296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE void LL_PWR_SetRegulVoltageScaling(uint32_t VoltageScaling)
 298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   MODIFY_REG(PWR->CR1, PWR_CR1_VOS, VoltageScaling);
 300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** 
 302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** /**
 303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @brief  Get the main internal Regulator output voltage
 304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @rmtoll CR1    VOS       LL_PWR_GetRegulVoltageScaling
 305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   * @retval Returned value can be one of the following values:
 306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE1
 307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE2
 308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   *         @arg @ref LL_PWR_REGU_VOLTAGE_SCALE3
 309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   */
 310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** __STATIC_INLINE uint32_t LL_PWR_GetRegulVoltageScaling(void)
 333              		.loc 4 310 26 view .LVU91
 334              	.LBB63:
 311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h ****   return (uint32_t)(READ_BIT(PWR->CR1, PWR_CR1_VOS));
 335              		.loc 4 312 3 view .LVU92
 336              		.loc 4 312 21 is_stmt 0 view .LVU93
 337 000a 4D4B     		ldr	r3, .L56
 338 000c 1B68     		ldr	r3, [r3]
 339              		.loc 4 312 10 view .LVU94
 340 000e 03F44043 		and	r3, r3, #49152
 341              	.LBE63:
 342              	.LBE62:
 340:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 343              		.loc 1 340 7 discriminator 1 view .LVU95
 344 0012 B3F5404F 		cmp	r3, #49152
 345 0016 14D0     		beq	.L54
 385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 346              		.loc 1 385 10 is_stmt 1 view .LVU96
 347              	.LBB64:
 348              	.LBI64:
 310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 349              		.loc 4 310 26 view .LVU97
 350              	.LBB65:
 351              		.loc 4 312 3 view .LVU98
 352              		.loc 4 312 21 is_stmt 0 view .LVU99
 353 0018 494B     		ldr	r3, .L56
 354 001a 1B68     		ldr	r3, [r3]
 355              		.loc 4 312 10 view .LVU100
 356 001c 03F44043 		and	r3, r3, #49152
ARM GAS  /tmp/ccqw5Uyy.s 			page 103


 357              	.LBE65:
 358              	.LBE64:
 385:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 359              		.loc 1 385 12 discriminator 1 view .LVU101
 360 0020 B3F5004F 		cmp	r3, #32768
 361 0024 41D0     		beq	.L55
 419:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 362              		.loc 1 419 7 is_stmt 1 view .LVU102
 419:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 363              		.loc 1 419 9 is_stmt 0 view .LVU103
 364 0026 474B     		ldr	r3, .L56+4
 365 0028 9842     		cmp	r0, r3
 366 002a 64D8     		bhi	.L44
 424:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 367              		.loc 1 424 12 is_stmt 1 view .LVU104
 424:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 368              		.loc 1 424 14 is_stmt 0 view .LVU105
 369 002c 464B     		ldr	r3, .L56+8
 370 002e 9842     		cmp	r0, r3
 371 0030 7BD8     		bhi	.L45
 429:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 372              		.loc 1 429 12 is_stmt 1 view .LVU106
 429:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 373              		.loc 1 429 14 is_stmt 0 view .LVU107
 374 0032 464B     		ldr	r3, .L56+12
 375 0034 9842     		cmp	r0, r3
 376 0036 7AD8     		bhi	.L46
 436:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 377              		.loc 1 436 9 is_stmt 1 view .LVU108
 436:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 378              		.loc 1 436 11 is_stmt 0 view .LVU109
 379 0038 454B     		ldr	r3, .L56+16
 380 003a 9842     		cmp	r0, r3
 381 003c 79D8     		bhi	.L47
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 382              		.loc 1 330 12 view .LVU110
 383 003e 0020     		movs	r0, #0
 384              	.LVL17:
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 385              		.loc 1 330 12 view .LVU111
 386 0040 5AE0     		b	.L28
 387              	.LVL18:
 388              	.L54:
 342:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 389              		.loc 1 342 7 is_stmt 1 view .LVU112
 390              	.LBB66:
 391              	.LBI66:
 283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** {
 392              		.loc 4 283 26 view .LVU113
 393              	.LBB67:
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 394              		.loc 4 285 3 view .LVU114
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 395              		.loc 4 285 11 is_stmt 0 view .LVU115
 396 0042 3F4B     		ldr	r3, .L56
 397 0044 1868     		ldr	r0, [r3]
 398              	.LVL19:
ARM GAS  /tmp/ccqw5Uyy.s 			page 104


 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_pwr.h **** }
 399              		.loc 4 285 11 view .LVU116
 400              	.LBE67:
 401              	.LBE66:
 342:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 402              		.loc 1 342 9 discriminator 1 view .LVU117
 403 0046 10F48030 		ands	r0, r0, #65536
 404 004a 03D0     		beq	.L27
 344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           {
 405              		.loc 1 344 11 is_stmt 1 view .LVU118
 344:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           {
 406              		.loc 1 344 13 is_stmt 0 view .LVU119
 407 004c 414B     		ldr	r3, .L56+20
 408 004e 9A42     		cmp	r2, r3
 409 0050 29D9     		bls	.L33
 347:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           }
 410              		.loc 1 347 21 view .LVU120
 411 0052 0720     		movs	r0, #7
 412              	.L27:
 413              	.LVL20:
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 414              		.loc 1 355 7 is_stmt 1 view .LVU121
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 415              		.loc 1 355 68 is_stmt 0 view .LVU122
 416 0054 B0FA80F3 		clz	r3, r0
 417 0058 5B09     		lsrs	r3, r3, #5
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 418              		.loc 1 355 56 view .LVU123
 419 005a 3F4C     		ldr	r4, .L56+24
 420 005c A242     		cmp	r2, r4
 421 005e 94BF     		ite	ls
 422 0060 0021     		movls	r1, #0
 423 0062 03F00101 		andhi	r1, r3, #1
 355:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 424              		.loc 1 355 9 view .LVU124
 425 0066 0029     		cmp	r1, #0
 426 0068 33D1     		bne	.L34
 360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 427              		.loc 1 360 12 is_stmt 1 view .LVU125
 360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 428              		.loc 1 360 61 is_stmt 0 view .LVU126
 429 006a 364C     		ldr	r4, .L56+4
 430 006c A242     		cmp	r2, r4
 431 006e 94BF     		ite	ls
 432 0070 0021     		movls	r1, #0
 433 0072 03F00101 		andhi	r1, r3, #1
 360:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 434              		.loc 1 360 14 view .LVU127
 435 0076 71BB     		cbnz	r1, .L35
 365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 436              		.loc 1 365 12 is_stmt 1 view .LVU128
 365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 437              		.loc 1 365 61 is_stmt 0 view .LVU129
 438 0078 334C     		ldr	r4, .L56+8
 439 007a A242     		cmp	r2, r4
 440 007c 94BF     		ite	ls
 441 007e 0021     		movls	r1, #0
ARM GAS  /tmp/ccqw5Uyy.s 			page 105


 442 0080 03F00101 		andhi	r1, r3, #1
 365:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 443              		.loc 1 365 14 view .LVU130
 444 0084 49BB     		cbnz	r1, .L36
 370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 445              		.loc 1 370 12 is_stmt 1 view .LVU131
 370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 446              		.loc 1 370 61 is_stmt 0 view .LVU132
 447 0086 314C     		ldr	r4, .L56+12
 448 0088 A242     		cmp	r2, r4
 449 008a 94BF     		ite	ls
 450 008c 0021     		movls	r1, #0
 451 008e 03F00101 		andhi	r1, r3, #1
 370:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 452              		.loc 1 370 14 view .LVU133
 453 0092 21BB     		cbnz	r1, .L37
 377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 454              		.loc 1 377 9 is_stmt 1 view .LVU134
 377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 455              		.loc 1 377 58 is_stmt 0 view .LVU135
 456 0094 2E49     		ldr	r1, .L56+16
 457 0096 8A42     		cmp	r2, r1
 458 0098 94BF     		ite	ls
 459 009a 0023     		movls	r3, #0
 460 009c 03F00103 		andhi	r3, r3, #1
 377:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 461              		.loc 1 377 11 view .LVU136
 462 00a0 53B3     		cbz	r3, .L28
 380:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 463              		.loc 1 380 19 view .LVU137
 464 00a2 0120     		movs	r0, #1
 465              	.LVL21:
 380:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 466              		.loc 1 380 19 view .LVU138
 467 00a4 28E0     		b	.L28
 468              	.LVL22:
 469              	.L33:
 352:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****           }
 470              		.loc 1 352 21 view .LVU139
 471 00a6 0620     		movs	r0, #6
 472 00a8 D4E7     		b	.L27
 473              	.LVL23:
 474              	.L55:
 387:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 475              		.loc 1 387 7 is_stmt 1 view .LVU140
 387:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 476              		.loc 1 387 9 is_stmt 0 view .LVU141
 477 00aa 03F10F63 		add	r3, r3, #149946368
 478 00ae 03F5A343 		add	r3, r3, #20864
 479 00b2 9842     		cmp	r0, r3
 480 00b4 15D8     		bhi	.L39
 392:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 481              		.loc 1 392 12 is_stmt 1 view .LVU142
 392:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 482              		.loc 1 392 14 is_stmt 0 view .LVU143
 483 00b6 234B     		ldr	r3, .L56+4
 484 00b8 9842     		cmp	r0, r3
ARM GAS  /tmp/ccqw5Uyy.s 			page 106


 485 00ba 14D8     		bhi	.L40
 397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 486              		.loc 1 397 12 is_stmt 1 view .LVU144
 397:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 487              		.loc 1 397 14 is_stmt 0 view .LVU145
 488 00bc 224B     		ldr	r3, .L56+8
 489 00be 9842     		cmp	r0, r3
 490 00c0 13D8     		bhi	.L41
 402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 491              		.loc 1 402 12 is_stmt 1 view .LVU146
 402:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 492              		.loc 1 402 14 is_stmt 0 view .LVU147
 493 00c2 224B     		ldr	r3, .L56+12
 494 00c4 9842     		cmp	r0, r3
 495 00c6 12D8     		bhi	.L42
 409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 496              		.loc 1 409 9 is_stmt 1 view .LVU148
 409:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         {
 497              		.loc 1 409 11 is_stmt 0 view .LVU149
 498 00c8 214B     		ldr	r3, .L56+16
 499 00ca 9842     		cmp	r0, r3
 500 00cc 11D8     		bhi	.L43
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 501              		.loc 1 330 12 view .LVU150
 502 00ce 0020     		movs	r0, #0
 503              	.LVL24:
 330:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 504              		.loc 1 330 12 view .LVU151
 505 00d0 12E0     		b	.L28
 506              	.LVL25:
 507              	.L34:
 358:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 508              		.loc 1 358 17 view .LVU152
 509 00d2 0520     		movs	r0, #5
 510              	.LVL26:
 358:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 511              		.loc 1 358 17 view .LVU153
 512 00d4 10E0     		b	.L28
 513              	.LVL27:
 514              	.L35:
 363:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 515              		.loc 1 363 17 view .LVU154
 516 00d6 0420     		movs	r0, #4
 517              	.LVL28:
 363:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 518              		.loc 1 363 17 view .LVU155
 519 00d8 0EE0     		b	.L28
 520              	.LVL29:
 521              	.L36:
 368:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 522              		.loc 1 368 17 view .LVU156
 523 00da 0320     		movs	r0, #3
 524              	.LVL30:
 368:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 525              		.loc 1 368 17 view .LVU157
 526 00dc 0CE0     		b	.L28
 527              	.LVL31:
ARM GAS  /tmp/ccqw5Uyy.s 			page 107


 528              	.L37:
 373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 529              		.loc 1 373 17 view .LVU158
 530 00de 0220     		movs	r0, #2
 531              	.LVL32:
 373:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 532              		.loc 1 373 17 view .LVU159
 533 00e0 0AE0     		b	.L28
 534              	.LVL33:
 535              	.L39:
 390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 536              		.loc 1 390 17 view .LVU160
 537 00e2 0520     		movs	r0, #5
 538              	.LVL34:
 390:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 539              		.loc 1 390 17 view .LVU161
 540 00e4 08E0     		b	.L28
 541              	.LVL35:
 542              	.L40:
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 543              		.loc 1 395 17 view .LVU162
 544 00e6 0420     		movs	r0, #4
 545              	.LVL36:
 395:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 546              		.loc 1 395 17 view .LVU163
 547 00e8 06E0     		b	.L28
 548              	.LVL37:
 549              	.L41:
 400:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 550              		.loc 1 400 17 view .LVU164
 551 00ea 0320     		movs	r0, #3
 552              	.LVL38:
 400:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 553              		.loc 1 400 17 view .LVU165
 554 00ec 04E0     		b	.L28
 555              	.LVL39:
 556              	.L42:
 405:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 557              		.loc 1 405 17 view .LVU166
 558 00ee 0220     		movs	r0, #2
 559              	.LVL40:
 405:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 560              		.loc 1 405 17 view .LVU167
 561 00f0 02E0     		b	.L28
 562              	.LVL41:
 563              	.L43:
 412:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 564              		.loc 1 412 19 view .LVU168
 565 00f2 0120     		movs	r0, #1
 566              	.LVL42:
 412:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 567              		.loc 1 412 19 view .LVU169
 568 00f4 00E0     		b	.L28
 569              	.LVL43:
 570              	.L44:
 422:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 571              		.loc 1 422 17 view .LVU170
ARM GAS  /tmp/ccqw5Uyy.s 			page 108


 572 00f6 0420     		movs	r0, #4
 573              	.LVL44:
 574              	.L28:
 445:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 575              		.loc 1 445 5 is_stmt 1 view .LVU171
 447:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 576              		.loc 1 447 7 view .LVU172
 577              	.LBB68:
 578              	.LBI68:
 579              		.file 5 "Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h"
   1:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
   2:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ******************************************************************************
   3:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @file    stm32f7xx_ll_system.h
   4:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @author  MCD Application Team
   5:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief   Header file of SYSTEM LL module.
   6:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ******************************************************************************
   7:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @attention
   8:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
   9:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * Copyright (c) 2017 STMicroelectronics.
  10:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * All rights reserved.
  11:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
  12:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * This software is licensed under terms that can be found in the LICENSE file
  13:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * in the root directory of this software component.
  14:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  15:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
  16:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ******************************************************************************
  17:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   @verbatim
  18:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ==============================================================================
  19:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                      ##### How to use this driver #####
  20:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ==============================================================================
  21:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****     [..]
  22:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****     The LL SYSTEM driver contains a set of generic APIs that can be
  23:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****     used by user:
  24:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****       (+) Some of the FLASH features need to be handled in the SYSTEM file.
  25:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****       (+) Access to DBGCMU registers
  26:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****       (+) Access to SYSCFG registers
  27:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  28:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   @endverbatim
  29:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   ******************************************************************************
  30:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  31:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  32:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Define to prevent recursive inclusion -------------------------------------*/
  33:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #ifndef __STM32F7xx_LL_SYSTEM_H
  34:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define __STM32F7xx_LL_SYSTEM_H
  35:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  36:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #ifdef __cplusplus
  37:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** extern "C" {
  38:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif
  39:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  40:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Includes ------------------------------------------------------------------*/
  41:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #include "stm32f7xx.h"
  42:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  43:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @addtogroup STM32F7xx_LL_Driver
  44:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
  45:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  46:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  47:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined (FLASH) || defined (SYSCFG) || defined (DBGMCU)
ARM GAS  /tmp/ccqw5Uyy.s 			page 109


  48:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  49:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL SYSTEM
  50:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
  51:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  52:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  53:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Private types -------------------------------------------------------------*/
  54:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Private variables ---------------------------------------------------------*/
  55:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  56:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Private constants ---------------------------------------------------------*/
  57:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_Private_Constants SYSTEM Private Constants
  58:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
  59:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  60:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  61:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
  62:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
  63:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  64:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  65:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Private macros ------------------------------------------------------------*/
  66:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  67:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Exported types ------------------------------------------------------------*/
  68:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Exported constants --------------------------------------------------------*/
  69:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_Exported_Constants SYSTEM Exported Constants
  70:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
  71:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  72:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  73:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_REMAP SYSCFG REMAP
  74:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** * @{
  75:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** */
  76:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_REMAP_BOOT0               0x00000000U                                         /*!
  77:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_REMAP_BOOT1               SYSCFG_MEMRMP_MEM_BOOT                              /*!
  78:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
  79:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
  80:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  81:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  82:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  83:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_MEMRMP_SWP_FB)
  84:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_BANKMODE SYSCFG BANK MODE
  85:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
  86:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  87:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_BANKMODE_BANK1          0x00000000U              /*!< Flash Bank 1 base address m
  88:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                                                                       and Flash Bank 2 base address
  89:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  90:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_BANKMODE_BANK2          SYSCFG_MEMRMP_SWP_FB     /*!< Flash Bank 2 base address m
  91:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                                                                       and Flash Bank 1 base address
  92:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
  93:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
  94:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
  95:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_MEMRMP_SWP_FB */
  96:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
  97:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_MII_RMII_SEL)
  98:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****  /** @defgroup SYSTEM_LL_EC_PMC SYSCFG PMC
  99:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** * @{
 100:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** */
 101:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_PMC_ETHMII               0x00000000U                                         /*!<
 102:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_PMC_ETHRMII              (uint32_t)SYSCFG_PMC_MII_RMII_SEL                   /*!<
 103:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 104:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
ARM GAS  /tmp/ccqw5Uyy.s 			page 110


 105:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 106:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 107:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_MII_RMII_SEL */
 108:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 109:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_I2C_FASTMODEPLUS SYSCFG I2C FASTMODEPLUS
 110:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 111:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 112:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_I2C1_FMP)
 113:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_I2C1        SYSCFG_PMC_I2C1_FMP       /*!< Enable Fast Mode Plus
 114:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_I2C2        SYSCFG_PMC_I2C2_FMP       /*!< Enable Fast Mode Plus
 115:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_I2C3        SYSCFG_PMC_I2C3_FMP       /*!< Enable Fast Mode Plus
 116:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_I2C1_FMP */
 117:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_I2C4_FMP)
 118:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_I2C4        SYSCFG_PMC_I2C4_FMP       /*!< Enable Fast Mode Plus
 119:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_I2C4_FMP */
 120:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_I2C_PB6_FMP)
 121:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_PB6         SYSCFG_PMC_I2C_PB6_FMP    /*!< Enable Fast Mode Plus
 122:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_PB7         SYSCFG_PMC_I2C_PB7_FMP    /*!< Enable Fast Mode Plus
 123:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_PB8         SYSCFG_PMC_I2C_PB8_FMP    /*!< Enable Fast Mode Plus
 124:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_I2C_FASTMODEPLUS_PB9         SYSCFG_PMC_I2C_PB9_FMP    /*!< Enable Fast Mode Plus
 125:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_I2C_PB6_FMP */
 126:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 127:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 128:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 129:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 130:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_EXTI_PORT SYSCFG EXTI PORT
 131:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 133:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTA               0U               /*!< EXTI PORT A                       
 134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTB               1U               /*!< EXTI PORT B                       
 135:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTC               2U               /*!< EXTI PORT C                       
 136:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTD               3U               /*!< EXTI PORT D                       
 137:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTE               4U               /*!< EXTI PORT E                       
 138:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(GPIOF)
 139:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTF               5U               /*!< EXTI PORT F                       
 140:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* GPIOF */
 141:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(GPIOG)
 142:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTG               6U               /*!< EXTI PORT G                       
 143:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* GPIOG */
 144:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTH               7U               /*!< EXTI PORT H                       
 145:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(GPIOI)
 146:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTI               8U               /*!< EXTI PORT I                       
 147:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* GPIOI */
 148:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(GPIOJ)
 149:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTJ               9U               /*!< EXTI PORT J                       
 150:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* GPIOJ */
 151:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(GPIOK)
 152:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_PORTK               10U              /*!< EXTI PORT k                       
 153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* GPIOK */
 154:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 156:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 157:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 158:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_EXTI_LINE SYSCFG EXTI LINE
 159:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 160:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 161:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE0               (0x000FU << 16U | 0U)  /*!< EXTI_POSITION_0  | EXTICR[0]
ARM GAS  /tmp/ccqw5Uyy.s 			page 111


 162:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE1               (0x00F0U << 16U | 0U)  /*!< EXTI_POSITION_4  | EXTICR[0]
 163:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE2               (0x0F00U << 16U | 0U)  /*!< EXTI_POSITION_8  | EXTICR[0]
 164:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE3               (0xF000U << 16U | 0U)  /*!< EXTI_POSITION_12 | EXTICR[0]
 165:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE4               (0x000FU << 16U | 1U)  /*!< EXTI_POSITION_0  | EXTICR[1]
 166:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE5               (0x00F0U << 16U | 1U)  /*!< EXTI_POSITION_4  | EXTICR[1]
 167:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE6               (0x0F00U << 16U | 1U)  /*!< EXTI_POSITION_8  | EXTICR[1]
 168:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE7               (0xF000U << 16U | 1U)  /*!< EXTI_POSITION_12 | EXTICR[1]
 169:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE8               (0x000FU << 16U | 2U)  /*!< EXTI_POSITION_0  | EXTICR[2]
 170:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE9               (0x00F0U << 16U | 2U)  /*!< EXTI_POSITION_4  | EXTICR[2]
 171:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE10              (0x0F00U << 16U | 2U)  /*!< EXTI_POSITION_8  | EXTICR[2]
 172:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE11              (0xF000U << 16U | 2U)  /*!< EXTI_POSITION_12 | EXTICR[2]
 173:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE12              (0x000FU << 16U | 3U)  /*!< EXTI_POSITION_0  | EXTICR[3]
 174:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE13              (0x00F0U << 16U | 3U)  /*!< EXTI_POSITION_4  | EXTICR[3]
 175:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE14              (0x0F00U << 16U | 3U)  /*!< EXTI_POSITION_8  | EXTICR[3]
 176:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_EXTI_LINE15              (0xF000U << 16U | 3U)  /*!< EXTI_POSITION_12 | EXTICR[3]
 177:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 178:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 179:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 180:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 181:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_TIMBREAK SYSCFG TIMER BREAK
 182:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 183:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 184:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_CBR_CLL)
 185:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_TIMBREAK_LOCKUP          SYSCFG_CBR_CLL     /*!< Enables and locks the Lockup out
 186:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                                                                    lockup state) of Cortex-M7 with 
 187:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_TIMBREAK_PVD             SYSCFG_CBR_PVDL    /*!< Enables and locks the PVD connec
 188:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                                                                    It also locks (write protect) th
 189:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****                                                                    of the power controller */
 190:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_CBR_CLL */
 191:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 192:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 193:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 194:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_CMP_PD SYSCFG CMP PD
 195:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 196:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 197:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_DISABLE_CMP_PD          0x00000000U             /*!< I/O compensation cell power-
 198:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_SYSCFG_ENABLE_CMP_PD           SYSCFG_CMPCR_CMP_PD     /*!< I/O compensation cell enable
 199:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 200:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 201:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 202:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 203:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_TRACE DBGMCU TRACE Pin Assignment
 204:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 205:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 206:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_TRACE_NONE               0x00000000U                                     /*!< TRA
 207:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_TRACE_ASYNCH             DBGMCU_CR_TRACE_IOEN                            /*!< TRA
 208:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_TRACE_SYNCH_SIZE1        (DBGMCU_CR_TRACE_IOEN | DBGMCU_CR_TRACE_MODE_0) /*!< TRA
 209:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_TRACE_SYNCH_SIZE2        (DBGMCU_CR_TRACE_IOEN | DBGMCU_CR_TRACE_MODE_1) /*!< TRA
 210:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_TRACE_SYNCH_SIZE4        (DBGMCU_CR_TRACE_IOEN | DBGMCU_CR_TRACE_MODE)   /*!< TRA
 211:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 212:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 213:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 215:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_APB1_GRP1_STOP_IP DBGMCU APB1 GRP1 STOP IP
 216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 217:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 218:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM2_STOP      DBGMCU_APB1_FZ_DBG_TIM2_STOP          /*!< TIM2 counter 
ARM GAS  /tmp/ccqw5Uyy.s 			page 112


 219:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM3_STOP      DBGMCU_APB1_FZ_DBG_TIM3_STOP          /*!< TIM3 counter 
 220:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM4_STOP      DBGMCU_APB1_FZ_DBG_TIM4_STOP          /*!< TIM4 counter 
 221:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM5_STOP      DBGMCU_APB1_FZ_DBG_TIM5_STOP          /*!< TIM5 counter 
 222:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM6_STOP      DBGMCU_APB1_FZ_DBG_TIM6_STOP          /*!< TIM6 counter 
 223:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM7_STOP      DBGMCU_APB1_FZ_DBG_TIM7_STOP          /*!< TIM7 counter 
 224:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM12_STOP     DBGMCU_APB1_FZ_DBG_TIM12_STOP         /*!< TIM12 counter
 225:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM13_STOP     DBGMCU_APB1_FZ_DBG_TIM13_STOP         /*!< TIM13 counter
 226:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_TIM14_STOP     DBGMCU_APB1_FZ_DBG_TIM14_STOP         /*!< TIM14 counter
 227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_LPTIM1_STOP    DBGMCU_APB1_FZ_DBG_LPTIM1_STOP        /*!< LPTIIM1 count
 228:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_RTC_STOP       DBGMCU_APB1_FZ_DBG_RTC_STOP           /*!< RTC counter s
 229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_WWDG_STOP      DBGMCU_APB1_FZ_DBG_WWDG_STOP          /*!< Debug Window 
 230:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_IWDG_STOP      DBGMCU_APB1_FZ_DBG_IWDG_STOP          /*!< Debug Indepen
 231:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_I2C1_STOP      DBGMCU_APB1_FZ_DBG_I2C1_SMBUS_TIMEOUT /*!< I2C1 SMBUS ti
 232:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_I2C2_STOP      DBGMCU_APB1_FZ_DBG_I2C2_SMBUS_TIMEOUT /*!< I2C2 SMBUS ti
 233:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_I2C3_STOP      DBGMCU_APB1_FZ_DBG_I2C3_SMBUS_TIMEOUT /*!< I2C3 SMBUS ti
 234:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(DBGMCU_APB1_FZ_DBG_I2C4_SMBUS_TIMEOUT)
 235:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_I2C4_STOP      DBGMCU_APB1_FZ_DBG_I2C4_SMBUS_TIMEOUT /*!< I2C4 SMBUS ti
 236:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* DBGMCU_APB1_FZ_DBG_I2C4_SMBUS_TIMEOUT */
 237:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_CAN1_STOP       DBGMCU_APB1_FZ_DBG_CAN1_STOP         /*!< CAN1 debug st
 238:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(DBGMCU_APB1_FZ_DBG_CAN2_STOP)
 239:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_CAN2_STOP       DBGMCU_APB1_FZ_DBG_CAN2_STOP         /*!< CAN2 debug st
 240:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* DBGMCU_APB1_FZ_DBG_CAN2_STOP */
 241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(DBGMCU_APB1_FZ_DBG_CAN3_STOP)
 242:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB1_GRP1_CAN3_STOP       DBGMCU_APB1_FZ_DBG_CAN3_STOP         /*!< CAN3 debug st
 243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /*DBGMCU_APB1_FZ_DBG_CAN3_STOP*/
 244:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 245:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 246:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 248:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_APB2_GRP1_STOP_IP DBGMCU APB2 GRP1 STOP IP
 249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 250:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 251:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB2_GRP1_TIM1_STOP      DBGMCU_APB2_FZ_DBG_TIM1_STOP     /*!< TIM1 counter stopp
 252:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB2_GRP1_TIM8_STOP      DBGMCU_APB2_FZ_DBG_TIM8_STOP     /*!< TIM8 counter stopp
 253:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB2_GRP1_TIM9_STOP      DBGMCU_APB2_FZ_DBG_TIM9_STOP     /*!< TIM9 counter stopp
 254:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB2_GRP1_TIM10_STOP     DBGMCU_APB2_FZ_DBG_TIM10_STOP    /*!< TIM10 counter stop
 255:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_DBGMCU_APB2_GRP1_TIM11_STOP     DBGMCU_APB2_FZ_DBG_TIM11_STOP    /*!< TIM11 counter stop
 256:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 257:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 258:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 259:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 260:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EC_LATENCY FLASH LATENCY
 261:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 262:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_0                 FLASH_ACR_LATENCY_0WS   /*!< FLASH Zero wait state */
 264:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_1                 FLASH_ACR_LATENCY_1WS   /*!< FLASH One wait state */
 265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_2                 FLASH_ACR_LATENCY_2WS   /*!< FLASH Two wait states */
 266:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_3                 FLASH_ACR_LATENCY_3WS   /*!< FLASH Three wait states */
 267:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_4                 FLASH_ACR_LATENCY_4WS   /*!< FLASH Four wait states */
 268:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_5                 FLASH_ACR_LATENCY_5WS   /*!< FLASH five wait state */
 269:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_6                 FLASH_ACR_LATENCY_6WS   /*!< FLASH six wait state */
 270:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_7                 FLASH_ACR_LATENCY_7WS   /*!< FLASH seven wait states */
 271:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_8                 FLASH_ACR_LATENCY_8WS   /*!< FLASH eight wait states */
 272:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_9                 FLASH_ACR_LATENCY_9WS   /*!< FLASH nine wait states */
 273:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_10                FLASH_ACR_LATENCY_10WS   /*!< FLASH ten wait states */
 274:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_11                FLASH_ACR_LATENCY_11WS   /*!< FLASH eleven wait states *
 275:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_12                FLASH_ACR_LATENCY_12WS   /*!< FLASH twelve wait states *
ARM GAS  /tmp/ccqw5Uyy.s 			page 113


 276:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_13                FLASH_ACR_LATENCY_13WS   /*!< FLASH thirteen wait states
 277:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_14                FLASH_ACR_LATENCY_14WS   /*!< FLASH fourteen wait states
 278:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #define LL_FLASH_LATENCY_15                FLASH_ACR_LATENCY_15WS   /*!< FLASH fifteen wait states 
 279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 280:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 282:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 283:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 284:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 285:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 286:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 287:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Exported macro ------------------------------------------------------------*/
 288:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 289:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /* Exported functions --------------------------------------------------------*/
 290:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_Exported_Functions SYSTEM Exported Functions
 291:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 292:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 293:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 294:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EF_SYSCFG SYSCFG
 295:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 296:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 297:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 298:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 299:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enables the FMC Memory Mapping Swapping
 300:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_MEMRMP SWP_FMC      LL_SYSCFG_EnableFMCMemorySwapping
 301:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note   SDRAM is accessible at 0x60000000 and NOR/RAM
 302:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         is accessible at 0xC0000000
 303:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 304:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 305:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_EnableFMCMemorySwapping(void)
 306:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 307:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(SYSCFG->MEMRMP, SYSCFG_MEMRMP_SWP_FMC_0);
 308:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 309:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 310:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 311:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disables the FMC Memory Mapping Swapping
 312:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_MEMRMP SWP_FMC      LL_SYSCFG_DisableFMCMemorySwapping
 313:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note   SDRAM is accessible at 0xC0000000 (default mapping)
 314:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         and NOR/RAM is accessible at 0x60000000 (default mapping)
 315:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 316:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 317:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_DisableFMCMemorySwapping(void)
 318:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 319:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(SYSCFG->MEMRMP, SYSCFG_MEMRMP_SWP_FMC);
 320:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 321:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 322:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 323:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enables the Compensation Cell
 324:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_CMPCR CMP_PD      LL_SYSCFG_EnableCompensationCell
 325:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note   The I/O compensation cell can be used only when the device supply
 326:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         voltage ranges from 2.4 to 3.6 V
 327:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 328:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 329:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_EnableCompensationCell(void)
 330:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 331:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(SYSCFG->CMPCR, SYSCFG_CMPCR_CMP_PD);
 332:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
ARM GAS  /tmp/ccqw5Uyy.s 			page 114


 333:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 334:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 335:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disables the Compensation Cell
 336:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_CMPCR CMP_PD      LL_SYSCFG_DisableCompensationCell
 337:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note   The I/O compensation cell can be used only when the device supply
 338:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         voltage ranges from 2.4 to 3.6 V
 339:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 340:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 341:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_DisableCompensationCell(void)
 342:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 343:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(SYSCFG->CMPCR, SYSCFG_CMPCR_CMP_PD);
 344:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 345:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 346:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 347:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get Compensation Cell ready Flag
 348:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_CMPCR READY  LL_SYSCFG_IsActiveFlag_CMPCR
 349:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval State of bit (1 or 0).
 350:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 351:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_IsActiveFlag_CMPCR(void)
 352:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 353:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (READ_BIT(SYSCFG->CMPCR, SYSCFG_CMPCR_READY) == (SYSCFG_CMPCR_READY));
 354:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 355:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 356:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 357:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 358:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get the memory boot mapping as configured by user
 359:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_MEMRMP MEM_BOOT      LL_SYSCFG_GetRemapMemoryBoot
 360:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 361:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *           @arg @ref LL_SYSCFG_REMAP_BOOT0
 362:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *           @arg @ref LL_SYSCFG_REMAP_BOOT1
 363:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 364:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices
 365:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 366:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_GetRemapMemoryBoot(void)
 367:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 368:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(SYSCFG->MEMRMP, SYSCFG_MEMRMP_MEM_BOOT));
 369:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 370:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 371:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_MII_RMII_SEL)
 372:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 373:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Select Ethernet PHY interface
 374:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_PMC MII_RMII_SEL       LL_SYSCFG_SetPHYInterface
 375:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Interface This parameter can be one of the following values:
 376:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_PMC_ETHMII
 377:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_PMC_ETHRMII
 378:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 379:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 380:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_SetPHYInterface(uint32_t Interface)
 381:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 382:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(SYSCFG->PMC, SYSCFG_PMC_MII_RMII_SEL, Interface);
 383:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 384:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 385:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 386:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get Ethernet PHY interface
 387:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_PMC MII_RMII_SEL       LL_SYSCFG_GetPHYInterface
 388:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 389:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_PMC_ETHMII
ARM GAS  /tmp/ccqw5Uyy.s 			page 115


 390:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_PMC_ETHRMII
 391:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 392:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 393:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_GetPHYInterface(void)
 394:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 395:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(SYSCFG->PMC, SYSCFG_PMC_MII_RMII_SEL));
 396:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 397:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_MII_RMII_SEL */
 398:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 399:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 400:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_MEMRMP_SWP_FB)
 401:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 402:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Select Flash bank mode (Bank flashed at 0x08000000)
 403:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_MEMRMP FB_MODE       LL_SYSCFG_SetFlashBankMode
 404:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Bank This parameter can be one of the following values:
 405:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_BANKMODE_BANK1
 406:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_BANKMODE_BANK2
 407:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 408:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 409:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_SetFlashBankMode(uint32_t Bank)
 410:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 411:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(SYSCFG->MEMRMP, SYSCFG_MEMRMP_SWP_FB, Bank);
 412:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 413:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 414:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 415:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get Flash bank mode (Bank flashed at 0x08000000)
 416:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_MEMRMP FB_MODE       LL_SYSCFG_GetFlashBankMode
 417:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 418:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_BANKMODE_BANK1
 419:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_BANKMODE_BANK2
 420:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 421:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_GetFlashBankMode(void)
 422:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 423:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(SYSCFG->MEMRMP, SYSCFG_MEMRMP_SWP_FB));
 424:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 425:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 426:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_MEMRMP_SWP_FB */
 427:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 428:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_PMC_I2C1_FMP)
 429:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 430:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enable the I2C fast mode plus driving capability.
 431:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_PMC I2C_PBx_FMP   LL_SYSCFG_EnableFastModePlus\n
 432:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_PMC I2Cx_FMP      LL_SYSCFG_EnableFastModePlus
 433:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  ConfigFastModePlus This parameter can be a combination of the following values:
 434:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB6
 435:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB7
 436:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB8 (*)
 437:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB9 (*)
 438:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C1
 439:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C2 (*)
 440:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C3
 441:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C4(*)
 442:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 443:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices
 444:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 445:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 446:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_EnableFastModePlus(uint32_t ConfigFastModePlus)
ARM GAS  /tmp/ccqw5Uyy.s 			page 116


 447:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 448:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(SYSCFG->PMC, ConfigFastModePlus);
 449:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 450:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 451:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 452:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disable the I2C fast mode plus driving capability.
 453:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_PMC I2C_PBx_FMP   LL_SYSCFG_DisableFastModePlus\n
 454:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_PMC I2Cx_FMP      LL_SYSCFG_DisableFastModePlus
 455:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  ConfigFastModePlus This parameter can be a combination of the following values:
 456:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB6
 457:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB7
 458:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB8 (*)
 459:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_PB9 (*)
 460:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C1
 461:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C2 (*)
 462:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C3
 463:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_I2C_FASTMODEPLUS_I2C4
 464:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices
 465:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 466:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 467:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_DisableFastModePlus(uint32_t ConfigFastModePlus)
 468:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 469:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(SYSCFG->PMC, ConfigFastModePlus);
 470:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 471:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_PMC_I2C1_FMP */
 472:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 473:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 474:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 475:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Configure source input for the EXTI external interrupt.
 476:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_EXTICR1 EXTIx         LL_SYSCFG_SetEXTISource\n
 477:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR2 EXTIx         LL_SYSCFG_SetEXTISource\n
 478:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR3 EXTIx         LL_SYSCFG_SetEXTISource\n
 479:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR4 EXTIx         LL_SYSCFG_SetEXTISource
 480:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Port This parameter can be one of the following values:
 481:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTA
 482:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTB
 483:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTC
 484:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTD
 485:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTE
 486:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTF
 487:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTG
 488:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTH
 489:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTI
 490:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTJ
 491:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTK
 492:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 493:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices
 494:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Line This parameter can be one of the following values:
 495:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE0
 496:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE1
 497:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE2
 498:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE3
 499:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE4
 500:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE5
 501:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE6
 502:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE7
 503:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE8
ARM GAS  /tmp/ccqw5Uyy.s 			page 117


 504:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE9
 505:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE10
 506:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE11
 507:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE12
 508:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE13
 509:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE14
 510:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE15
 511:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 512:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 513:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_SetEXTISource(uint32_t Port, uint32_t Line)
 514:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 515:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(SYSCFG->EXTICR[Line & 0xFFU], (Line >> 16U), Port << POSITION_VAL((Line >> 16U)));
 516:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 517:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 518:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 519:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get the configured defined for specific EXTI Line
 520:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll SYSCFG_EXTICR1 EXTIx         LL_SYSCFG_GetEXTISource\n
 521:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR2 EXTIx         LL_SYSCFG_GetEXTISource\n
 522:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR3 EXTIx         LL_SYSCFG_GetEXTISource\n
 523:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_EXTICR4 EXTIx         LL_SYSCFG_GetEXTISource
 524:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Line This parameter can be one of the following values:
 525:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE0
 526:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE1
 527:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE2
 528:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE3
 529:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE4
 530:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE5
 531:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE6
 532:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE7
 533:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE8
 534:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE9
 535:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE10
 536:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE11
 537:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE12
 538:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE13
 539:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE14
 540:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_LINE15
 541:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 542:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTA
 543:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTB
 544:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTC
 545:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTD
 546:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTE
 547:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTF
 548:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTG
 549:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTH
 550:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTI
 551:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTJ
 552:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_EXTI_PORTK
 553:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices
 554:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 555:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_GetEXTISource(uint32_t Line)
 556:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 557:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(SYSCFG->EXTICR[Line & 0xFFU], (Line >> 16U)) >> POSITION_VAL(Line >> 1
 558:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 559:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 560:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #if defined(SYSCFG_CBR_CLL)
ARM GAS  /tmp/ccqw5Uyy.s 			page 118


 561:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 562:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Set connections to TIM1/8/15/16/17 Break inputs
 563:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_CBR CLL             LL_SYSCFG_SetTIMBreakInputs\n
 564:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_CBR PVDL            LL_SYSCFG_SetTIMBreakInputs
 565:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Break This parameter can be a combination of the following values:
 566:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_TIMBREAK_LOCKUP
 567:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_TIMBREAK_PVD
 568:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 569:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 570:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_SYSCFG_SetTIMBreakInputs(uint32_t Break)
 571:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 572:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(SYSCFG->CBR, SYSCFG_CBR_CLL | SYSCFG_CBR_PVDL, Break);
 573:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 574:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 575:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 576:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get connections to TIM1/8/15/16/17 Break inputs
 577:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_CBR CLL             LL_SYSCFG_GetTIMBreakInputs\n
 578:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         SYSCFG_CBR PVDL            LL_SYSCFG_GetTIMBreakInputs
 579:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be can be a combination of the following values:
 580:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_TIMBREAK_LOCKUP
 581:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_SYSCFG_TIMBREAK_PVD
 582:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 583:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_SYSCFG_GetTIMBreakInputs(void)
 584:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 585:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(SYSCFG->CBR, SYSCFG_CBR_CLL | SYSCFG_CBR_PVDL));
 586:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 587:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** #endif /* SYSCFG_CBR_CLL */
 588:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 589:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 590:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 591:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 592:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 593:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EF_DBGMCU DBGMCU
 594:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 595:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 596:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 597:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 598:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Return the device identifier
 599:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note For STM32F75xxx and STM32F74xxx devices, the device ID is 0x449
 600:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note For STM32F77xxx and STM32F76xxx devices, the device ID is 0x451
 601:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note For STM32F72xxx and STM32F73xxx devices, the device ID is 0x452
 602:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_IDCODE DEV_ID        LL_DBGMCU_GetDeviceID
 603:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Values between Min_Data=0x00 and Max_Data=0xFFF
 604:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 605:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_DBGMCU_GetDeviceID(void)
 606:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 607:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(DBGMCU->IDCODE, DBGMCU_IDCODE_DEV_ID));
 608:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 609:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 610:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 611:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Return the device revision identifier
 612:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @note This field indicates the revision of the device.
 613:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****           For example, it is read as RevA -> 0x1000, Cat 2 revZ -> 0x1001
 614:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_IDCODE REV_ID        LL_DBGMCU_GetRevisionID
 615:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Values between Min_Data=0x00 and Max_Data=0xFFFF
 616:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 617:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_DBGMCU_GetRevisionID(void)
ARM GAS  /tmp/ccqw5Uyy.s 			page 119


 618:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 619:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(DBGMCU->IDCODE, DBGMCU_IDCODE_REV_ID) >> DBGMCU_IDCODE_REV_ID_Pos);
 620:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 621:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 622:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 623:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enable the Debug Module during SLEEP mode
 624:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_SLEEP     LL_DBGMCU_EnableDBGSleepMode
 625:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 626:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 627:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_EnableDBGSleepMode(void)
 628:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 629:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(DBGMCU->CR, DBGMCU_CR_DBG_SLEEP);
 630:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 631:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 632:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 633:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disable the Debug Module during SLEEP mode
 634:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_SLEEP     LL_DBGMCU_DisableDBGSleepMode
 635:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 636:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 637:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_DisableDBGSleepMode(void)
 638:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 639:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(DBGMCU->CR, DBGMCU_CR_DBG_SLEEP);
 640:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 641:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 642:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 643:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enable the Debug Module during STOP mode
 644:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_STOP      LL_DBGMCU_EnableDBGStopMode
 645:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 646:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 647:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_EnableDBGStopMode(void)
 648:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 649:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(DBGMCU->CR, DBGMCU_CR_DBG_STOP);
 650:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 651:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 652:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 653:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disable the Debug Module during STOP mode
 654:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_STOP      LL_DBGMCU_DisableDBGStopMode
 655:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 656:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 657:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_DisableDBGStopMode(void)
 658:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 659:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(DBGMCU->CR, DBGMCU_CR_DBG_STOP);
 660:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 661:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 662:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 663:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Enable the Debug Module during STANDBY mode
 664:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_STANDBY   LL_DBGMCU_EnableDBGStandbyMode
 665:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 666:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 667:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_EnableDBGStandbyMode(void)
 668:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 669:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(DBGMCU->CR, DBGMCU_CR_DBG_STANDBY);
 670:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 671:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 672:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 673:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Disable the Debug Module during STANDBY mode
 674:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    DBG_STANDBY   LL_DBGMCU_DisableDBGStandbyMode
ARM GAS  /tmp/ccqw5Uyy.s 			page 120


 675:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 676:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 677:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_DisableDBGStandbyMode(void)
 678:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 679:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(DBGMCU->CR, DBGMCU_CR_DBG_STANDBY);
 680:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 681:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 682:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 683:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Set Trace pin assignment control
 684:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    TRACE_IOEN    LL_DBGMCU_SetTracePinAssignment\n
 685:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_CR    TRACE_MODE    LL_DBGMCU_SetTracePinAssignment
 686:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  PinAssignment This parameter can be one of the following values:
 687:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_NONE
 688:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_ASYNCH
 689:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE1
 690:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE2
 691:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE4
 692:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 693:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 694:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_SetTracePinAssignment(uint32_t PinAssignment)
 695:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 696:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(DBGMCU->CR, DBGMCU_CR_TRACE_IOEN | DBGMCU_CR_TRACE_MODE, PinAssignment);
 697:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 698:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 699:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 700:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get Trace pin assignment control
 701:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_CR    TRACE_IOEN    LL_DBGMCU_GetTracePinAssignment\n
 702:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_CR    TRACE_MODE    LL_DBGMCU_GetTracePinAssignment
 703:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 704:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_NONE
 705:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_ASYNCH
 706:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE1
 707:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE2
 708:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_TRACE_SYNCH_SIZE4
 709:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 710:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_DBGMCU_GetTracePinAssignment(void)
 711:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 712:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(DBGMCU->CR, DBGMCU_CR_TRACE_IOEN | DBGMCU_CR_TRACE_MODE));
 713:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 714:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 715:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 716:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Freeze APB1 peripherals (group1 peripherals)
 717:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_APB1_FZ      DBG_TIM2_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 718:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM3_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 719:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM4_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 720:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM5_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 721:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM6_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 722:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM7_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 723:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM12_STOP          LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 724:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM13_STOP          LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 725:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM14_STOP          LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 726:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_LPTIM1_STOP         LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 727:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_RTC_STOP            LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 728:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_WWDG_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 729:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_IWDG_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 730:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C1_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 731:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C2_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_FreezePeriph\n
ARM GAS  /tmp/ccqw5Uyy.s 			page 121


 732:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C3_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 733:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C4_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 734:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN1_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 735:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN2_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph\n
 736:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN3_STOP           LL_DBGMCU_APB1_GRP1_FreezePeriph
 737:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Periphs This parameter can be a combination of the following values:
 738:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM2_STOP
 739:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM3_STOP
 740:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM4_STOP
 741:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM5_STOP
 742:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM6_STOP
 743:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM7_STOP
 744:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM12_STOP
 745:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM13_STOP
 746:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM14_STOP
 747:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_LPTIM1_STOP
 748:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_RTC_STOP
 749:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_WWDG_STOP
 750:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_IWDG_STOP
 751:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C1_STOP
 752:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C2_STOP
 753:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C3_STOP
 754:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C4_STOP (*)
 755:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN1_STOP
 756:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN2_STOP (*)
 757:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN3_STOP (*)
 758:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 759:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices.
 760:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 761:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 762:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_APB1_GRP1_FreezePeriph(uint32_t Periphs)
 763:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 764:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(DBGMCU->APB1FZ, Periphs);
 765:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 766:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 767:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 768:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Unfreeze APB1 peripherals (group1 peripherals)
 769:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_APB1_FZ      DBG_TIM2_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 770:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM3_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 771:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM4_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 772:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM5_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 773:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM6_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 774:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM7_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 775:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM12_STOP          LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 776:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM13_STOP          LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 777:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_TIM14_STOP          LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 778:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_LPTIM1_STOP         LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 779:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_RTC_STOP            LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 780:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_WWDG_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 781:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_IWDG_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 782:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C1_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 783:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C2_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 784:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C3_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 785:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_I2C4_SMBUS_TIMEOUT  LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 786:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN1_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 787:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN2_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph\n
 788:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB1_FZ      DBG_CAN3_STOP           LL_DBGMCU_APB1_GRP1_UnFreezePeriph
ARM GAS  /tmp/ccqw5Uyy.s 			page 122


 789:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Periphs This parameter can be a combination of the following values:
 790:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM2_STOP
 791:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM3_STOP
 792:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM4_STOP
 793:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM5_STOP
 794:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM6_STOP
 795:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM7_STOP
 796:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM12_STOP
 797:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM13_STOP
 798:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_TIM14_STOP
 799:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_LPTIM1_STOP
 800:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_RTC_STOP
 801:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_WWDG_STOP
 802:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_IWDG_STOP
 803:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C1_STOP
 804:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C2_STOP
 805:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C3_STOP
 806:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_I2C4_STOP (*)
 807:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN1_STOP
 808:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN2_STOP (*)
 809:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB1_GRP1_CAN3_STOP (*)
 810:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices.
 811:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 812:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 813:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_APB1_GRP1_UnFreezePeriph(uint32_t Periphs)
 814:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 815:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(DBGMCU->APB1FZ, Periphs);
 816:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 817:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 818:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 819:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Freeze APB2 peripherals
 820:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_APB2_FZ      DBG_TIM1_STOP    LL_DBGMCU_APB2_GRP1_FreezePeriph\n
 821:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM8_STOP    LL_DBGMCU_APB2_GRP1_FreezePeriph\n
 822:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM9_STOP    LL_DBGMCU_APB2_GRP1_FreezePeriph\n
 823:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM10_STOP   LL_DBGMCU_APB2_GRP1_FreezePeriph\n
 824:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM11_STOP   LL_DBGMCU_APB2_GRP1_FreezePeriph
 825:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Periphs This parameter can be a combination of the following values:
 826:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM1_STOP
 827:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM8_STOP
 828:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM9_STOP
 829:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM10_STOP
 830:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM11_STOP
 831:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 832:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices.
 833:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 834:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 835:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_APB2_GRP1_FreezePeriph(uint32_t Periphs)
 836:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 837:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   SET_BIT(DBGMCU->APB2FZ, Periphs);
 838:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 839:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 840:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 841:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Unfreeze APB2 peripherals
 842:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll DBGMCU_APB2_FZ      DBG_TIM1_STOP    LL_DBGMCU_APB2_GRP1_UnFreezePeriph\n
 843:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM8_STOP    LL_DBGMCU_APB2_GRP1_UnFreezePeriph\n
 844:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM9_STOP    LL_DBGMCU_APB2_GRP1_UnFreezePeriph\n
 845:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM10_STOP   LL_DBGMCU_APB2_GRP1_UnFreezePeriph\n
ARM GAS  /tmp/ccqw5Uyy.s 			page 123


 846:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         DBGMCU_APB2_FZ      DBG_TIM11_STOP   LL_DBGMCU_APB2_GRP1_UnFreezePeriph
 847:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Periphs This parameter can be a combination of the following values:
 848:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM1_STOP
 849:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM8_STOP
 850:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM9_STOP
 851:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM10_STOP
 852:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_DBGMCU_APB2_GRP1_TIM11_STOP
 853:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *
 854:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         (*) value not defined in all devices.
 855:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 856:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 857:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_DBGMCU_APB2_GRP1_UnFreezePeriph(uint32_t Periphs)
 858:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 859:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   CLEAR_BIT(DBGMCU->APB2FZ, Periphs);
 860:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 861:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 862:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @}
 863:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 864:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 865:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /** @defgroup SYSTEM_LL_EF_FLASH FLASH
 866:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @{
 867:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 868:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 869:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 870:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Set FLASH Latency
 871:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll FLASH_ACR    LATENCY       LL_FLASH_SetLatency
 872:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @param  Latency This parameter can be one of the following values:
 873:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_0
 874:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_1
 875:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_2
 876:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_3
 877:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_4
 878:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_5
 879:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_6
 880:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_7
 881:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_8
 882:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_9
 883:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_10
 884:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_11
 885:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_12
 886:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_13
 887:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_14
 888:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_15
 889:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval None
 890:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 891:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE void LL_FLASH_SetLatency(uint32_t Latency)
 580              		.loc 5 891 22 view .LVU173
 581              	.LBB69:
 892:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 893:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   MODIFY_REG(FLASH->ACR, FLASH_ACR_LATENCY, Latency);
 582              		.loc 5 893 3 view .LVU174
 583 00f8 184A     		ldr	r2, .L56+28
 584              	.LVL45:
 585              		.loc 5 893 3 is_stmt 0 view .LVU175
 586 00fa 1368     		ldr	r3, [r2]
 587 00fc 23F00F03 		bic	r3, r3, #15
 588 0100 0343     		orrs	r3, r3, r0
ARM GAS  /tmp/ccqw5Uyy.s 			page 124


 589 0102 1360     		str	r3, [r2]
 590              	.LVL46:
 591              		.loc 5 893 3 view .LVU176
 592              	.LBE69:
 593              	.LBE68:
 451:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       do
 594              		.loc 1 451 7 is_stmt 1 view .LVU177
 451:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       do
 595              		.loc 1 451 15 is_stmt 0 view .LVU178
 596 0104 0222     		movs	r2, #2
 597              	.LVL47:
 598              	.L30:
 452:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 599              		.loc 1 452 7 is_stmt 1 view .LVU179
 455:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       timeout--;
 600              		.loc 1 455 7 view .LVU180
 601              	.LBB70:
 602              	.LBI70:
 894:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** }
 895:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** 
 896:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** /**
 897:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @brief  Get FLASH Latency
 898:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @rmtoll FLASH_ACR    LATENCY       LL_FLASH_GetLatency
 899:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   * @retval Returned value can be one of the following values:
 900:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_0
 901:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_1
 902:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_2
 903:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_3
 904:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_4
 905:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_5
 906:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_6
 907:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_7
 908:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_8
 909:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_9
 910:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_10
 911:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_11
 912:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_12
 913:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_13
 914:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_14
 915:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   *         @arg @ref LL_FLASH_LATENCY_15
 916:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   */
 917:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** __STATIC_INLINE uint32_t LL_FLASH_GetLatency(void)
 603              		.loc 5 917 26 view .LVU181
 604              	.LBB71:
 918:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h **** {
 919:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_system.h ****   return (uint32_t)(READ_BIT(FLASH->ACR, FLASH_ACR_LATENCY));
 605              		.loc 5 919 3 view .LVU182
 606              		.loc 5 919 21 is_stmt 0 view .LVU183
 607 0106 154B     		ldr	r3, .L56+28
 608 0108 1B68     		ldr	r3, [r3]
 609              		.loc 5 919 10 view .LVU184
 610 010a 03F00F03 		and	r3, r3, #15
 611              	.LVL48:
 612              		.loc 5 919 10 view .LVU185
 613              	.LBE71:
 614              	.LBE70:
 456:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       } while ((getlatency != latency) && (timeout > 0));
ARM GAS  /tmp/ccqw5Uyy.s 			page 125


 615              		.loc 1 456 7 is_stmt 1 view .LVU186
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 616              		.loc 1 457 40 discriminator 1 view .LVU187
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 617              		.loc 1 457 52 is_stmt 0 discriminator 1 view .LVU188
 618 010e 013A     		subs	r2, r2, #1
 619              	.LVL49:
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 620              		.loc 1 457 52 discriminator 1 view .LVU189
 621 0110 14BF     		ite	ne
 622 0112 0121     		movne	r1, #1
 623 0114 0021     		moveq	r1, #0
 457:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 624              		.loc 1 457 40 discriminator 1 view .LVU190
 625 0116 9842     		cmp	r0, r3
 626 0118 01D0     		beq	.L49
 627 011a 0029     		cmp	r1, #0
 628 011c F3D1     		bne	.L30
 629              	.L49:
 459:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 630              		.loc 1 459 7 is_stmt 1 view .LVU191
 459:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 631              		.loc 1 459 9 is_stmt 0 view .LVU192
 632 011e 9842     		cmp	r0, r3
 633 0120 0BD0     		beq	.L48
 461:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 634              		.loc 1 461 16 view .LVU193
 635 0122 0120     		movs	r0, #1
 636              	.LVL50:
 637              	.L25:
 469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 638              		.loc 1 469 3 is_stmt 1 view .LVU194
 470:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 639              		.loc 1 470 1 is_stmt 0 view .LVU195
 640 0124 5DF8044B 		ldr	r4, [sp], #4
 641              	.LCFI3:
 642              		.cfi_remember_state
 643              		.cfi_restore 4
 644              		.cfi_def_cfa_offset 0
 645 0128 7047     		bx	lr
 646              	.LVL51:
 647              	.L45:
 648              	.LCFI4:
 649              		.cfi_restore_state
 427:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 650              		.loc 1 427 17 view .LVU196
 651 012a 0320     		movs	r0, #3
 652              	.LVL52:
 427:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 653              		.loc 1 427 17 view .LVU197
 654 012c E4E7     		b	.L28
 655              	.LVL53:
 656              	.L46:
 432:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 657              		.loc 1 432 17 view .LVU198
 658 012e 0220     		movs	r0, #2
 659              	.LVL54:
ARM GAS  /tmp/ccqw5Uyy.s 			page 126


 432:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 660              		.loc 1 432 17 view .LVU199
 661 0130 E2E7     		b	.L28
 662              	.LVL55:
 663              	.L47:
 439:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 664              		.loc 1 439 19 view .LVU200
 665 0132 0120     		movs	r0, #1
 666              	.LVL56:
 439:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****         }
 667              		.loc 1 439 19 view .LVU201
 668 0134 E0E7     		b	.L28
 669              	.LVL57:
 670              	.L32:
 671              	.LCFI5:
 672              		.cfi_def_cfa_offset 0
 673              		.cfi_restore 4
 336:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 674              		.loc 1 336 12 view .LVU202
 675 0136 0120     		movs	r0, #1
 676              	.LVL58:
 469:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 677              		.loc 1 469 3 is_stmt 1 view .LVU203
 470:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 678              		.loc 1 470 1 is_stmt 0 view .LVU204
 679 0138 7047     		bx	lr
 680              	.LVL59:
 681              	.L48:
 682              	.LCFI6:
 683              		.cfi_def_cfa_offset 4
 684              		.cfi_offset 4, -4
 465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 685              		.loc 1 465 16 view .LVU205
 686 013a 0020     		movs	r0, #0
 687              	.LVL60:
 465:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 688              		.loc 1 465 16 view .LVU206
 689 013c F2E7     		b	.L25
 690              	.L57:
 691 013e 00BF     		.align	2
 692              	.L56:
 693 0140 00700040 		.word	1073770496
 694 0144 000E2707 		.word	120000000
 695 0148 804A5D05 		.word	90000000
 696 014c 00879303 		.word	60000000
 697 0150 80C3C901 		.word	30000000
 698 0154 8058840C 		.word	210000000
 699 0158 80D1F008 		.word	150000000
 700 015c 003C0240 		.word	1073888256
 701              		.cfi_endproc
 702              	.LFE408:
 704              		.section	.text.UTILS_EnablePLLAndSwitchSystem,"ax",%progbits
 705              		.align	1
 706              		.syntax unified
 707              		.thumb
 708              		.thumb_func
 710              	UTILS_EnablePLLAndSwitchSystem:
ARM GAS  /tmp/ccqw5Uyy.s 			page 127


 711              	.LVL61:
 712              	.LFB413:
 673:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 674:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** /**
 675:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @brief  Function to enable PLL and switch system clock to PLL
 676:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  SYSCLK_Frequency SYSCLK frequency
 677:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @param  UTILS_ClkInitStruct pointer to a @ref LL_UTILS_ClkInitTypeDef structure that contains
 678:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *                             the configuration information for the BUS prescalers.
 679:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   * @retval An ErrorStatus enumeration value:
 680:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - SUCCESS: No problem to switch system to PLL
 681:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   *          - ERROR: Problem to switch system to PLL
 682:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   */
 683:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** static ErrorStatus UTILS_EnablePLLAndSwitchSystem(uint32_t SYSCLK_Frequency, LL_UTILS_ClkInitTypeDe
 684:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** {
 713              		.loc 1 684 1 is_stmt 1 view -0
 714              		.cfi_startproc
 715              		@ args = 0, pretend = 0, frame = 0
 716              		@ frame_needed = 0, uses_anonymous_args = 0
 717              		.loc 1 684 1 is_stmt 0 view .LVU208
 718 0000 70B5     		push	{r4, r5, r6, lr}
 719              	.LCFI7:
 720              		.cfi_def_cfa_offset 16
 721              		.cfi_offset 4, -16
 722              		.cfi_offset 5, -12
 723              		.cfi_offset 6, -8
 724              		.cfi_offset 14, -4
 725 0002 0C46     		mov	r4, r1
 685:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 726              		.loc 1 685 3 is_stmt 1 view .LVU209
 727              	.LVL62:
 686:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t hclk_frequency = 0U;
 728              		.loc 1 686 3 view .LVU210
 687:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 688:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_SYSCLK_DIV(UTILS_ClkInitStruct->AHBCLKDivider));
 729              		.loc 1 688 3 view .LVU211
 689:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_APB1_DIV(UTILS_ClkInitStruct->APB1CLKDivider));
 730              		.loc 1 689 3 view .LVU212
 690:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_APB2_DIV(UTILS_ClkInitStruct->APB2CLKDivider));
 731              		.loc 1 690 3 view .LVU213
 691:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 692:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Calculate HCLK frequency */
 693:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   hclk_frequency = __LL_RCC_CALC_HCLK_FREQ(SYSCLK_Frequency, UTILS_ClkInitStruct->AHBCLKDivider);
 732              		.loc 1 693 3 view .LVU214
 733              		.loc 1 693 20 is_stmt 0 view .LVU215
 734 0004 0B68     		ldr	r3, [r1]
 735 0006 C3F30313 		ubfx	r3, r3, #4, #4
 736 000a 254A     		ldr	r2, .L70
 737 000c D35C     		ldrb	r3, [r2, r3]	@ zero_extendqisi2
 738              		.loc 1 693 18 view .LVU216
 739 000e 20FA03F5 		lsr	r5, r0, r3
 740              	.LVL63:
 694:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 695:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Increasing the number of wait states because of higher CPU frequency */
 696:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(SystemCoreClock < hclk_frequency)
 741              		.loc 1 696 3 is_stmt 1 view .LVU217
 742              		.loc 1 696 22 is_stmt 0 view .LVU218
 743 0012 244B     		ldr	r3, .L70+4
ARM GAS  /tmp/ccqw5Uyy.s 			page 128


 744 0014 1B68     		ldr	r3, [r3]
 745              		.loc 1 696 5 view .LVU219
 746 0016 AB42     		cmp	r3, r5
 747 0018 31D3     		bcc	.L67
 685:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t hclk_frequency = 0U;
 748              		.loc 1 685 15 view .LVU220
 749 001a 0026     		movs	r6, #0
 750              	.LVL64:
 751              	.L59:
 697:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 698:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Set FLASH latency to highest latency */
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = LL_SetFlashLatency(hclk_frequency);
 700:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 701:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 702:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Update system clock configuration */
 703:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(status == SUCCESS)
 704:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 705:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Enable PLL */
 706:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_PLL_Enable();
 752              		.loc 1 706 5 is_stmt 1 view .LVU221
 753              	.LBB72:
 754              	.LBI72:
3132:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 755              		.loc 2 3132 22 view .LVU222
 756              	.LBB73:
3134:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 757              		.loc 2 3134 3 view .LVU223
 758 001c 224A     		ldr	r2, .L70+8
 759 001e 1368     		ldr	r3, [r2]
 760 0020 43F08073 		orr	r3, r3, #16777216
 761 0024 1360     		str	r3, [r2]
 762              	.LBE73:
 763              	.LBE72:
 707:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     while (LL_RCC_PLL_IsReady() != 1U)
 764              		.loc 1 707 5 view .LVU224
 765              	.L61:
 708:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 709:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Wait for PLL ready */
 710:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 766              		.loc 1 710 5 view .LVU225
 707:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     while (LL_RCC_PLL_IsReady() != 1U)
 767              		.loc 1 707 33 discriminator 1 view .LVU226
 768              	.LBB74:
 769              	.LBI74:
3153:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 770              		.loc 2 3153 26 view .LVU227
 771              	.LBB75:
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 772              		.loc 2 3155 3 view .LVU228
3155:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 773              		.loc 2 3155 11 is_stmt 0 view .LVU229
 774 0026 204B     		ldr	r3, .L70+8
 775 0028 1B68     		ldr	r3, [r3]
 776              	.LBE75:
 777              	.LBE74:
 707:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 778              		.loc 1 707 33 discriminator 1 view .LVU230
ARM GAS  /tmp/ccqw5Uyy.s 			page 129


 779 002a 13F0007F 		tst	r3, #33554432
 780 002e FAD0     		beq	.L61
 711:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 712:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Sysclk activation on the main PLL */
 713:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_SetAHBPrescaler(UTILS_ClkInitStruct->AHBCLKDivider);
 781              		.loc 1 713 5 is_stmt 1 view .LVU231
 782 0030 2368     		ldr	r3, [r4]
 783              	.LVL65:
 784              	.LBB76:
 785              	.LBI76:
2247:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 786              		.loc 2 2247 22 view .LVU232
 787              	.LBB77:
2249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 788              		.loc 2 2249 3 view .LVU233
 789 0032 1D4A     		ldr	r2, .L70+8
 790 0034 9168     		ldr	r1, [r2, #8]
 791 0036 21F0F001 		bic	r1, r1, #240
 792 003a 0B43     		orrs	r3, r3, r1
 793              	.LVL66:
2249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 794              		.loc 2 2249 3 is_stmt 0 view .LVU234
 795 003c 9360     		str	r3, [r2, #8]
 796              	.LVL67:
2249:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 797              		.loc 2 2249 3 view .LVU235
 798              	.LBE77:
 799              	.LBE76:
 714:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_SetSysClkSource(LL_RCC_SYS_CLKSOURCE_PLL);
 800              		.loc 1 714 5 is_stmt 1 view .LVU236
 801              	.LBB78:
 802              	.LBI78:
2214:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 803              		.loc 2 2214 22 view .LVU237
 804              	.LBB79:
2216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 805              		.loc 2 2216 3 view .LVU238
 806 003e 9368     		ldr	r3, [r2, #8]
 807 0040 23F00303 		bic	r3, r3, #3
 808 0044 43F00203 		orr	r3, r3, #2
 809 0048 9360     		str	r3, [r2, #8]
 810              	.LVL68:
2216:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 811              		.loc 2 2216 3 is_stmt 0 view .LVU239
 812              	.LBE79:
 813              	.LBE78:
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     while (LL_RCC_GetSysClkSource() != LL_RCC_SYS_CLKSOURCE_STATUS_PLL)
 814              		.loc 1 715 5 is_stmt 1 view .LVU240
 815              	.L62:
 716:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 717:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       /* Wait for system clock switch to PLL */
 718:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 816              		.loc 1 718 5 view .LVU241
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     while (LL_RCC_GetSysClkSource() != LL_RCC_SYS_CLKSOURCE_STATUS_PLL)
 817              		.loc 1 715 37 discriminator 1 view .LVU242
 818              	.LBB80:
 819              	.LBI80:
ARM GAS  /tmp/ccqw5Uyy.s 			page 130


2227:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 820              		.loc 2 2227 26 view .LVU243
 821              	.LBB81:
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 822              		.loc 2 2229 3 view .LVU244
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 823              		.loc 2 2229 21 is_stmt 0 view .LVU245
 824 004a 174B     		ldr	r3, .L70+8
 825 004c 9B68     		ldr	r3, [r3, #8]
2229:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 826              		.loc 2 2229 10 view .LVU246
 827 004e 03F00C03 		and	r3, r3, #12
 828              	.LBE81:
 829              	.LBE80:
 715:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 830              		.loc 1 715 37 discriminator 1 view .LVU247
 831 0052 082B     		cmp	r3, #8
 832 0054 F9D1     		bne	.L62
 719:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 720:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Set APB1 & APB2 prescaler*/
 721:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_SetAPB1Prescaler(UTILS_ClkInitStruct->APB1CLKDivider);
 833              		.loc 1 721 5 is_stmt 1 view .LVU248
 834 0056 6268     		ldr	r2, [r4, #4]
 835              	.LVL69:
 836              	.LBB82:
 837              	.LBI82:
2263:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 838              		.loc 2 2263 22 view .LVU249
 839              	.LBB83:
2265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 840              		.loc 2 2265 3 view .LVU250
 841 0058 134B     		ldr	r3, .L70+8
 842 005a 9968     		ldr	r1, [r3, #8]
 843 005c 21F4E051 		bic	r1, r1, #7168
 844 0060 0A43     		orrs	r2, r2, r1
 845              	.LVL70:
2265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 846              		.loc 2 2265 3 is_stmt 0 view .LVU251
 847 0062 9A60     		str	r2, [r3, #8]
 848              	.LVL71:
2265:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 849              		.loc 2 2265 3 view .LVU252
 850              	.LBE83:
 851              	.LBE82:
 722:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_RCC_SetAPB2Prescaler(UTILS_ClkInitStruct->APB2CLKDivider);
 852              		.loc 1 722 5 is_stmt 1 view .LVU253
 853 0064 A268     		ldr	r2, [r4, #8]
 854              	.LVL72:
 855              	.LBB84:
 856              	.LBI84:
2279:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 857              		.loc 2 2279 22 view .LVU254
 858              	.LBB85:
2281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 859              		.loc 2 2281 3 view .LVU255
 860 0066 9968     		ldr	r1, [r3, #8]
 861 0068 21F46041 		bic	r1, r1, #57344
ARM GAS  /tmp/ccqw5Uyy.s 			page 131


 862 006c 0A43     		orrs	r2, r2, r1
 863              	.LVL73:
2281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 864              		.loc 2 2281 3 is_stmt 0 view .LVU256
 865 006e 9A60     		str	r2, [r3, #8]
 866              	.LVL74:
 867              	.L60:
2281:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 868              		.loc 2 2281 3 view .LVU257
 869              	.LBE85:
 870              	.LBE84:
 723:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 724:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     
 725:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Decreasing the number of wait states because of lower CPU frequency */
 726:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(SystemCoreClock > hclk_frequency)
 871              		.loc 1 726 3 is_stmt 1 view .LVU258
 872              		.loc 1 726 22 is_stmt 0 view .LVU259
 873 0070 0C4B     		ldr	r3, .L70+4
 874 0072 1B68     		ldr	r3, [r3]
 875              		.loc 1 726 5 view .LVU260
 876 0074 AB42     		cmp	r3, r5
 877 0076 09D8     		bhi	.L68
 878              	.L63:
 879              	.LVL75:
 727:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 728:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     /* Set FLASH latency to lowest latency */
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     status = LL_SetFlashLatency(hclk_frequency);
 730:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 731:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 732:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   /* Update SystemCoreClock variable */
 733:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   if(status == SUCCESS)
 880              		.loc 1 733 3 is_stmt 1 view .LVU261
 881              		.loc 1 733 5 is_stmt 0 view .LVU262
 882 0078 6EB1     		cbz	r6, .L69
 883              	.L64:
 734:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 735:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     LL_SetSystemCoreClock(hclk_frequency);
 736:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 737:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 738:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   return status;
 884              		.loc 1 738 3 is_stmt 1 view .LVU263
 739:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 885              		.loc 1 739 1 is_stmt 0 view .LVU264
 886 007a 3046     		mov	r0, r6
 887 007c 70BD     		pop	{r4, r5, r6, pc}
 888              	.LVL76:
 889              	.L67:
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 890              		.loc 1 699 5 is_stmt 1 view .LVU265
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 891              		.loc 1 699 14 is_stmt 0 view .LVU266
 892 007e 2846     		mov	r0, r5
 893              	.LVL77:
 699:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 894              		.loc 1 699 14 view .LVU267
 895 0080 FFF7FEFF 		bl	LL_SetFlashLatency
 896              	.LVL78:
ARM GAS  /tmp/ccqw5Uyy.s 			page 132


 703:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 897              		.loc 1 703 3 is_stmt 1 view .LVU268
 703:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 898              		.loc 1 703 5 is_stmt 0 view .LVU269
 899 0084 0646     		mov	r6, r0
 900 0086 0028     		cmp	r0, #0
 901 0088 F2D1     		bne	.L60
 902 008a C7E7     		b	.L59
 903              	.LVL79:
 904              	.L68:
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 905              		.loc 1 729 5 is_stmt 1 view .LVU270
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 906              		.loc 1 729 14 is_stmt 0 view .LVU271
 907 008c 2846     		mov	r0, r5
 908 008e FFF7FEFF 		bl	LL_SetFlashLatency
 909              	.LVL80:
 910 0092 0646     		mov	r6, r0
 911              	.LVL81:
 729:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 912              		.loc 1 729 14 view .LVU272
 913 0094 F0E7     		b	.L63
 914              	.L69:
 735:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 915              		.loc 1 735 5 is_stmt 1 view .LVU273
 916 0096 2846     		mov	r0, r5
 917 0098 FFF7FEFF 		bl	LL_SetSystemCoreClock
 918              	.LVL82:
 919 009c EDE7     		b	.L64
 920              	.L71:
 921 009e 00BF     		.align	2
 922              	.L70:
 923 00a0 00000000 		.word	AHBPrescTable
 924 00a4 00000000 		.word	SystemCoreClock
 925 00a8 00380240 		.word	1073887232
 926              		.cfi_endproc
 927              	.LFE413:
 929              		.section	.text.LL_PLL_ConfigSystemClock_HSI,"ax",%progbits
 930              		.align	1
 931              		.global	LL_PLL_ConfigSystemClock_HSI
 932              		.syntax unified
 933              		.thumb
 934              		.thumb_func
 936              	LL_PLL_ConfigSystemClock_HSI:
 937              	.LVL83:
 938              	.LFB409:
 490:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 939              		.loc 1 490 1 view -0
 940              		.cfi_startproc
 941              		@ args = 0, pretend = 0, frame = 0
 942              		@ frame_needed = 0, uses_anonymous_args = 0
 490:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 943              		.loc 1 490 1 is_stmt 0 view .LVU275
 944 0000 F8B5     		push	{r3, r4, r5, r6, r7, lr}
 945              	.LCFI8:
 946              		.cfi_def_cfa_offset 24
 947              		.cfi_offset 3, -24
ARM GAS  /tmp/ccqw5Uyy.s 			page 133


 948              		.cfi_offset 4, -20
 949              		.cfi_offset 5, -16
 950              		.cfi_offset 6, -12
 951              		.cfi_offset 7, -8
 952              		.cfi_offset 14, -4
 953 0002 0446     		mov	r4, r0
 954 0004 0D46     		mov	r5, r1
 491:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t pllfreq = 0U;
 955              		.loc 1 491 3 is_stmt 1 view .LVU276
 956              	.LVL84:
 492:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 957              		.loc 1 492 3 view .LVU277
 495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 958              		.loc 1 495 3 view .LVU278
 495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 959              		.loc 1 495 6 is_stmt 0 view .LVU279
 960 0006 FFF7FEFF 		bl	UTILS_PLL_IsBusy
 961              	.LVL85:
 495:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 962              		.loc 1 495 5 discriminator 1 view .LVU280
 963 000a 10BB     		cbnz	r0, .L76
 498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 964              		.loc 1 498 5 is_stmt 1 view .LVU281
 498:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 965              		.loc 1 498 15 is_stmt 0 view .LVU282
 966 000c 2146     		mov	r1, r4
 967 000e 1248     		ldr	r0, .L78
 968 0010 FFF7FEFF 		bl	UTILS_GetPLLOutputFrequency
 969              	.LVL86:
 501:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 970              		.loc 1 501 5 is_stmt 1 view .LVU283
 971              	.LBB86:
 972              	.LBI86:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 973              		.loc 2 2030 26 view .LVU284
 974              	.LBB87:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 975              		.loc 2 2032 3 view .LVU285
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 976              		.loc 2 2032 11 is_stmt 0 view .LVU286
 977 0014 114B     		ldr	r3, .L78+4
 978 0016 1B68     		ldr	r3, [r3]
 979              	.LBE87:
 980              	.LBE86:
 501:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 981              		.loc 1 501 7 discriminator 1 view .LVU287
 982 0018 13F0020F 		tst	r3, #2
 983 001c 09D1     		bne	.L74
 503:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       while (LL_RCC_HSI_IsReady() != 1U)
 984              		.loc 1 503 7 is_stmt 1 view .LVU288
 985              	.LBB88:
 986              	.LBI88:
2010:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 987              		.loc 2 2010 22 view .LVU289
 988              	.LBB89:
2012:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 989              		.loc 2 2012 3 view .LVU290
ARM GAS  /tmp/ccqw5Uyy.s 			page 134


 990 001e 0F4A     		ldr	r2, .L78+4
 991 0020 1368     		ldr	r3, [r2]
 992 0022 43F00103 		orr	r3, r3, #1
 993 0026 1360     		str	r3, [r2]
 994              	.LBE89:
 995              	.LBE88:
 504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 996              		.loc 1 504 7 view .LVU291
 997              	.L75:
 507:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 998              		.loc 1 507 7 view .LVU292
 504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 999              		.loc 1 504 35 discriminator 1 view .LVU293
 1000              	.LBB90:
 1001              	.LBI90:
2030:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1002              		.loc 2 2030 26 view .LVU294
 1003              	.LBB91:
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1004              		.loc 2 2032 3 view .LVU295
2032:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1005              		.loc 2 2032 11 is_stmt 0 view .LVU296
 1006 0028 0C4B     		ldr	r3, .L78+4
 1007 002a 1B68     		ldr	r3, [r3]
 1008              	.LBE91:
 1009              	.LBE90:
 504:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 1010              		.loc 1 504 35 discriminator 1 view .LVU297
 1011 002c 13F0020F 		tst	r3, #2
 1012 0030 FAD0     		beq	.L75
 1013              	.L74:
 511:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                 UTILS_PLLInitStruct->PLLP);
 1014              		.loc 1 511 5 is_stmt 1 view .LVU298
 1015 0032 2168     		ldr	r1, [r4]
 1016 0034 6668     		ldr	r6, [r4, #4]
 1017 0036 A268     		ldr	r2, [r4, #8]
 1018              	.LVL87:
 1019              	.LBB92:
 1020              	.LBI92:
3241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1021              		.loc 2 3241 22 view .LVU299
 1022              	.LBB93:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1023              		.loc 2 3243 3 view .LVU300
 1024 0038 084C     		ldr	r4, .L78+4
 1025              	.LVL88:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1026              		.loc 2 3243 3 is_stmt 0 view .LVU301
 1027 003a 6768     		ldr	r7, [r4, #4]
 1028 003c 084B     		ldr	r3, .L78+8
 1029 003e 3B40     		ands	r3, r3, r7
 1030 0040 41EA8611 		orr	r1, r1, r6, lsl #6
 1031              	.LVL89:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1032              		.loc 2 3243 3 view .LVU302
 1033 0044 0A43     		orrs	r2, r2, r1
 1034              	.LVL90:
ARM GAS  /tmp/ccqw5Uyy.s 			page 135


3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1035              		.loc 2 3243 3 view .LVU303
 1036 0046 1343     		orrs	r3, r3, r2
 1037 0048 6360     		str	r3, [r4, #4]
 1038              	.LVL91:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1039              		.loc 2 3243 3 view .LVU304
 1040              	.LBE93:
 1041              	.LBE92:
 515:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1042              		.loc 1 515 5 is_stmt 1 view .LVU305
 515:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1043              		.loc 1 515 14 is_stmt 0 view .LVU306
 1044 004a 2946     		mov	r1, r5
 1045 004c FFF7FEFF 		bl	UTILS_EnablePLLAndSwitchSystem
 1046              	.LVL92:
 1047              	.L73:
 523:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 1048              		.loc 1 523 3 is_stmt 1 view .LVU307
 524:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1049              		.loc 1 524 1 is_stmt 0 view .LVU308
 1050 0050 F8BD     		pop	{r3, r4, r5, r6, r7, pc}
 1051              	.LVL93:
 1052              	.L76:
 520:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1053              		.loc 1 520 12 view .LVU309
 1054 0052 0120     		movs	r0, #1
 1055 0054 FCE7     		b	.L73
 1056              	.L79:
 1057 0056 00BF     		.align	2
 1058              	.L78:
 1059 0058 0024F400 		.word	16000000
 1060 005c 00380240 		.word	1073887232
 1061 0060 0080BCFF 		.word	-4423680
 1062              		.cfi_endproc
 1063              	.LFE409:
 1065              		.section	.text.LL_PLL_ConfigSystemClock_HSE,"ax",%progbits
 1066              		.align	1
 1067              		.global	LL_PLL_ConfigSystemClock_HSE
 1068              		.syntax unified
 1069              		.thumb
 1070              		.thumb_func
 1072              	LL_PLL_ConfigSystemClock_HSE:
 1073              	.LVL94:
 1074              	.LFB410:
 548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 1075              		.loc 1 548 1 is_stmt 1 view -0
 1076              		.cfi_startproc
 1077              		@ args = 0, pretend = 0, frame = 0
 1078              		@ frame_needed = 0, uses_anonymous_args = 0
 548:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   ErrorStatus status = SUCCESS;
 1079              		.loc 1 548 1 is_stmt 0 view .LVU311
 1080 0000 F8B5     		push	{r3, r4, r5, r6, r7, lr}
 1081              	.LCFI9:
 1082              		.cfi_def_cfa_offset 24
 1083              		.cfi_offset 3, -24
 1084              		.cfi_offset 4, -20
ARM GAS  /tmp/ccqw5Uyy.s 			page 136


 1085              		.cfi_offset 5, -16
 1086              		.cfi_offset 6, -12
 1087              		.cfi_offset 7, -8
 1088              		.cfi_offset 14, -4
 1089 0002 0646     		mov	r6, r0
 1090 0004 0F46     		mov	r7, r1
 1091 0006 1446     		mov	r4, r2
 1092 0008 1D46     		mov	r5, r3
 549:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   uint32_t pllfreq = 0U;
 1093              		.loc 1 549 3 is_stmt 1 view .LVU312
 1094              	.LVL95:
 550:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1095              		.loc 1 550 3 view .LVU313
 553:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   assert_param(IS_LL_UTILS_HSE_BYPASS(HSEBypass));
 1096              		.loc 1 553 3 view .LVU314
 554:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1097              		.loc 1 554 3 view .LVU315
 557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 1098              		.loc 1 557 3 view .LVU316
 557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 1099              		.loc 1 557 6 is_stmt 0 view .LVU317
 1100 000a FFF7FEFF 		bl	UTILS_PLL_IsBusy
 1101              	.LVL96:
 557:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   {
 1102              		.loc 1 557 5 discriminator 1 view .LVU318
 1103 000e 0028     		cmp	r0, #0
 1104 0010 31D1     		bne	.L86
 560:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1105              		.loc 1 560 5 is_stmt 1 view .LVU319
 560:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1106              		.loc 1 560 15 is_stmt 0 view .LVU320
 1107 0012 2146     		mov	r1, r4
 1108 0014 3046     		mov	r0, r6
 1109 0016 FFF7FEFF 		bl	UTILS_GetPLLOutputFrequency
 1110              	.LVL97:
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 1111              		.loc 1 563 5 is_stmt 1 view .LVU321
 1112              	.LBB94:
 1113              	.LBI94:
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1114              		.loc 2 1992 26 view .LVU322
 1115              	.LBB95:
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1116              		.loc 2 1994 3 view .LVU323
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1117              		.loc 2 1994 11 is_stmt 0 view .LVU324
 1118 001a 184B     		ldr	r3, .L89
 1119 001c 1B68     		ldr	r3, [r3]
 1120              	.LBE95:
 1121              	.LBE94:
 563:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     {
 1122              		.loc 1 563 7 discriminator 1 view .LVU325
 1123 001e 13F4003F 		tst	r3, #131072
 1124 0022 10D1     		bne	.L82
 566:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 1125              		.loc 1 566 7 is_stmt 1 view .LVU326
 566:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
ARM GAS  /tmp/ccqw5Uyy.s 			page 137


 1126              		.loc 1 566 9 is_stmt 0 view .LVU327
 1127 0024 012F     		cmp	r7, #1
 1128 0026 20D0     		beq	.L88
 572:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
 1129              		.loc 1 572 9 is_stmt 1 view .LVU328
 1130              	.LBB96:
 1131              	.LBI96:
1962:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1132              		.loc 2 1962 22 view .LVU329
 1133              	.LBB97:
1964:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1134              		.loc 2 1964 3 view .LVU330
 1135 0028 144A     		ldr	r2, .L89
 1136 002a 1368     		ldr	r3, [r2]
 1137 002c 23F48023 		bic	r3, r3, #262144
 1138 0030 1360     		str	r3, [r2]
 1139              	.L84:
 1140              	.LBE97:
 1141              	.LBE96:
 576:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       while (LL_RCC_HSE_IsReady() != 1U)
 1142              		.loc 1 576 7 view .LVU331
 1143              	.LBB98:
 1144              	.LBI98:
1972:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1145              		.loc 2 1972 22 view .LVU332
 1146              	.LBB99:
1974:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1147              		.loc 2 1974 3 view .LVU333
 1148 0032 124A     		ldr	r2, .L89
 1149 0034 1368     		ldr	r3, [r2]
 1150 0036 43F48033 		orr	r3, r3, #65536
 1151 003a 1360     		str	r3, [r2]
 1152              	.LBE99:
 1153              	.LBE98:
 577:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 1154              		.loc 1 577 7 view .LVU334
 1155              	.L85:
 580:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****     }
 1156              		.loc 1 580 7 view .LVU335
 577:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 1157              		.loc 1 577 35 discriminator 1 view .LVU336
 1158              	.LBB100:
 1159              	.LBI100:
1992:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1160              		.loc 2 1992 26 view .LVU337
 1161              	.LBB101:
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1162              		.loc 2 1994 3 view .LVU338
1994:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1163              		.loc 2 1994 11 is_stmt 0 view .LVU339
 1164 003c 0F4A     		ldr	r2, .L89
 1165 003e 1268     		ldr	r2, [r2]
 1166              	.LBE101:
 1167              	.LBE100:
 577:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       {
 1168              		.loc 1 577 35 discriminator 1 view .LVU340
 1169 0040 12F4003F 		tst	r2, #131072
ARM GAS  /tmp/ccqw5Uyy.s 			page 138


 1170 0044 FAD0     		beq	.L85
 1171              	.L82:
 584:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                 UTILS_PLLInitStruct->PLLP);
 1172              		.loc 1 584 5 is_stmt 1 view .LVU341
 1173 0046 2268     		ldr	r2, [r4]
 1174 0048 6668     		ldr	r6, [r4, #4]
 1175              	.LVL98:
 584:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****                                 UTILS_PLLInitStruct->PLLP);
 1176              		.loc 1 584 5 is_stmt 0 view .LVU342
 1177 004a A168     		ldr	r1, [r4, #8]
 1178              	.LVL99:
 1179              	.LBB102:
 1180              	.LBI102:
3241:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1181              		.loc 2 3241 22 is_stmt 1 view .LVU343
 1182              	.LBB103:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1183              		.loc 2 3243 3 view .LVU344
 1184 004c 0B4C     		ldr	r4, .L89
 1185              	.LVL100:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1186              		.loc 2 3243 3 is_stmt 0 view .LVU345
 1187 004e 6768     		ldr	r7, [r4, #4]
 1188              	.LVL101:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1189              		.loc 2 3243 3 view .LVU346
 1190 0050 0B4B     		ldr	r3, .L89+4
 1191 0052 3B40     		ands	r3, r3, r7
 1192 0054 42F48002 		orr	r2, r2, #4194304
 1193              	.LVL102:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1194              		.loc 2 3243 3 view .LVU347
 1195 0058 42EA8612 		orr	r2, r2, r6, lsl #6
 1196 005c 0A43     		orrs	r2, r2, r1
 1197 005e 1343     		orrs	r3, r3, r2
 1198 0060 6360     		str	r3, [r4, #4]
 1199              	.LVL103:
3243:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h ****              Source | PLLM | PLLN << RCC_PLLCFGR_PLLN_Pos | PLLP);
 1200              		.loc 2 3243 3 view .LVU348
 1201              	.LBE103:
 1202              	.LBE102:
 588:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1203              		.loc 1 588 5 is_stmt 1 view .LVU349
 588:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1204              		.loc 1 588 14 is_stmt 0 view .LVU350
 1205 0062 2946     		mov	r1, r5
 1206 0064 FFF7FEFF 		bl	UTILS_EnablePLLAndSwitchSystem
 1207              	.LVL104:
 1208              	.L81:
 596:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** }
 1209              		.loc 1 596 3 is_stmt 1 view .LVU351
 597:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c **** 
 1210              		.loc 1 597 1 is_stmt 0 view .LVU352
 1211 0068 F8BD     		pop	{r3, r4, r5, r6, r7, pc}
 1212              	.LVL105:
 1213              	.L88:
 568:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****       }
ARM GAS  /tmp/ccqw5Uyy.s 			page 139


 1214              		.loc 1 568 9 is_stmt 1 view .LVU353
 1215              	.LBB104:
 1216              	.LBI104:
1952:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** {
 1217              		.loc 2 1952 22 view .LVU354
 1218              	.LBB105:
1954:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** }
 1219              		.loc 2 1954 3 view .LVU355
 1220 006a 044A     		ldr	r2, .L89
 1221 006c 1368     		ldr	r3, [r2]
 1222 006e 43F48023 		orr	r3, r3, #262144
 1223 0072 1360     		str	r3, [r2]
1955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 1224              		.loc 2 1955 1 is_stmt 0 view .LVU356
 1225 0074 DDE7     		b	.L84
 1226              	.LVL106:
 1227              	.L86:
1955:Drivers/STM32F7xx_HAL_Driver/Inc/stm32f7xx_ll_rcc.h **** 
 1228              		.loc 2 1955 1 view .LVU357
 1229              	.LBE105:
 1230              	.LBE104:
 593:Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_ll_utils.c ****   }
 1231              		.loc 1 593 12 view .LVU358
 1232 0076 0120     		movs	r0, #1
 1233 0078 F6E7     		b	.L81
 1234              	.L90:
 1235 007a 00BF     		.align	2
 1236              	.L89:
 1237 007c 00380240 		.word	1073887232
 1238 0080 0080BCFF 		.word	-4423680
 1239              		.cfi_endproc
 1240              	.LFE410:
 1242              		.text
 1243              	.Letext0:
 1244              		.file 6 "/usr/lib/gcc/arm-none-eabi/13.2.1/include/stdint.h"
 1245              		.file 7 "Drivers/CMSIS/Include/core_cm7.h"
 1246              		.file 8 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/system_stm32f7xx.h"
 1247              		.file 9 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/stm32f767xx.h"
 1248              		.file 10 "Drivers/CMSIS/Device/ST/STM32F7xx/Include/stm32f7xx.h"
ARM GAS  /tmp/ccqw5Uyy.s 			page 140


DEFINED SYMBOLS
                            *ABS*:00000000 stm32f7xx_ll_utils.c
     /tmp/ccqw5Uyy.s:20     .text.UTILS_GetPLLOutputFrequency:00000000 $t
     /tmp/ccqw5Uyy.s:25     .text.UTILS_GetPLLOutputFrequency:00000000 UTILS_GetPLLOutputFrequency
     /tmp/ccqw5Uyy.s:74     .text.UTILS_PLL_IsBusy:00000000 $t
     /tmp/ccqw5Uyy.s:79     .text.UTILS_PLL_IsBusy:00000000 UTILS_PLL_IsBusy
     /tmp/ccqw5Uyy.s:154    .text.UTILS_PLL_IsBusy:0000002c $d
     /tmp/ccqw5Uyy.s:159    .text.LL_Init1msTick:00000000 $t
     /tmp/ccqw5Uyy.s:165    .text.LL_Init1msTick:00000000 LL_Init1msTick
     /tmp/ccqw5Uyy.s:206    .text.LL_Init1msTick:0000001c $d
     /tmp/ccqw5Uyy.s:211    .text.LL_mDelay:00000000 $t
     /tmp/ccqw5Uyy.s:217    .text.LL_mDelay:00000000 LL_mDelay
     /tmp/ccqw5Uyy.s:273    .text.LL_SetSystemCoreClock:00000000 $t
     /tmp/ccqw5Uyy.s:279    .text.LL_SetSystemCoreClock:00000000 LL_SetSystemCoreClock
     /tmp/ccqw5Uyy.s:296    .text.LL_SetSystemCoreClock:00000008 $d
     /tmp/ccqw5Uyy.s:301    .text.LL_SetFlashLatency:00000000 $t
     /tmp/ccqw5Uyy.s:307    .text.LL_SetFlashLatency:00000000 LL_SetFlashLatency
     /tmp/ccqw5Uyy.s:693    .text.LL_SetFlashLatency:00000140 $d
     /tmp/ccqw5Uyy.s:705    .text.UTILS_EnablePLLAndSwitchSystem:00000000 $t
     /tmp/ccqw5Uyy.s:710    .text.UTILS_EnablePLLAndSwitchSystem:00000000 UTILS_EnablePLLAndSwitchSystem
     /tmp/ccqw5Uyy.s:923    .text.UTILS_EnablePLLAndSwitchSystem:000000a0 $d
     /tmp/ccqw5Uyy.s:930    .text.LL_PLL_ConfigSystemClock_HSI:00000000 $t
     /tmp/ccqw5Uyy.s:936    .text.LL_PLL_ConfigSystemClock_HSI:00000000 LL_PLL_ConfigSystemClock_HSI
     /tmp/ccqw5Uyy.s:1059   .text.LL_PLL_ConfigSystemClock_HSI:00000058 $d
     /tmp/ccqw5Uyy.s:1066   .text.LL_PLL_ConfigSystemClock_HSE:00000000 $t
     /tmp/ccqw5Uyy.s:1072   .text.LL_PLL_ConfigSystemClock_HSE:00000000 LL_PLL_ConfigSystemClock_HSE
     /tmp/ccqw5Uyy.s:1237   .text.LL_PLL_ConfigSystemClock_HSE:0000007c $d

UNDEFINED SYMBOLS
SystemCoreClock
AHBPrescTable
